{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["SUMMARY","CENA","KORISNICI","vendors list"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":7,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"SUMMARY","index":0,"n_rows":19,"n_cols":3,"rows_kept":19,"cut":false,"hidden":false,"merged":[[12,2,12,5],[10,2,10,5],[15,2,15,5],[17,2,17,5],[18,2,18,5],[13,2,13,5]]}
[]
[]
[null,null,"SUMMARY / REKAPITULACIJA"]
[]
[]
[null,null,"SUM PRICE /\n UKUPNA CENA\n"]
[null,"UKUPNO/\nTOTAL",{"$f":"CENA!I267","v":0}]
[]
[]
[]
[null,"Napomena:","štampati samo sheetove (SUMMARY, CENA, VendorsList)"]
[]
[null,null,"unositi cene samo u zeleno obeležen sheet u zelena polja (CENA) \nod G5 - G266 (jedinične cene)"]
[null,null,"popuniti zelena polja u VendorsList"]
[]
[null,"Remark:","print only green sheet (SUMMARY, CENA, VendorsList)"]
[]
[null,null,"The prices entered only in the green marked sheet in green cells (CENA) \nG5 - G266 (unit price)"]
[null,null,"Fill only green cells in VendorsList"]

{"sheet":"CENA","index":1,"n_rows":267,"n_cols":9,"rows_kept":267,"cut":false,"hidden":false,"merged":[]}
[null,null,null,null,null,null,null,"LOT 1"]
["KOD/\nCODE",null,null,"Opis građevinskog materijala ","Description of building materials","Jed.\nprod./\nUNIT","Jedinična\nprod.cena/\nUNIT PRICE ","Zbir Količina po materijalima/\nSUM QTY","ZBIR UKUPNO PO MATERIJALIMA/\nSUM PRICE"]
[]
[1,"A",null,"OSNOVNI GRAĐEVINSKI MATERIJAL","BASIC BUILDING MATERIALS"]
["1.1","O",1,"Cement  za betone do MB 30","Cement for concrete up to 30 MB","kg",null,{"$f":"KORISNICI!H14","v":97950},{"$f":"G5*H5","v":0}]
["1.2","O",2,"Hidratisani gašeni kreč pripremljen u prahu","Hydrated slaked lime powdered","kg",null,{"$f":"KORISNICI!H15","v":11150},{"$f":"G6*H6","v":0}]
["1.3","O",3,"Rebrasto betonsko gvožđe (RA) ","Ribbed reinforcement steel","/","/","/","/"]
["1.3.1",null,"A","10 mm   - dužine 12m","10 mm   - length 12m ","kg",null,{"$f":"KORISNICI!H17","v":402.48},{"$f":"G8*H8","v":0}]
["1.3.2",null,"B","12 mm   - dužine 12m","12 mm   - length 12m","kg",null,{"$f":"KORISNICI!H18","v":6082.4400000000005},0]
["1.3.3",null,"C","14 mm   - dužine 12m","14 mm   - length 12m","kg",null,{"$f":"KORISNICI!H19","v":0},0]
["1.3.4",null,"D","16 mm   - dužine 12m","16 mm   - length 12m","kg",null,{"$f":"KORISNICI!H20","v":0},0]
["1.4","O",4,"Glatko betonsko gvožđe (GA) ","Glibly reinforcement steel","/","/","/","/"]
["1.4.1",null,"B","  8 mm   - dužine 12m","  8 mm   - length 12m","kg",null,{"$f":"KORISNICI!H22","v":1763.2800000000002},{"$f":"G13*H13","v":0}]
["1.4.2",null,"C","10 mm  - dužine 12m","10 mm  - length 12m","kg",null,{"$f":"KORISNICI!H23","v":0},0]
["1.5","O",5,"Armaturna betonska mreža \ndim. (dxš) 6000 x 2150 = 12,9 m2/kom","Reinforcement mesh\ndim. (lxw) 6000 x 2150 = 12,9 m2/pcs","/","/","/","/"]
["1.5.1",null,"A","Q84    /4x4/150x150/ ","Q84    /4x4/150x150/ ","kg",null,{"$f":"KORISNICI!H25","v":1408},{"$f":"G16*H16","v":0}]
["1.5.2",null,"B","Q131  /5x5/150x150/ ","Q131  /5x5/150x150/ ","kg",null,{"$f":"KORISNICI!H26","v":2299.92},0]
["1.5.3",null,"C","Q188  /6x6/150x150/ ","Q188  /6x6/150x150/ ","kg",null,{"$f":"KORISNICI!H27","v":315.68},0]
["1.5.4",null,"D","Q283  /6x6/100x100/","Q283  /6x6/100x100/","kg",null,{"$f":"KORISNICI!H28","v":0},0]
["1.5.5",null,"E","Q335  /8x8/150x150/","Q335  /8x8/150x150/","kg",null,{"$f":"KORISNICI!H29","v":631.98},0]
[]
[2,"Z",null,"MATERIJAL ZA ZIDANJE, MALTERISANJE, GLETOVANJE I FARBANJE","MASONRY, PLASTERING FAIRING AND PAINTING MATERIAL"]
["2.1","Z",1,"Giter blok (d/š/v) 250x190x190 mm","Gitter block (l/w/h) 250x190x190 mm","kom/pcs",null,{"$f":"KORISNICI!H32","v":20480},{"$f":"G23*H23","v":0}]
["2.2","Z",2,"Giter polublok (12cm) (d/š/v) 250x120x190mm","Gitter half block (12cm) (l/w/h) 250x120x190mm","kom/pcs",null,{"$f":"KORISNICI!H33","v":3990},0]
["2.3","Z",3,"Opeka puna (d/š/v) 250x120x65 mm","Brick (full-without holes) (l/w/h) 250x120x65 mm","kom/pcs",null,{"$f":"KORISNICI!H34","v":30720},0]
["2.4","Z",4,"Blok od porobetona za pregradni zid\n(d/š/v) 625x200x200 mm","Aerated concrete block for partition wall\n(l/w/h) 625x200x200 mm","kom/pcs",null,{"$f":"KORISNICI!H35","v":0},0]
["2.5","Z",5,"Fert nosači (gredice)\nDužina nosača je jednaka dužini binora = \nširina otvora između zidova + 30 cm.\nBroj gredica = dužina prostorije x 0,40","Fert beams\nBoom length is equal to the length of Binor =\nwidth of the openings between the walls + 30 cm.\nNumber of beams = length of room x 0.40","/","/","/","/"]
["2.5.1",null,"A","0,00-3,90 m ","0,00-3,90 m ","m1",null,{"$f":"KORISNICI!H37","v":737.09999999999991},{"$f":"G28*H28","v":0}]
["2.5.2",null,"B","3,91-4,50 m ","3,91-4,50 m ","m1",null,{"$f":"KORISNICI!H38","v":445.5},0]
["2.5.3",null,"C","4,51-4,90 m ","4,51-4,90 m ","m1",null,{"$f":"KORISNICI!H39","v":406.7},0]
["2.5.4",null,"D","4,91-5,30 m ","4,91-5,30 m ","m1",null,{"$f":"KORISNICI!H40","v":0},0]
["2.5.5",null,"E","5,31-5,90 m ","5,31-5,90 m ","m1",null,{"$f":"KORISNICI!H41","v":165.20000000000002},0]
["2.5.6",null,"F","5,91-6,30 m ","5,91-6,30 m ","m1",null,{"$f":"KORISNICI!H42","v":176.4},0]
["2.6","Z",6,"Fert ispuna (d/š/v) 245x285/275x160 mm ","Fert fillings (l/w/h) 245x285/275x160 mm ","kom/pcs",null,{"$f":"KORISNICI!H43","v":5670},0]
["2.7","Z",7,"Malter za zidanje \nPripremljeno krečno - cementno vezivo","Mortar for masonry\nPrepared lime - cement binder","kg",null,{"$f":"KORISNICI!H44","v":0},0]
["2.8","Z",8,"Malter za malterisanje \nPripremljeno krečno - cementno vezivo","Mortar for plastering\nPrepared lime - cement binder","kg",null,{"$f":"KORISNICI!H45","v":2600},0]
["2.9","Z",9,"Krečna glet masa\nBezcementna krečna masa za gletovanje","Lime smoothing mass\nNo cement lime compound for smoothing","kg",null,{"$f":"KORISNICI!H46","v":7325},0]
["2.10","Z",10,"Poludisperzivna boja \nPoludisperziona boja  razrediva vodom","Semi dispersion paint","kg",null,{"$f":"KORISNICI!H47","v":1100},0]
[]
["3","K",null,"MATERIJAL ZA KROVNU KONSTRUKCIJU, KROVNI POKRIVAČ, OSB I GIPS KARONSKE TABLE","ROOF CONSTRUCTION AND ROOFING MATERIAL, OSB AND PLASTERBOARD TABLE"]
["3.1","K",1,"Presovani glineni crep I klase\ndimenzija: 400-450x245-275 mm","Pressed clay tiles class 1\ndim: 400-450x245-275 mm","kom/pcs",null,{"$f":"KORISNICI!H50","v":59840},{"$f":"G41*H41","v":0}]
["3.2","K",3,"Biber crep I klase dimenzija: 180x380 mm","Biber clay tiles class 1 dim: 180x380 mm","kom/pcs",null,{"$f":"KORISNICI!H51","v":0},0]
["3.3","K",2,"Slemeni crep I klase (žljebnjak)","Ridge clay tiles class 1","kom/pcs",null,{"$f":"KORISNICI!H52","v":870},0]
["3.4","K",4,"Paropropusna i vodonepropusna krovna  folija kontrola vodene pare iznad termoizolacije","Vapour permeable and waterproof roof sheeting control of water vapor above the insulation","m2",null,{"$f":"KORISNICI!H53","v":3825},0]
["3.5","K",5,"Staklena mineralna vuna \ntermoizolacija potkrovlja između rogova","Glass Mineral Wool \nloft insulation between the rafters","/","/","/","/"]
["3.5.1",null,"A","debljina d=10 cm  ","thickness d=10 cm  ","m2",null,{"$f":"KORISNICI!H55","v":2226},{"$f":"G46*H46","v":0}]
["3.5.2",null,"B","debljina d=12 cm  ","thickness d=12 cm  ","m2",null,{"$f":"KORISNICI!H56","v":0},0]
["3.5.3",null,"C","debljina d=14 cm  ","thickness d=14 cm  ","m2",null,{"$f":"KORISNICI!H57","v":0},0]
["3.6","K",6,"Parna brana\nkontrola vodene pare ispod termoizolacije","Vapor barrier \ncontrol of water vapor below the insulation","m2",null,{"$f":"KORISNICI!H58","v":2550},0]
["3.7","K",7,"Čamova rezana građa različitog preseka\ndužine 400 cm","Fir lumber of different cross-section\nlength 400 cm","/","/","/","/"]
["3.7.1",null,"A","Rog/Venčanica/Raspinjača           10/12 cm","rafters / wall plate / ridge collar 10/12 cm","m3",null,{"$f":"KORISNICI!H60","v":0},{"$f":"G51*H51","v":0}]
["3.7.2",null,"B","Rog/Stub/Grebenjača/Slemenja.   12/14 cm","column / pile / hip rafter / ridge 12/14 cm","m3",null,{"$f":"KORISNICI!H61","v":0},0]
["3.7.3",null,"C","Stub/Grebenjača                         14/14 cm","column / hip rafter 14/14 cm","m3",null,{"$f":"KORISNICI!H62","v":14.975999999999999},0]
["3.7.4",null,"H","Tavanjače                                   18/26 cm","attic beams 18/26 cm","m3",null,{"$f":"KORISNICI!H63","v":0},0]
["3.8","K",8,"Čamova rezana građa različitog preseka\ndužine 600 cm","Fir lumber of different cross-section\nlength 600 cm","/","/","/","/"]
["3.8.1",null,"A","Rog/Venčanica/Raspinjača          10/12 cm","rafters / wall plate / ridge collar 10/12 cm","m3",null,{"$f":"KORISNICI!H65","v":67.24799999999999},{"$f":"G56*H56","v":0}]
["3.8.2",null,"B","Rog/Stub/Grebenjača/Slemenja.   12/14 cm","column / pile / hip rafter / ridge 12/14 cm","m3",null,{"$f":"KORISNICI!H66","v":0.2016},0]
["3.8.3",null,"C","Stub/Grebenjača                         14/14 cm","column / hip rafter 14/14 cm","m3",null,{"$f":"KORISNICI!H67","v":12.870000000000001},0]
["3.8.4",null,"D","Rožnjača                                    14/16 cm","Purlin 14/16 cm","m3",null,{"$f":"KORISNICI!H68","v":15.276000000000003},0]
["3.8.5",null,"E","Kosnik/Pajanta                           10/10 cm","Strut 10/10 cm","m3",null,{"$f":"KORISNICI!H69","v":11.04},0]
["3.8.6",null,"F","Klešta                                         6/12 cm","Collar tie 6/12 cm","m3",null,{"$f":"KORISNICI!H70","v":8.0839999999999979},0]
["3.8.7",null,"G","Krovna štafla                                5/8  cm","Roof battens 5/8  cm","m3",null,{"$f":"KORISNICI!H71","v":2.4},0]
["3.8.8",null,"H","Tavanjače                                   18/26 cm","attic beams 18/26 cm","m3",null,{"$f":"KORISNICI!H72","v":6.7439999999999998},0]
["3.9","K",9,"Građevinska daska - fosna\n4,8/25/400 cm","Fir board\n4,8/25/400 cm","m3",null,{"$f":"KORISNICI!H73","v":2.016},0]
["3.10","K",10,"Krovna daska od čamove rezane građe \n2,4-2,5/15 cm, isporučuje se dužine l=3,0 metra","Roof fir board\n2,4-2,5/15 cm, lenght l=3,0 m","m3",null,{"$f":"KORISNICI!H74","v":84.900797029702986},0]
["3.11","K",11,"Krovna letva od čamove rezane građe \n 3 / 5 cm , isporučuje se dužine l=3,0 metra","Fir batten\n 3 / 5 cm , lenght l=3,0 m","m1",null,{"$f":"KORISNICI!H75","v":14364},0]
["3.12","K",12,"OSB3  vlagootporne konstruktivne ploče\nd=18 mm / dim. 2440 x 1220","OSB3  moisture resistant structural panels\nd=18 mm / dim. 2440 x 1220","kom/pcs",null,{"$f":"KORISNICI!H76","v":26},0]
["3.13","K",13,"Standardne gips kartonske ploče - Tip A\ndimenzije: 1200-1250 x 2000 mm","Standard plasterboard table - Type A\ndim: 1200-1250 x 2000 mm","kom/pcs",null,{"$f":"KORISNICI!H77","v":100},0]
["3.14","K",14,"Vlagootporne gips kartonske ploče - Tip H2\ndimenzije: 1200-1250 x 2000 mm","Moisture resistant Plasterboard - Type H2\ndim: 1200-1250 x 2000 mm","kom/pcs",null,{"$f":"KORISNICI!H78","v":245},0]
["3.15","K",15,"Čelični pocinkovani i farbani olučni elementi prečnika: Ø 100 mm dužine 600 cm","Galvanized steel and painted gutter elements diameter: Ø 100 mm length 600 cm","/","/","/","/"]
["3.15.1",null,"A","Horizontalni polukružni","horizontal semicircular gutter","kom/pcs",null,{"$f":"KORISNICI!H80","v":109},{"$f":"G71*H71","v":0}]
["3.15.2",null,"B","Vertikalni kružni oluk","Vertical circular gutter","kom/pcs",null,{"$f":"KORISNICI!H81","v":52},0]
[]
["4","P",null,"MATERIJAL ZA PODOVE, LAMINAT, PLOČICE I XPS","FLOORING, LAMINATE, TILES AND XPS"]
["4.1","P",1,"Unutrašnje podne keramičke pločice\nMin. dimenzije pločica: 200x300 mm","Floor tiles for inside\nMin. tile size: 200x300 mm","m2",null,{"$f":"KORISNICI!H84","v":396},{"$f":"G75*H75","v":0}]
["4.2","P",2,"Unutrašnje zidne keramičke pločice \nMin. dimenzije pločica: 200x300 mm","Wall tiles for inside\nMin. tile size: 200x300 mm","m2",null,{"$f":"KORISNICI!H85","v":605},0]
["4.3","P",3,"Lepak za keramičke pločice\nFleksibilni, polimer-cementni lepak","Glue for ceramic tiles\nFlexible, polymer-cement glue","kg",null,{"$f":"KORISNICI!H86","v":3550},0]
["4.4","P",4,"Fleksibilna masa za fugovanje\nVodoodbojna fug masa na bazi cementa","Flexible mass for grouting\nWaterproof grout cement based","kg",null,{"$f":"KORISNICI!H87","v":636},0]
["4.5","P",5,"Laminat - jakopresovani (HLP)\nsa klik sistemom, dezen: hrast natur (prirodni)","Laminate (HLP)\nwith click system, design: oak natural (natural)","m2",null,{"$f":"KORISNICI!H88","v":1042},0]
["4.6","P",6,"Lajsne za laminat od medijapana \nmaterijal: medijapan / MDF","Moldings for laminate MDF\nMaterial: MDF / MDF","m1",null,{"$f":"KORISNICI!H89","v":1029.5999999999999},0]
["4.7","P",7,"Podloga za laminat od polietilenske pene\nSunđerasta podloga za laminat","The base for laminate of polyethylene foam\nFoam base for laminate","m2",null,{"$f":"KORISNICI!H90","v":1221},0]
["4.8","P",8,"Cementni suvi estrih (cementna košuljica).\nPripremljeno cementno praškasto vezivo","Cement dry screed (cement screed)\nPrepared cement powder binder","kg",null,{"$f":"KORISNICI!H91","v":0},0]
["4.9","P",9,"Građevinska PVC folija Za razdvajanje cementne košuljice od termo izolacije.","PVC foil for construction. To separate the cement screed of thermal insulation.","m2",null,{"$f":"KORISNICI!H92","v":1960},0]
["4.10","P",10,"Stirodur (XPS za izolaciju na podovima)\nploča od ekstrudirane polistirenske pene","Stirodur (XPS insulation for floors)\npanel of extruded polystyrene foam","/","/","/","/"]
["4.10.1",null,"A","debljine d=2 cm","d=2 cm","m2",null,{"$f":"KORISNICI!H94","v":1455},{"$f":"G85*H85","v":0}]
["4.10.2",null,"B","debljine d=5 cm","d=5 cm","m2",null,{"$f":"KORISNICI!H95","v":0},0]
[]
["5","F",null,"MATERIJAL ZA IZRADU FASADE","FACADE MATERIAL"]
["5.1","F",1,"EPS za termoizolaciju fasadnih zidova\nploča od ekspandiranog polistirena ","Thermal insulation for facade walls (EPS)\nplates made of expanded polystyrene","/","/","/","/"]
["5.1.1",null,"A","debljina d=8 cm","d=8 cm","m2",null,{"$f":"KORISNICI!H99","v":351},{"$f":"G90*H90","v":0}]
["5.1.2",null,"B","debljina d=10 cm","d=10 cm","m2",null,{"$f":"KORISNICI!H100","v":2000},0]
["5.1.3",null,"C","debljina d=12 cm","d=12 cm","m2",null,{"$f":"KORISNICI!H101","v":0},0]
["5.1.4",null,"D","debljina d=14 cm","d=14 cm","m2",null,{"$f":"KORISNICI!H102","v":0},0]
["5.2","F",2,"GrađevinskI lepak za EPS ploče \ncementni lepak namenjen za lepljenje ploča od ekspandiranog polistirena (EPS) i armiranje armaturne (rabic) mrežice ","Construction glue for EPS plates\ncement adhesive for gluing plates made of expanded polystyrene (EPS) and reinforcing wire (rabic) net","kg",null,{"$f":"KORISNICI!H103","v":29970},0]
["5.3","F",3,"Armaturna (rabic) staklena mrežica.\nVisokokvalitetna alkalno postojana staklena mrežica","Reinforcing (rabic) fiberglass mesh\nHigh quality alkali resistant fiberglass mesh","m2",null,{"$f":"KORISNICI!H104","v":2650},0]
["5.4","F",4,"Aktivni predpremaz pre nanošenja tankoslojnog fasadnog maltera.\npredpremaz za izjednačavanje upijanja - podloga","Active primer before applying the thin-layer plaster primer for the equalization of absorption surface","kg",null,{"$f":"KORISNICI!H105","v":750},0]
["5.5","F",5,"Fasadni tankoslojni akrilni malter\nZavršni malter u pastoznom stanju, namenjen za zaštitu fasadnih zidnih površina","Facade thin-layer acrylic plaster\nFinishing plaster in paste-like state, intended for the protection of facade wall surfaces","/","/","/","/"]
["5.5.1",null,"A","boja približna RAL 1034 -kajsija ","color similar to RAL 1034-apricot","kg",null,{"$f":"KORISNICI!H107","v":8025},{"$f":"G98*H98","v":0}]
["5.5.2",null,"B","boja približna RAL 6005 -pastelno zelena","color similar to RAL 6005 pastel-green","kg",null,{"$f":"KORISNICI!H108","v":0},0]
["5.5.3",null,"C","boja približna RAL 5023 -pastelno plava","color similar to RAL 5023 pastel-blue","kg",null,{"$f":"KORISNICI!H109","v":0},0]
["5.5.4",null,"D","boja približna RAL 3011 -pastelno crvena","color similar to RAL 3011 pastel-red","kg",null,{"$f":"KORISNICI!H110","v":0},0]
["5.5.5",null,"E","boja približna RAL 8002 -braon","color similar to RAL 8002 brown","kg",null,{"$f":"KORISNICI!H111","v":0},0]
[]
["6","H",null,"MATERIJAL ZA HIDRO IZOLACIJE","WATERPROOFING MATERIAL"]
["6.1","H",1,"Bitulit (prethodni premaz za hidroizolaciju)\nUpotrebljava se u isporučenom stanju (hladan  postupak ) bez zagrevanja","Bitulit (previous coating for waterproofing)\nIt is used as delivered (cold process) without heating","kg",null,{"$f":"KORISNICI!H114","v":135},{"$f":"G105*H105","v":0}]
["6.2","H",2,"Poliazbitol (hladni premaz za hidroizolaciju) Upotrebljava se u isporučenom stanju (hladan postupak) bez zagrevanja","POLYASBITOL (cold coating for waterproofing)\nIt is used as delivered (cold process) without heating","kg",null,{"$f":"KORISNICI!H115","v":0},0]
["6.3","H",3,"Ter papir Bitumenska hidroizolaciona traka.","Ter paper Bituminous waterproofing tape.","m2",null,{"$f":"KORISNICI!H116","v":0},0]
["6.4","H",4,"Kondor V-3 (hidroizolaciona traka)\nPlastomer-bitumenska traka, \nuložak stakleni voal, debljina:  ≥ 3 mm","Condor V-3 (waterproof tape)\nPlastomer-bituminous tape,\nglass mat, thickness: ≥ 3 mm","m2",null,{"$f":"KORISNICI!H117","v":450},0]
[]
["7","S",null,"STOLARIJA","DOORS AND WINDOWS"]
["7.1","S",1,"Ulazna vrata od PVC-a (komplet pozicija). \nboja profila: bela RAL 9003\nbroj komora: ≥  5 komora\nširina x visina (zidarske mere)","Entrance door of PVC (set position)\nProfile color: white RAL 9003 \nNumber of chambers: ≥ 5 chambers \nwidth x height (masonry measures)","/","/","/","/"]
["7.1.1",null,"A","JK    90x210 cm - Leva       90 cm ","one wing  90x210 cm - Left      90 cm ","kom/pcs",null,{"$f":"KORISNICI!H121","v":5},{"$f":"G112*H112","v":0}]
["7.1.2",null,"B","JK    90x210 cm - Desna    90 cm","one wing  90x210 cm - Right    90 cm","kom/pcs",null,{"$f":"KORISNICI!H122","v":9},0]
["7.1.3",null,"C","DK 120x210 cm - Leva       90+30 cm","two wings 120x210 cm - Left        90+30 cm","kom/pcs",null,{"$f":"KORISNICI!H123","v":5},0]
["7.1.4",null,"D","DK 120x210 cm - Desna    90+30 cm","two wings 120x210 cm - Right    90+30 cm","kom/pcs",null,{"$f":"KORISNICI!H124","v":2},0]
["7.2","S",2,"Prozori od PVC-a (komplet pozicija).\nVertikalno i horizontalno otvaranje, boja profila: bela RAL 9003, broj komora: ≥  5 komora\nširina x visina (zidarske mere)","Windows made of PVC (set position)\nVertical and horizontal opening, color profile: white RAL 9003, the number of chambers: ≥ 5 chambers \nwidth x height (masonry measures)","/","/","/","/"]
["7.2.1",null,"A","JK     60x60 cm ","one wing 60x60 cm ","kom/pcs",null,{"$f":"KORISNICI!H126","v":31},{"$f":"G117*H117","v":0}]
["7.2.2",null,"B","JK     80x80 cm","one wing 80x80 cm","kom/pcs",null,{"$f":"KORISNICI!H127","v":9},0]
["7.2.3",null,"C","JK    80x120 cm    ","one wing 80x120 cm    ","kom/pcs",null,{"$f":"KORISNICI!H128","v":30},0]
["7.2.4",null,"D","JK    80x140 cm    ","one wing 80x140 cm ","kom/pcs",null,{"$f":"KORISNICI!H129","v":2},0]
["7.2.5",null,"E","JK  100x120 cm","one wing 100x120 cm","kom/pcs",null,{"$f":"KORISNICI!H130","v":15},0]
["7.2.6",null,"F","JK  100x140 cm","one wing 100x140 cm","kom/pcs",null,{"$f":"KORISNICI!H131","v":3},0]
["7.2.7",null,"G","DK  120x120 cm","two wings 120x120 cm","kom/pcs",null,{"$f":"KORISNICI!H132","v":12},0]
["7.2.8",null,"H","DK  120x140 cm","two wings 120x140 cm","kom/pcs",null,{"$f":"KORISNICI!H133","v":6},0]
["7.2.9",null,"I","DK  140x120 cm ","two wings 140x120 cm ","kom/pcs",null,{"$f":"KORISNICI!H134","v":9},0]
["7.2.10",null,"J","DK  140x140 cm ","two wings 140x140 cm ","kom/pcs",null,{"$f":"KORISNICI!H135","v":6},0]
["7.2.11",null,"K","DK  160x120 cm","two wings 160x120 cm","kom/pcs",null,{"$f":"KORISNICI!H136","v":6},0]
["7.2.12",null,"L","DK  160x140 cm","two wings 160x140 cm","kom/pcs",null,{"$f":"KORISNICI!H137","v":12},0]
["7.3","S",3,"Krovni prozor sa  aluminijumskom opšivkom od laminirane i impregnirane čamove građe","Roof window with aluminum flashings of laminated and impregnated fir timber","/","/","/","/"]
["7.3.1",null,"A","dimenzije 66 x 118   (širinaxvisina)","66 x 118 (width x height)","kom/pcs",null,{"$f":"KORISNICI!H139","v":0},{"$f":"G130*H130","v":0}]
["7.3.2",null,"B","dimenzije 78 x 98     (širinaxvisina)","78 x 98   (width x height)","kom/pcs",null,{"$f":"KORISNICI!H140","v":0},0]
["7.3.3",null,"C","dimenzije 78 x 118   (širinaxvisina)","78 x 118 (width x height)","kom/pcs",null,{"$f":"KORISNICI!H141","v":0},0]
["7.4","S",4,"Balkonska vrata od PVC-a (komplet pozicija). \nboja profila: bela RAL 9003\nbroj komora: ≥  5 komora\nširina x visina (zidarske mere)","Balcony doors from PVC (set position)\nProfile color: white RAL 9003 \nNumber of chambers: ≥ 5 chambers \nwidth x height (masonry measures)","/","/","/","/"]
["7.4.1",null,"A","JK     90x210 cm   - Leva","one wing  90x210 cm - Left     ","kom/pcs",null,{"$f":"KORISNICI!H143","v":0},{"$f":"G134*H134","v":0}]
["7.4.2",null,"B","JK     90x210 cm   - Desna ","one wing  90x210 cm - Right    ","kom/pcs",null,{"$f":"KORISNICI!H144","v":0},0]
["7.4.3",null,"C","DK  140x210 cm","two wings 140x210 cm","kom/pcs",null,{"$f":"KORISNICI!H145","v":2},0]
["7.5","S",5,"Unutrašnja vrata sa ispunom od kartonskog saća (komplet pozicija). \nširina x visina (spoljna mera futera)","Internal doors filled with cardboard honeycomb (set position)\nwidth x height (external measures footer)","/","/","/","/"]
["7.5.1",null,"A","70x205 cm - Leva  (dubina štoka 0-16 cm)","70x205 cm - Left     (depth door 0-16 cm)","kom/pcs",null,{"$f":"KORISNICI!H147","v":0},{"$f":"G138*H138","v":0}]
["7.5.2",null,"B","70x205 cm - Leva  (dubina štoka 16-30 cm)","70x205 cm - Left     (depth door 16-30 cm)","kom/pcs",null,{"$f":"KORISNICI!H148","v":12},0]
["7.5.3",null,"C","70x205 cm - Desna (dubina štoka 0-16 cm)","70x205 cm - Right   (depth door  0-16 cm)","kom/pcs",null,{"$f":"KORISNICI!H149","v":0},0]
["7.5.4",null,"D","70x205 cm - Desna (dubina štoka 16-30 cm)","70x205 cm - Right   (depth door  16-30 cm)","kom/pcs",null,{"$f":"KORISNICI!H150","v":6},0]
["7.5.5",null,"E","80x205 cm - Leva  (dubina štoka 0-16 cm)","80x205 cm - Left     (depth door 0-16 cm)","kom/pcs",null,{"$f":"KORISNICI!H151","v":0},0]
["7.5.6",null,"F","80x205 cm - Leva  (dubina štoka 16-30 cm)","80x205 cm - Left     (depth door 16-30 cm)","kom/pcs",null,{"$f":"KORISNICI!H152","v":3},0]
["7.5.7",null,"G","80x205 cm - Desna (dubina štoka 0-16 cm)","80x205 cm - Right   (depth door  0-16 cm)","kom/pcs",null,{"$f":"KORISNICI!H153","v":0},0]
["7.5.8",null,"H","80x205 cm - Desna (dubina štoka 16-30 cm)","80x205 cm - Right   (depth door  16-30 cm)","kom/pcs",null,{"$f":"KORISNICI!H154","v":8},0]
["7.5.9",null,"I","90x205 cm - Leva  (dubina štoka 0-16 cm)","90x205 cm - Left     (depth door 0-16 cm)","kom/pcs",null,{"$f":"KORISNICI!H155","v":0},0]
["7.5.10",null,"J","90x205 cm - Leva  (dubina štoka 16-30 cm)","90x205 cm - Left     (depth door 16-30 cm)","kom/pcs",null,{"$f":"KORISNICI!H156","v":35},0]
["7.5.11",null,"K","90x205 cm - Desna (dubina štoka 0-16 cm)","90x205 cm - Right   (depth door  0-16 cm)","kom/pcs",null,{"$f":"KORISNICI!H157","v":0},0]
["7.5.12",null,"L","90x205 cm - Desna (dubina štoka 16-30 cm)","90x205 cm - Right   (depth door  16-30 cm)","kom/pcs",null,{"$f":"KORISNICI!H158","v":43},0]
[]
["8","D",null,"OSTALA OPREMA I MATERIJAL \n","OTHER EQUIPMENT AND SUPPLIES"]
["8.1","D",1,"Jednostruki dimnjak prečnika Ф 140 mm.\nTroslojni montažni dimnjački sistem namenjen za sva ložišta i sve vrste goriva, bez ventilacije.\nSastavljen je od: dimnjačke cevi od tehničke keramike, izolacije oko cevi dimnjaka od kamene vune minimalne specifične težine 80kg/m3, spoljneg dimnjačkog plašta od lakog betona, vatrostalnog lepka u kartušama, vatrootpornih i gasnonepropusnih atestiranih troslojnih vratanaca , kondenz posude, priključaka za reviziju i ložišta, krovne ploče od staklo betona, nosača tervola i tvrdih tervol ploča za priključke, ventilacione rešetke, dilatacione rozete od nerđajućeg čelika. \nSpoljna dimenzija dimnjačkog plašta za fi14cm=32x32cm.","A single chimney diameter 140 mm.\nThree-layer prefabricated chimney system designed for all furnaces and all types of fuel, with no ventilation. It is composed of: chimney pipe of technical ceramics, pipe insulation around the chimney of stone wool minimum specific weight of 80kg/m3, external chimney mantle of lightweight concrete, refractory adhesive in cartouches, fireproof and gas impermeable certified three-layer side door, condensate pots, connectors for the audit and furnaces, roof tiles of glass concrete girders Tervola and hard tervol plate connections, ventilation grilles, rosettes expansion of stainless steel. The external dimensions of the chimney sleeve fi14cm = 32x32cm.","m1",null,{"$f":"KORISNICI!H161","v":24},{"$f":"G152*H152","v":0}]
[]
["9","V",null,"Vodovod Kanalizacija Oprema","WATER SUPPLY AND SEWAGE"]
[null,null,null,"Vodovod","WATER SUPPLY"]
["9.1","V",1,"Vodovodne polietilenske cevi  PE 100 PN16\nza radni pritisak 16 bara (SDR 11)","Water supply polyethylene pipe PE 100 PN16\nthe working pressure of 16 bar (SDR 11)","/","/","/","/"]
["9.1.1",null,"A","d25  (s min. 2,3)    - 3/4\"","d25  (s min. 2,3)    - 3/4\"","m1",null,{"$f":"KORISNICI!H166","v":0},{"$f":"G157*H157","v":0}]
["9.1.2",null,"B","d32  (s min. 3,0)   -       1\"","d32  (s min. 3,0)   -       1\"","m1",null,{"$f":"KORISNICI!H167","v":0},0]
["9.1.3",null,"C","d40  (s min. 3,7)   -  5/4\"","d40  (s min. 3,7)   -  5/4\"","m1",null,{"$f":"KORISNICI!H168","v":0},0]
["9.2","V",2,"Vodovodne cevi  PP-R 80 PN20 \nza radni pritisak 20 bara, bele ili zelene boje\n(materijal: polipropilen-random kapolimer)","Water pipe PP-R 80 PN20 \nthe working pressure of 20 bar, white or green \n(material: polypropylene random kapolimer)","/","/","/","/"]
["9.2.1",null,"B","d20  (s min.   3,4)    - 1/2\"","d20  (s min.   3,4)    - 1/2\"","m1",null,{"$f":"KORISNICI!H170","v":515},{"$f":"G161*H161","v":0}]
["9.2.2",null,"C","d25  (s min.   4,2)    - 3/4\"","d25  (s min.   4,2)    - 3/4\"","m1",null,{"$f":"KORISNICI!H171","v":0},0]
["9.2.3",null,"D","d32  (s min.   5,4)    -     1\"","d32  (s min.   5,4)    -     1\"","m1",null,{"$f":"KORISNICI!H172","v":20},0]
["9.3","V",3,"Vodomer \nsa prirubnicama, holenderima i pripadajućom opremom za montažu, za pritisak do 16 bara","water gauge\nflanges, unions and associated equipment for assembly, for pressure up to 16 bar","/","/","/","/"]
["9.3.1",null,"A","horizontalni 3/4\"    ","Horizontal 3/4\"    ","kom/pcs",null,{"$f":"KORISNICI!H174","v":0},{"$f":"G165*H165","v":0}]
["9.3.2",null,"B","horizontalni     1\"    ","Horizontal     1\"    ","kom/pcs",null,{"$f":"KORISNICI!H175","v":0},0]
["9.3.3",null,"C","horizontalni 5/4\"","Horizontal 5/4\"","kom/pcs",null,{"$f":"KORISNICI!H176","v":0},0]
["9.4","V",4,"Ravni propusni ventil sa ogrankom za pražnjenje","Skip straight valve with a branch drain","/","/","/","/"]
["9.4.1",null,"A","d25  (s min. 2,3)    - 3/4\"","d25  (s min. 2,3)    - 3/4\"","kom/pcs",null,{"$f":"KORISNICI!H178","v":0},{"$f":"G169*H169","v":0}]
["9.4.2",null,"B","d32  (s min. 3,0)   -       1\"","d32  (s min. 3,0)   -       1\"","kom/pcs",null,{"$f":"KORISNICI!H179","v":0},0]
["9.5","V",5,"Propusni ventil za uzidanje sa kapom ","Gate valve for the wall with cap","/","/","/","/"]
["9.5.1",null,"A","d20  (s min.   3,4)    - 1/2\"","d20  (s min.   3,4)    - 1/2\"","kom/pcs",null,{"$f":"KORISNICI!H181","v":74},{"$f":"G172*H172","v":0}]
["9.5.2",null,"B","d25  (s min.   4,2)    - 3/4\"","d25  (s min.   4,2)    - 3/4\"","kom/pcs",null,{"$f":"KORISNICI!H182","v":0},0]
["9.5.3",null,"C","d32  (s min. 3,0)   -       1\"","d32  (s min. 3,0)   -       1\"","kom/pcs",null,{"$f":"KORISNICI!H183","v":0},0]
["9.6","V",6,"Ugaoni \"EK\" sa kapom","Angle valve \"EK\" with cap","/","/","/","/"]
["9.6.1",null,"A","d20  (s min.   3,4)    - 1/2\"","d20  (s min.   3,4)    - 1/2\"","kom/pcs",null,{"$f":"KORISNICI!H185","v":74},{"$f":"G176*H176","v":0}]
["9.7","V",7,"Termička izolacija vodovodnih cevi  -tipa plamaflex ISO ili sl.","Thermal insulation of water pipes-type PLAMAFLEX ISO etc..","/","/","/","/"]
["9.7.1",null,"B","d20   (22/9)   - 1/2\"","d20   (22/9)   - 1/2\"","m1",null,{"$f":"KORISNICI!H187","v":0},{"$f":"G178*H178","v":0}]
["9.7.2",null,"C","d25   (25/9) - 3/4\"","d25   (25/9) - 3/4\"","m1",null,{"$f":"KORISNICI!H188","v":0},0]
["9.7.3",null,"D","d32   (35/9)-     1\"","d32   (35/9)-     1\"","m1",null,{"$f":"KORISNICI!H189","v":0},0]
[null,null,null,"Kanalizacija","SEWAGE"]
["9.8","V",8,"PVC kanalizacione cevi SDR 41 / SN4 / PN5\nza spoljni razvod, kućna i ulična kanalizacija","PVC sewer pipe SDR 41 / CH4 / PN5\nfor external distribution, household and street sewage","/","/","/","/"]
["9.8.1",null,"A","d110 (s min.   3,2)    dužina 6,0m","d110 (s min.   3,2)    length 6,0m","kom/pcs",null,{"$f":"KORISNICI!H192","v":0},{"$f":"G183*H183","v":0}]
["9.8.2",null,"B","d160 (s min.   4,0)    dužina 6,0m","d160 (s min.   4,0)    length 6,0m","kom/pcs",null,{"$f":"KORISNICI!H193","v":0},0]
["9.9","V",9,"Plastične PP cevi SDR 51 / SN2 / PN4\nza unutrašnji (kućni) razvod, kućna kanalizacija","Plastic PP pipes SDR 51 / SN2 / PN4\nfor internal (home) distribution, household sewage","/","/","/","/"]
["9.9.1",null,"A","d50     (s min.   1,8)    dužina 3,0m","d50     (s min.   1,8)    length 3,0m","kom/pcs",null,{"$f":"KORISNICI!H195","v":78},{"$f":"G186*H186","v":0}]
["9.9.2",null,"B","d75     (s min.   1,9)    dužina 3,0m","d75     (s min.   1,9)    length 3,0m","kom/pcs",null,{"$f":"KORISNICI!H196","v":0},0]
["9.9.3",null,"C","d110  (s min.   2,7)    dužina 3,0m","d110  (s min.   2,7)    length 3,0m","kom/pcs",null,{"$f":"KORISNICI!H197","v":32},0]
["9.10","V",10,"Plitki PE podni slivnik d50 sa horizontalnim odvodom dimenzija 150x150mm","Shallow PE floor drain with horizontal outlet d50 size 150x150mm","kom/pcs",null,{"$f":"KORISNICI!H198","v":16},0]
["9.11","V",11,"Zidni sifoni sa odvodnom mesinganom cevi d32 (mašina za pranje veša i sudova)","Wall siphon with drainage brass tubes d32 (washing machines, dishwashers)","kom/pcs",null,{"$f":"KORISNICI!H199","v":16},0]
[null,null,null,"Oprema u kupatilu","BATHROOM EQUPIMENT"]
["9.12","V",12,"WC šolja od keramike  I klase","Ceramic toilet bowl class 1","kom/pcs",null,{"$f":"KORISNICI!H201","v":17},{"$f":"G192*H192","v":0}]
["9.13","V",13,"Niskomontažni plastični predzidni vodokotlić \nza nisku montažu iznad wc šolje sa plovkom i svim potrebnim delovima za funkcionisanje vodokotlića","Low mounting plastic-wall toilet tank\nfor low installation above the toilet bowl float and all the parts required for the operation of flushing","kom/pcs",null,{"$f":"KORISNICI!H202","v":17},0]
["9.14","V",14,"Umivaonikom sa stubom od keramike  I klase","Washbasin with ceramic pillar class 1","kom/pcs",null,{"$f":"KORISNICI!H203","v":17},0]
["9.15","V",15,"Pravougaona akrilna tuš kada\ndimenzija 90x90cm sa odlivnim ventilom","Rectangular acrylic shower \nsize 90x90cm with discharge valve","kom/pcs",null,{"$f":"KORISNICI!H204","v":18},0]
["9.16","V",16,"Električni akumulacioni bojler 50l vertikalni \ngrejač 2 kW, napon 230V, kazan izrađen od emajliranog lima, sa  pratećim materijalom za ugradnju","Electric storage water heater 50l vertical \nheater 2 kW, 230V, caldron made ​​of enameled steel, with supporting material for installation","kom/pcs",null,{"$f":"KORISNICI!H205","v":17},0]
["9.17","V",17,"Ogledalo sa etažerom (iznad umivaonika)\nčetvrtasto, min. dimenzija 80x60cm","Mirror with shelf above wash basin \nsquare, min. 80x60cm","kom/pcs",null,{"$f":"KORISNICI!H206","v":17},0]
["9.18","V",18,"Baterije (slavine) \nhromirane baterije za hladnu i toplu vodu","Lever\nchrome lever for cold and hot water","/","/","/","/"]
["9.18.1",null,"A","za umivaonik jednoručna stojeća ","For washbasin single lever basin standing","kom/pcs",null,{"$f":"KORISNICI!H208","v":17},{"$f":"G199*H199","v":0}]
["9.18.2",null,"B","za tuš kadu (sa tuš ručicom i tuš crevom)\njednoručna sa poniklovanim savitljivim crevom","For shower bath (with shower head and shower hose) Single lever with nickel hoses","kom/pcs",null,{"$f":"KORISNICI!H209","v":17},0]
["9.18.3",null,"C","za mašinu za veš i sudove, holender slavina DN20/15, s pripadajućom opremom za ugradnju ","for washing machine and dishwasher, union DN20/15 taps, and all the equipment for installation","kom/pcs",null,{"$f":"KORISNICI!H210","v":17},0]
[null,null,null,"Oprema u kuhinji","KITCHEN EQUIPMENT"]
["9.19","V",19,"Korito sudopere od \"Inox \"-a (dvodelno)\n(izrađeno od plemenitog nerđajućeg čelika)\norjenacione dimenzije:  780 x 435 x 150 mm","kitchen sink \"Inox\" two-part\n(made of stainless steel)\napprox. dim:  780 x 435 x 150 mm","kom/pcs",null,{"$f":"KORISNICI!H212","v":9},{"$f":"G203*H203","v":0}]
["9.20","V",20,"Električni akumulacioni bojler 5l\nza ugradnju iznad sudopere, vertikalni grejač 2 kW, napon 230V, kazan izrađen od plastike\nsa  pratećim materijalom za ugradnju","Electric storage water heater 5l\nFitting over the sink, vertical heater 2 kW, 230V, caldron made ​​of plastic with the materials for installation","kom/pcs",null,{"$f":"KORISNICI!H213","v":8},0]
["9.21","V",21,"Baterija za sudoperu jednoručna stojeća hromirana baterija za hladnu i toplu vodu ","Sink-standing single lever chrome mixer for hot and cold water","kom/pcs",null,{"$f":"KORISNICI!H214","v":13},0]
[]
["10","E",null,"ELEKTRO MATERIJAL I OPREMA\n","Electrical materials and equipment"]
[null,null,null,"Kablovi i kablovski pribor","Electrical cables and cable accessories"]
["10.1","E",1,"Napojni kablovi","Power cables","/","/","/","/"]
["10.1.1",null,"A","X00-A      4x16 mm2","X00-A      4x16 mm2","m",null,{"$f":"KORISNICI!H219","v":0},{"$f":"G210*H210","v":0}]
["10.1.2",null,"B","PP00-Y   5x6    mm2","PP00-Y   5x6    mm2","m",null,{"$f":"KORISNICI!H220","v":0},0]
["10.1.3",null,"C","PP00-Y   5x10  mm2","PP00-Y   5x10  mm2","m",null,{"$f":"KORISNICI!H221","v":0},0]
["10.2","E",2,"Instalacioni kablovi","Installation cables","/","/","/","/"]
["10.2.1",null,"A","PP-Y       3x1,5  mm2","PP-Y       3x1,5  mm2","m",null,{"$f":"KORISNICI!H223","v":790},{"$f":"G214*H214","v":0}]
["10.2.2",null,"B","PP-Y       4x1,5  mm2","PP-Y       4x1,5  mm2","m",null,{"$f":"KORISNICI!H224","v":0},0]
["10.2.3",null,"C","PP-Y       3x2,5  mm2","PP-Y       3x2,5  mm2","m",null,{"$f":"KORISNICI!H225","v":1080},0]
["10.2.4",null,"D","PP-Y       5x2,5  mm2","PP-Y       5x2,5  mm2","m",null,{"$f":"KORISNICI!H226","v":620},0]
["10.3","E",3,"Instalacione PVC cevi","PVC pipe for installations of cables","/","/","/","/"]
["10.3.1",null,"A","fi 16mm2","fi 16mm2","m",null,{"$f":"KORISNICI!H228","v":0},{"$f":"G219*H219","v":0}]
["10.3.2",null,"B","fi 50mm2","fi 50mm2","m",null,{"$f":"KORISNICI!H229","v":0},0]
[null,null,null,"Razvodne table i oprema","The junction boards and equipment"]
["10.4","E",4,"Razvodna tabla Stanska, za ugradnju na zid sa transparentim vratima, sa mestom za 18 modula, DIN šinom, IP40\nRazvodna tabla sadrži :","Junction board (for flat) for wall mounting with transparent door, with space for 18 modules, DIN rail, IP40\nJunction board contains:","kom/pcs",null,{"$f":"KORISNICI!H231","v":8},{"$f":"G222*H222","v":0}]
[null,null,null,"Jednopolni instalacioni prekidač\n(automatski osigurač) za montažu na DIN šinu nom. napona 230V/400V, 50Hz; karakteristike B; prekidne moći 6kA:","Single-pole fuse\n(Automatic fuse) for mounting on DIN rail nom. voltage 230V/400V, 50Hz, features B; breaking capacity 6kA:","/","/","/","/"]
[null,null,null,"nazivne struje 6A, komada 1","rated current of 6A","kom/pcs","/","/","/"]
[null,null,null,"nazivne struje 10A, komada 2","rated current of 10A","kom/pcs","/","/","/"]
[null,null,null,"nazivne struje 16A, komada 9","rated current of 16A","kom/pcs","/","/","/"]
[null,null,null,"Signalna sijalica\nza signalizaciju tarife 230V za ugradnju u stansku razvodnu tablu, montažu na DIN šinu, komada 1","The indicator lamp\nfor signaling rates 230V for use in flat junction board, mounting on DIN rail","kom/pcs","/","/","/"]
[null,null,null,"FID sklopka za ugradnju u stansku razvodnu tablu, montažu na DIN šinu, ","FID switch for installation in junction board, mounting on DIN rail","/","/","/","/"]
[null,null,null,"16A/30mA,  2-polna,   230V, 50Hz; komada 2","16A/30mA, 2-pole, 230V, 50Hz;","kom/pcs","/","/","/"]
[null,null,null,"25A/0,5A,    4-polna,    230V/400V, 50Hz; komada 1","25A / 0,5 A, 4-pole, 230V/400V, 50Hz;","kom/pcs","/","/","/"]
[null,null,null,"Instalaciono zvono 230V, 50Hz; za ugradnju u stansku razvodnu tablu, montažu na DIN šinu, komada 1","Bell 230V, 50Hz, for use in junction board, mounting on DIN rail","kom/pcs","/","/","/"]
[null,null,null,"Instalacioni materijal","Installation material"]
["10.5","E",5,"Instalaciona kutija\nza ugradnju u završnu obradu zida","Installation box\nfor installation in the wall","/","/","/","/"]
["10.5.1",null,"A","fi 60 mm","fi 60 mm","kom/pcs",null,{"$f":"KORISNICI!H243","v":140},{"$f":"G234*H234","v":0}]
["10.5.2",null,"B","fi 78 mm","fi 78 mm","kom/pcs",null,{"$f":"KORISNICI!H244","v":89},0]
["10.5.3",null,"C","100x100mm","100x100mm","kom/pcs",null,{"$f":"KORISNICI!H245","v":63},0]
["10.6","E",6,"Instalaciona priključnica IP20 za ugradnju u završnu obradu zida sa zaštitnim kontaktom","Installation socket IP20 for installation in the wall with a protection contact","/","/","/","/"]
["10.6.1",null,"A","16A, monofazna, 250 V","16A, single-phase, 250 V","kom/pcs",null,{"$f":"KORISNICI!H247","v":91},{"$f":"G238*H238","v":0}]
["10.6.2",null,"B","16A, monofazna, dupla, 250 V","16A, single-phase, double, 250 V","kom/pcs",null,{"$f":"KORISNICI!H248","v":64},0]
["10.6.3",null,"C","16A, trofazna, 400V","16A, three-phase, 400V","kom/pcs",null,{"$f":"KORISNICI!H249","v":13},0]
["10.7","E",7,"Instalaciona priključnica IP43 sa poklopcem za ugradnju u završnu obradu zida, sa zaštit. kontaktom, 16A, monofazna, 250 V","Installation socket IP43 with cover for use in wall with protection. contact, 16A, single-phase, 250 V","kom/pcs",null,{"$f":"KORISNICI!H250","v":9},0]
["10.8","E",8,"Prekidači\n IP20 za ugradnju u završnu obradu zida","Switches \n IP20 for installation in wall","/","/","/","/"]
["10.8.1",null,"A","običan, 10A","regular, 10A","kom/pcs",null,{"$f":"KORISNICI!H252","v":74},{"$f":"G243*H243","v":0}]
["10.8.2",null,"B","serijski, 10A","serial, 10A","kom/pcs",null,{"$f":"KORISNICI!H253","v":36},0]
["10.8.3",null,"C","za zvono ","for bell","kom/pcs",null,{"$f":"KORISNICI!H254","v":9},0]
["10.8.4",null,"D","Instalacioni  prekidač \"KIP\" 16A","Installation switch \"KIP\" 16A","kom/pcs",null,{"$f":"KORISNICI!H255","v":9},0]
["10.9","E",9,"Indikator za kupatilo\n sa tri sklopke 16A i signalnim sijalicama","The indicator for the bathroom \nThree switches 16A and signal lights","kom/pcs",null,{"$f":"KORISNICI!H256","v":13},0]
[null,null,null,"Svetiljke","Lighting"]
["10.10","E",10,"Svetiljka za montažu na plafon  sa inkadescentnom sijalicom 60W, E-27, ","Luminaire to be mounted on the ceiling with a 60W incandescent bulb, E-27","/","/","/","/"]
["10.10.1",null,"A"," IP 43 za sanitarni čvor","IP 43 for toilet",null,null,{"$f":"KORISNICI!H259","v":13},{"$f":"G250*H250","v":0}]
["10.10.2",null,"B","IP 20 za unutrašnje prostorije","IP 20 for indoor rooms",null,null,{"$f":"KORISNICI!H260","v":61},0]
[null,null,null,"Instalacija uzemljenja i gromobrana","Earthing and lightning protection"]
["10.11","E",11,"Pocinkovana traka","Galvanized strip",null,null,"/","/"]
["10.11.1",null,"A","FeZn 25x4mm","FeZn 25x4mm","m",null,{"$f":"KORISNICI!H263","v":0},{"$f":"G254*H254","v":0}]
["10.11.2",null,"B","FeZn 20x3mm","FeZn 20x3mm","m",null,{"$f":"KORISNICI!H264","v":0},0]
["10.12","E",12,"SIP ormarić (PS49) sa sabirnicom za izjednačenje potencijala","SIP boxes (PS 49) with bonding","kom/pcs",null,{"$f":"KORISNICI!H265","v":0},0]
["10.13","E",13,"Provodnici za uzemljenje","Grounding conductors","/","/","/","/"]
["10.13.1",null,"A","PP00-Y  1x16mm2","PP00-Y  1x16mm2","m",null,{"$f":"KORISNICI!H267","v":0},{"$f":"G258*H258","v":0}]
["10.13.2",null,"B","P/F-Y      1x6mm2","P/F-Y      1x6mm2","m",null,{"$f":"KORISNICI!H268","v":0},0]
["10.13.3",null,"C","P/F-Y      1x4mm2","P/F-Y      1x4mm2","m",null,{"$f":"KORISNICI!H269","v":0},0]
[null,null,null,"Instalacija slabe struje","Installation of low voltage"]
["10.14","E",14,"Antenski koaksijalni kabl RG 6","Antenna Coaxial Cable RG 6","m",null,{"$f":"KORISNICI!H271","v":0},{"$f":"G262*H262","v":0}]
["10.15","E",15,"Telefonski kabl sa bakarnim provodnicima \nIY(St)Y 2x2x0.8mm","Telephone cable with copper conductors \nIY (St) Y 2x2x0.8mm","m",null,{"$f":"KORISNICI!H272","v":0},0]
["10.16","E",16,"Priključnice","Connectors","/","/","/","/"]
["10.16.1",null,"A","Telefonska - RJ11 za montažu u dozni fi 60mm","Phone - RJ11 for mounting in enclosure fi 60mm","m",null,{"$f":"KORISNICI!H274","v":0},{"$f":"G265*H265","v":0}]
["10.16.2",null,"B","RTV priključnica za montažu u dozni fi 60mm","RTV connector for mounting in enclosure fi 60 mm","kom/pcs",null,{"$f":"KORISNICI!H275","v":0},0]
[null,null,null,null,null,null,null,null,{"$f":"SUM(I5:I266)","v":0}]

{"sheet":"KORISNICI","index":2,"n_rows":276,"n_cols":83,"rows_kept":276,"cut":false,"hidden":false,"merged":[]}
[null,null,null,null,null,null,"POTPROJEKAT/ SUBPROJECT",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4",null,null,"SRB4"]
[null,null,null,null,null,null,"ID KORISNIKA/ USER ID",null,{"$f":"COUNTA(J2:CA2)","v":24},1,null,null,2,null,null,3,null,null,4,null,null,5,null,null,6,null,null,7,null,null,8,null,null,9,null,null,10,null,null,11,null,null,12,null,null,13,null,null,14,null,null,15,null,null,16,null,null,17,null,null,18,null,null,19,null,null,20,null,null,21,null,null,22,null,null,23,null,null,24]
[null,null,null,null,null,null,"IME KORISNIKA/ NAME",null,{"$f":"COUNTA(J3:CA3)","v":24},"Svetlana ",null,null,"Ljubinka ",null,null,"Dušan",null,null,"Pero",null,null,"Ana",null,null,"Branko",null,null,"Saša",null,null,"Borislav ",null,null,"Desa",null,null,"Sanja ",null,null,"Mirjana ",null,null,"Dragan ",null,null,"Ljuba ",null,null,"Dušan",null,null,"Stevo",null,null,"Željko ",null,null,"Milorad ",null,null,"Mira ",null,null,"Velimir",null,null,"Miroslav",null,null,"Rade",null,null,"Mile",null,null,"Mile",null,null,"Milka"]
[null,null,null,null,null,null,"PREZIME KORISNIKA/ SURNAME",null,24,"Kovačević",null,null,"Popović",null,null,"Ilić",null,null,"Smrzlić",null,null,"Ostojić",null,null,"Kuduz",null,null,"Janačković",null,null,"Purić",null,null,"Đurić",null,null,"Ivčić",null,null,"Ivanišević",null,null,"Tomašević ",null,null,"Pantelić",null,null,"Beader",null,null,"Vujčić",null,null,"Pećanac",null,null,"Svjetlanović",null,null,"Vujović",null,null,"Subašić",null,null,"Vrbljanac",null,null,"Šakić",null,null,"Lukić",null,null,"Kecman",null,null,"Bebek"]
[null,null,null,null,null,null,"TELEFON KORISNIKA/ PHONE",null,24,"0641617995",null,null,643629473,null,null,643974350,null,null,649117164,null,null,618149807,null,null,62351652,null,null,23077696,null,null,23077933,null,null,641191074,null,null,642437992,null,null,616272223,null,null,23066237,null,null,644292019,null,null,628472445,null,null,642115970,null,null,638633858,null,null,644098831,null,null,646656964,null,null,640489625,null,null,642920188,null,null,631120059,null,null,23071027,null,null,230454869,null,null,230454869]
[null,null,null,null,null,null,"OPŠTINA ISPORUKE/ MUNICIPALITY",null,24,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda ",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda",null,null,"Kikinda"]
[null,null,null,null,null,null,"MESTO ISPORUKE/ CITY",null,24,"Iđoš",null,null,"Bikač",null,null,"Sajan",null,null,"Ostojićevo",null,null,"Ostojićevo",null,null,"Nakovo",null,null,"Ostojićevo",null,null,"Ostojićevo",null,null,"Kikinda",null,null,"Kikinda",null,null,"Crna Bara",null,null,"Sajan",null,null,"Kikinda ",null,null,"Novi Kneževac",null,null,"Padej",null,null,"Banatsko Veliko Selo",null,null,"Ostojićevo",null,null,"Rusko Selo",null,null,"Crna Bara",null,null,"Rusko Selo",null,null,"Čoka",null,null,"Čoka",null,null,"Nakovo",null,null,"Sanad"]
[null,null,null,null,null,null,"LOKACIJA ISPORUKE/ LOCATION OF DELIVERY",null,24,"Žarka Zrenjanina 22",null,null,"Jovana Popovića 56",null,null,"Egete Jožefa 9",null,null,"Kosovska 86",null,null,"Štrosmajerova 4",null,null,"Miladina Zorića 16",null,null,"Obilićeva 15",null,null,"Sinđelićeva 20",null,null,"Teremijski drum 30",null,null,"Kiš Mihalja 6",null,null,"Dože Đerđa 8",null,null,"Mora Karolja 8",null,null,"Rade Trnića 37",null,null,"Branka Radičevića 100",null,null,"Beogradska 11",null,null,"Vojvođanska 1",null,null,"Miletićeva 37",null,null,"Solunskih Dobrovoljaca 8",null,null,"JNA 66",null,null,"Vojvode Knićanina 57",null,null,"Borisa Kidrića 10",null,null,"Vuka Karadžića",null,null,"Glavna 83",null,null,"Hajduk Veljka 27"]
[null,null,null,null,null,null,"UKUPNO PO KORISNIKU/ TOTAL BY BENEFICIARY",null,24,{"$f":"K276","v":0},null,null,{"$f":"N276","v":0},null,null,{"$f":"Q276","v":0},null,null,{"$f":"T276","v":0},null,null,{"$f":"W276","v":0},null,null,{"$f":"Z276","v":0},null,null,{"$f":"AC276","v":0},null,null,{"$f":"AF276","v":0},null,null,{"$f":"AI276","v":0},null,null,{"$f":"AL276","v":0},null,null,{"$f":"AO276","v":0},null,null,{"$f":"AR276","v":0},null,null,{"$f":"AU276","v":0},null,null,{"$f":"AX276","v":0},null,null,{"$f":"BA276","v":0},null,null,{"$f":"BD276","v":0},null,null,{"$f":"BG276","v":0},null,null,{"$f":"BJ276","v":0},null,null,{"$f":"BM276","v":0},null,null,{"$f":"BP276","v":0},null,null,{"$f":"BS276","v":0},null,null,{"$f":"BV276","v":0},null,null,{"$f":"BY276","v":0},null,null,{"$f":"CB276","v":0}]
[null,null,null,null,null,null,null,"LOT 1"]
["KOD/\nCODE",null,null,"Opis građevinskog materijala ","Description of building materials","Jed.\nprod./\nUNIT","Jedinična\nprod.cena/\nUNIT PRICE ","Zbir Količina po materijalima/\nSUM QTY","ZBIR UKUPNO PO MATERIJALIMA/\nSUM PRICE","Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL",null,"Količina/\nQTY","UKUPNO/\nTOTAL"]
[null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"ID\",J2)","v":"ID1"},null,null,{"$f":"CONCATENATE(\"ID\",M2)","v":"ID2"},null,null,{"$f":"CONCATENATE(\"ID\",P2)","v":"ID3"},null,null,{"$f":"CONCATENATE(\"ID\",S2)","v":"ID4"},null,null,{"$f":"CONCATENATE(\"ID\",V2)","v":"ID5"},null,null,{"$f":"CONCATENATE(\"ID\",Y2)","v":"ID6"},null,null,{"$f":"CONCATENATE(\"ID\",AB2)","v":"ID7"},null,null,{"$f":"CONCATENATE(\"ID\",AE2)","v":"ID8"},null,null,{"$f":"CONCATENATE(\"ID\",AH2)","v":"ID9"},null,null,{"$f":"CONCATENATE(\"ID\",AK2)","v":"ID10"},null,null,{"$f":"CONCATENATE(\"ID\",AN2)","v":"ID11"},null,null,{"$f":"CONCATENATE(\"ID\",AQ2)","v":"ID12"},null,null,{"$f":"CONCATENATE(\"ID\",AT2)","v":"ID13"},null,null,{"$f":"CONCATENATE(\"ID\",AW2)","v":"ID14"},null,null,{"$f":"CONCATENATE(\"ID\",AZ2)","v":"ID15"},null,null,{"$f":"CONCATENATE(\"ID\",BC2)","v":"ID16"},null,null,{"$f":"CONCATENATE(\"ID\",BF2)","v":"ID17"},null,null,{"$f":"CONCATENATE(\"ID\",BI2)","v":"ID18"},null,null,{"$f":"CONCATENATE(\"ID\",BL2)","v":"ID19"},null,null,{"$f":"CONCATENATE(\"ID\",BO2)","v":"ID20"},null,null,{"$f":"CONCATENATE(\"ID\",BR2)","v":"ID21"},null,null,{"$f":"CONCATENATE(\"ID\",BU2)","v":"ID22"},null,null,{"$f":"CONCATENATE(\"ID\",BX2)","v":"ID23"},null,null,{"$f":"CONCATENATE(\"ID\",CA2)","v":"ID24"}]
[1,"A",null,"OSNOVNI GRAĐEVINSKI MATERIJAL","BASIC BUILDING MATERIALS"]
["1.1","O",1,"Cement  za betone do MB 30","Cement for concrete up to 30 MB","kg",{"$f":"CENA!G5","v":0},{"$f":"J14+M14+P14+S14+V14+Y14+AB14+AE14+AH14+AK14+AN14+AQ14+AT14+AW14+AZ14+BC14+BF14+BI14+BL14+BO14+BR14+BU14+BX14+CA14","v":97950},{"$f":"G14*H14","v":0},12950,{"$f":"$G14*J14","v":0},null,3150,{"$f":"$G14*M14","v":0},null,10000,{"$f":"$G14*P14","v":0},null,2000,{"$f":"$G14*S14","v":0},null,10000,{"$f":"$G14*V14","v":0},null,3100,{"$f":"$G14*Y14","v":0},null,2450,{"$f":"$G14*AB14","v":0},null,12650,{"$f":"$G14*AE14","v":0},null,2100,{"$f":"$G14*AH14","v":0},null,1100,{"$f":"$G14*AK14","v":0},null,1500,{"$f":"$G14*AN14","v":0},null,3500,{"$f":"$G14*AQ14","v":0},null,1800,{"$f":"$G14*AT14","v":0},null,4250,{"$f":"$G14*AW14","v":0},null,800,{"$f":"$G14*AZ14","v":0},null,3650,{"$f":"$G14*BC14","v":0},null,2100,{"$f":"$G14*BF14","v":0},null,1050,{"$f":"$G14*BI14","v":0},null,1400,{"$f":"$G14*BL14","v":0},null,6100,{"$f":"$G14*BO14","v":0},null,3500,{"$f":"$G14*BR14","v":0},null,7050,{"$f":"$G14*BU14","v":0},null,750,{"$f":"$G14*BX14","v":0},null,1000,{"$f":"$G14*CA14","v":0}]
["1.2","O",2,"Hidratisani gašeni kreč pripremljen u prahu","Hydrated slaked lime powdered","kg",{"$f":"CENA!G6","v":0},{"$f":"J15+M15+P15+S15+V15+Y15+AB15+AE15+AH15+AK15+AN15+AQ15+AT15+AW15+AZ15+BC15+BF15+BI15+BL15+BO15+BR15+BU15+BX15+CA15","v":11150},{"$f":"G15*H15","v":0},1000,{"$f":"$G15*J15","v":0},null,500,0,null,600,{"$f":"$G15*P15","v":0},null,1200,{"$f":"$G15*S15","v":0},null,1500,{"$f":"$G15*V15","v":0},null,400,{"$f":"$G15*Y15","v":0},null,250,{"$f":"$G15*AB15","v":0},null,1200,{"$f":"$G15*AE15","v":0},null,400,{"$f":"$G15*AH15","v":0},null,0,{"$f":"$G15*AK15","v":0},null,200,{"$f":"$G15*AN15","v":0},null,600,{"$f":"$G15*AQ15","v":0},null,0,{"$f":"$G15*AT15","v":0},null,0,{"$f":"$G15*AW15","v":0},null,200,{"$f":"$G15*AZ15","v":0},null,400,{"$f":"$G15*BC15","v":0},null,400,{"$f":"$G15*BF15","v":0},null,500,{"$f":"$G15*BI15","v":0},null,200,{"$f":"$G15*BL15","v":0},null,600,{"$f":"$G15*BO15","v":0},null,400,{"$f":"$G15*BR15","v":0},null,600,{"$f":"$G15*BU15","v":0},null,0,{"$f":"$G15*BX15","v":0},null,0,{"$f":"$G15*CA15","v":0}]
["1.3","O",3,"Rebrasto betonsko gvožđe (RA) ","Ribbed reinforcement steel","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["1.3.1",null,"A","10 mm   - dužine 12m","10 mm   - length 12m ","kg",{"$f":"CENA!G8","v":0},{"$f":"J17+M17+P17+S17+V17+Y17+AB17+AE17+AH17+AK17+AN17+AQ17+AT17+AW17+AZ17+BC17+BF17+BI17+BL17+BO17+BR17+BU17+BX17+CA17","v":402.48},{"$f":"G17*H17","v":0},0,{"$f":"$G17*J17","v":0},{"$f":"J17/$CE$17","v":0},0,{"$f":"$G17*M17","v":0},{"$f":"M17/$CE$17","v":0},0,{"$f":"$G17*P17","v":0},{"$f":"P17/$CE$17","v":0},92.88,{"$f":"$G17*S17","v":0},{"$f":"S17/$CE$17","v":11.999999999999998},309.60000000000002,{"$f":"$G17*V17","v":0},{"$f":"V17/$CE$17","v":40},0,{"$f":"$G17*Y17","v":0},{"$f":"Y17/$CE$17","v":0},0,{"$f":"$G17*AB17","v":0},{"$f":"AB17/$CE$17","v":0},0,{"$f":"$G17*AE17","v":0},{"$f":"AE17/$CE$17","v":0},0,{"$f":"$G17*AH17","v":0},{"$f":"AH17/$CE$17","v":0},0,{"$f":"$G17*AK17","v":0},{"$f":"AK17/$CE$17","v":0},0,{"$f":"$G17*AN17","v":0},{"$f":"AN17/$CE$17","v":0},0,{"$f":"$G17*AQ17","v":0},{"$f":"AQ17/$CE$17","v":0},0,{"$f":"$G17*AT17","v":0},{"$f":"AT17/$CE$17","v":0},0,{"$f":"$G17*AW17","v":0},{"$f":"AW17/$CE$17","v":0},0,{"$f":"$G17*AZ17","v":0},{"$f":"AZ17/$CE$17","v":0},0,{"$f":"$G17*BC17","v":0},{"$f":"BC17/$CE$17","v":0},0,{"$f":"$G17*BF17","v":0},{"$f":"BF17/$CE$17","v":0},0,{"$f":"$G17*BI17","v":0},{"$f":"BI17/$CE$17","v":0},0,{"$f":"$G17*BL17","v":0},{"$f":"BL17/$CE$17","v":0},0,{"$f":"$G17*BO17","v":0},{"$f":"BO17/$CE$17","v":0},0,{"$f":"$G17*BR17","v":0},{"$f":"BR17/$CE$17","v":0},0,{"$f":"$G17*BU17","v":0},{"$f":"BU17/$CE$17","v":0},0,{"$f":"$G17*BX17","v":0},{"$f":"BX17/$CE$17","v":0},0,{"$f":"$G17*CA17","v":0},{"$f":"CA17/$CE$17","v":0},null,7.74]
["1.3.2",null,"B","12 mm   - dužine 12m","12 mm   - length 12m","kg",{"$f":"CENA!G9","v":0},{"$f":"J18+M18+P18+S18+V18+Y18+AB18+AE18+AH18+AK18+AN18+AQ18+AT18+AW18+AZ18+BC18+BF18+BI18+BL18+BO18+BR18+BU18+BX18+CA18","v":6082.4400000000005},{"$f":"G18*H18","v":0},690.68000000000006,{"$f":"$G18*J18","v":0},{"$f":"J18/$CE$18","v":62},178.24,0,{"$f":"M18/$CE$18","v":16},690.68000000000006,{"$f":"$G18*P18","v":0},{"$f":"P18/$CE$18","v":62},133.68,{"$f":"$G18*S18","v":0},{"$f":"S18/$CE$18","v":12},200.52,{"$f":"$G18*V18","v":0},{"$f":"V18/$CE$18","v":18},278.5,{"$f":"$G18*Y18","v":0},{"$f":"Y18/$CE$18","v":25},55.7,{"$f":"$G18*AB18","v":0},{"$f":"AB18/$CE$18","v":5},690.68000000000006,{"$f":"$G18*AE18","v":0},{"$f":"AE18/$CE$18","v":62},0,{"$f":"$G18*AH18","v":0},{"$f":"AH18/$CE$18","v":0},178.24,{"$f":"$G18*AK18","v":0},{"$f":"AK18/$CE$18","v":16},0,{"$f":"$G18*AN18","v":0},{"$f":"AN18/$CE$18","v":0},345.34000000000003,{"$f":"$G18*AQ18","v":0},{"$f":"AQ18/$CE$18","v":31},278.5,{"$f":"$G18*AT18","v":0},{"$f":"AT18/$CE$18","v":25},178.24,{"$f":"$G18*AW18","v":0},{"$f":"AW18/$CE$18","v":16},0,{"$f":"$G18*AZ18","v":0},{"$f":"AZ18/$CE$18","v":0},245.08,{"$f":"$G18*BC18","v":0},{"$f":"BC18/$CE$18","v":22},0,{"$f":"$G18*BF18","v":0},{"$f":"BF18/$CE$18","v":0},0,{"$f":"$G18*BI18","v":0},{"$f":"BI18/$CE$18","v":0},200.52,{"$f":"$G18*BL18","v":0},{"$f":"BL18/$CE$18","v":18},523.58000000000004,{"$f":"$G18*BO18","v":0},{"$f":"BO18/$CE$18","v":47},523.58000000000004,{"$f":"$G18*BR18","v":0},{"$f":"BR18/$CE$18","v":47},690.68000000000006,{"$f":"$G18*BU18","v":0},{"$f":"BU18/$CE$18","v":62},0,{"$f":"$G18*BX18","v":0},{"$f":"BX18/$CE$18","v":0},0,{"$f":"$G18*CA18","v":0},{"$f":"CA18/$CE$18","v":0},null,11.14]
["1.3.3",null,"C","14 mm   - dužine 12m","14 mm   - length 12m","kg",{"$f":"CENA!G10","v":0},{"$f":"J19+M19+P19+S19+V19+Y19+AB19+AE19+AH19+AK19+AN19+AQ19+AT19+AW19+AZ19+BC19+BF19+BI19+BL19+BO19+BR19+BU19+BX19+CA19","v":0},{"$f":"G19*H19","v":0},0,{"$f":"$G19*J19","v":0},{"$f":"J19/$CE$19","v":0},0,0,{"$f":"M19/$CE$19","v":0},0,{"$f":"$G19*P19","v":0},{"$f":"P19/$CE$19","v":0},0,{"$f":"$G19*S19","v":0},{"$f":"S19/$CE$19","v":0},0,{"$f":"$G19*V19","v":0},{"$f":"V19/$CE$19","v":0},0,{"$f":"$G19*Y19","v":0},{"$f":"Y19/$CE$19","v":0},0,{"$f":"$G19*AB19","v":0},{"$f":"AB19/$CE$19","v":0},0,{"$f":"$G19*AE19","v":0},{"$f":"AE19/$CE$19","v":0},0,{"$f":"$G19*AH19","v":0},{"$f":"AH19/$CE$19","v":0},0,{"$f":"$G19*AK19","v":0},{"$f":"AK19/$CE$19","v":0},0,{"$f":"$G19*AN19","v":0},{"$f":"AN19/$CE$19","v":0},0,{"$f":"$G19*AQ19","v":0},{"$f":"AQ19/$CE$19","v":0},0,{"$f":"$G19*AT19","v":0},{"$f":"AT19/$CE$19","v":0},0,{"$f":"$G19*AW19","v":0},{"$f":"AW19/$CE$19","v":0},0,{"$f":"$G19*AZ19","v":0},{"$f":"AZ19/$CE$19","v":0},0,{"$f":"$G19*BC19","v":0},{"$f":"BC19/$CE$19","v":0},0,{"$f":"$G19*BF19","v":0},{"$f":"BF19/$CE$19","v":0},0,{"$f":"$G19*BI19","v":0},{"$f":"BI19/$CE$19","v":0},0,{"$f":"$G19*BL19","v":0},{"$f":"BL19/$CE$19","v":0},0,{"$f":"$G19*BO19","v":0},{"$f":"BO19/$CE$19","v":0},0,{"$f":"$G19*BR19","v":0},{"$f":"BR19/$CE$19","v":0},0,{"$f":"$G19*BU19","v":0},{"$f":"BU19/$CE$19","v":0},0,{"$f":"$G19*BX19","v":0},{"$f":"BX19/$CE$19","v":0},0,{"$f":"$G19*CA19","v":0},{"$f":"CA19/$CE$19","v":0},null,15.17]
["1.3.4",null,"D","16 mm   - dužine 12m","16 mm   - length 12m","kg",{"$f":"CENA!G11","v":0},{"$f":"J20+M20+P20+S20+V20+Y20+AB20+AE20+AH20+AK20+AN20+AQ20+AT20+AW20+AZ20+BC20+BF20+BI20+BL20+BO20+BR20+BU20+BX20+CA20","v":0},{"$f":"G20*H20","v":0},null,{"$f":"$G20*J20","v":0},{"$f":"J20/$CE$20","v":0},null,0,{"$f":"M20/$CE$20","v":0},null,{"$f":"$G20*P20","v":0},{"$f":"P20/$CE$20","v":0},null,{"$f":"$G20*S20","v":0},{"$f":"S20/$CE$20","v":0},null,{"$f":"$G20*V20","v":0},{"$f":"V20/$CE$20","v":0},null,{"$f":"$G20*Y20","v":0},{"$f":"Y20/$CE$20","v":0},null,{"$f":"$G20*AB20","v":0},{"$f":"AB20/$CE$20","v":0},null,{"$f":"$G20*AE20","v":0},{"$f":"AE20/$CE$20","v":0},null,{"$f":"$G20*AH20","v":0},{"$f":"AH20/$CE$20","v":0},null,{"$f":"$G20*AK20","v":0},{"$f":"AK20/$CE$20","v":0},null,{"$f":"$G20*AN20","v":0},{"$f":"AN20/$CE$20","v":0},null,{"$f":"$G20*AQ20","v":0},{"$f":"AQ20/$CE$20","v":0},null,{"$f":"$G20*AT20","v":0},{"$f":"AT20/$CE$20","v":0},null,{"$f":"$G20*AW20","v":0},{"$f":"AW20/$CE$20","v":0},null,{"$f":"$G20*AZ20","v":0},{"$f":"AZ20/$CE$20","v":0},null,{"$f":"$G20*BC20","v":0},{"$f":"BC20/$CE$20","v":0},null,{"$f":"$G20*BF20","v":0},{"$f":"BF20/$CE$20","v":0},null,{"$f":"$G20*BI20","v":0},{"$f":"BI20/$CE$20","v":0},null,{"$f":"$G20*BL20","v":0},{"$f":"BL20/$CE$20","v":0},null,{"$f":"$G20*BO20","v":0},{"$f":"BO20/$CE$20","v":0},null,{"$f":"$G20*BR20","v":0},{"$f":"BR20/$CE$20","v":0},null,{"$f":"$G20*BU20","v":0},{"$f":"BU20/$CE$20","v":0},null,{"$f":"$G20*BX20","v":0},{"$f":"BX20/$CE$20","v":0},null,{"$f":"$G20*CA20","v":0},{"$f":"CA20/$CE$20","v":0},null,19.809999999999999]
["1.4","O",4,"Glatko betonsko gvožđe (GA) ","Glibly reinforcement steel","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["1.4.1",null,"B","  8 mm   - dužine 12m","  8 mm   - length 12m","kg",{"$f":"CENA!G13","v":0},{"$f":"J22+M22+P22+S22+V22+Y22+AB22+AE22+AH22+AK22+AN22+AQ22+AT22+AW22+AZ22+BC22+BF22+BI22+BL22+BO22+BR22+BU22+BX22+CA22","v":1763.2800000000002},{"$f":"G22*H22","v":0},189.60000000000002,{"$f":"$G22*J22","v":0},{"$f":"J22/$CE$22","v":40},47.400000000000006,{"$f":"$G22*M22","v":0},{"$f":"M22/$CE$22","v":10},189.60000000000002,{"$f":"$G22*P22","v":0},{"$f":"P22/$CE$22","v":40},47.4,{"$f":"$G22*S22","v":0},{"$f":"S22/$CE$22","v":10},142.19999999999999,{"$f":"$G22*V22","v":0},{"$f":"V22/$CE$22","v":29.999999999999996},75.84,{"$f":"$G22*Y22","v":0},{"$f":"Y22/$CE$22","v":16},23.7,{"$f":"$G22*AB22","v":0},{"$f":"AB22/$CE$22","v":5},189.60000000000002,{"$f":"$G22*AE22","v":0},{"$f":"AE22/$CE$22","v":40},0,{"$f":"$G22*AH22","v":0},{"$f":"AH22/$CE$22","v":0},47.400000000000006,{"$f":"$G22*AK22","v":0},{"$f":"AK22/$CE$22","v":10},0,{"$f":"$G22*AN22","v":0},{"$f":"AN22/$CE$22","v":0},94.800000000000011,{"$f":"$G22*AQ22","v":0},{"$f":"AQ22/$CE$22","v":20},75.84,{"$f":"$G22*AT22","v":0},{"$f":"AT22/$CE$22","v":16},47.400000000000006,{"$f":"$G22*AW22","v":0},{"$f":"AW22/$CE$22","v":10},0,{"$f":"$G22*AZ22","v":0},{"$f":"AZ22/$CE$22","v":0},66.36,{"$f":"$G22*BC22","v":0},{"$f":"BC22/$CE$22","v":14},0,{"$f":"$G22*BF22","v":0},{"$f":"BF22/$CE$22","v":0},0,{"$f":"$G22*BI22","v":0},{"$f":"BI22/$CE$22","v":0},52.14,{"$f":"$G22*BL22","v":0},{"$f":"BL22/$CE$22","v":11},142.20000000000002,{"$f":"$G22*BO22","v":0},{"$f":"BO22/$CE$22","v":30.000000000000004},142.20000000000002,{"$f":"$G22*BR22","v":0},{"$f":"BR22/$CE$22","v":30.000000000000004},189.60000000000002,{"$f":"$G22*BU22","v":0},{"$f":"BU22/$CE$22","v":40},0,{"$f":"$G22*BX22","v":0},{"$f":"BX22/$CE$22","v":0},0,{"$f":"$G22*CA22","v":0},{"$f":"CA22/$CE$22","v":0},null,4.74]
["1.4.2",null,"C","10 mm  - dužine 12m","10 mm  - length 12m","kg",{"$f":"CENA!G14","v":0},{"$f":"J23+M23+P23+S23+V23+Y23+AB23+AE23+AH23+AK23+AN23+AQ23+AT23+AW23+AZ23+BC23+BF23+BI23+BL23+BO23+BR23+BU23+BX23+CA23","v":0},{"$f":"G23*H23","v":0},null,{"$f":"$G23*J23","v":0},{"$f":"J23/$CE$23","v":0},null,0,{"$f":"M23/$CE$23","v":0},null,{"$f":"$G23*P23","v":0},{"$f":"P23/$CE$23","v":0},null,{"$f":"$G23*S23","v":0},{"$f":"S23/$CE$23","v":0},null,{"$f":"$G23*V23","v":0},{"$f":"V23/$CE$23","v":0},null,{"$f":"$G23*Y23","v":0},{"$f":"Y23/$CE$23","v":0},null,{"$f":"$G23*AB23","v":0},{"$f":"AB23/$CE$23","v":0},null,{"$f":"$G23*AE23","v":0},{"$f":"AE23/$CE$23","v":0},null,{"$f":"$G23*AH23","v":0},{"$f":"AH23/$CE$23","v":0},null,{"$f":"$G23*AK23","v":0},{"$f":"AK23/$CE$23","v":0},null,{"$f":"$G23*AN23","v":0},{"$f":"AN23/$CE$23","v":0},null,{"$f":"$G23*AQ23","v":0},{"$f":"AQ23/$CE$23","v":0},null,{"$f":"$G23*AT23","v":0},{"$f":"AT23/$CE$23","v":0},null,{"$f":"$G23*AW23","v":0},{"$f":"AW23/$CE$23","v":0},null,{"$f":"$G23*AZ23","v":0},{"$f":"AZ23/$CE$23","v":0},null,{"$f":"$G23*BC23","v":0},{"$f":"BC23/$CE$23","v":0},null,{"$f":"$G23*BF23","v":0},{"$f":"BF23/$CE$23","v":0},null,{"$f":"$G23*BI23","v":0},{"$f":"BI23/$CE$23","v":0},null,{"$f":"$G23*BL23","v":0},{"$f":"BL23/$CE$23","v":0},null,{"$f":"$G23*BO23","v":0},{"$f":"BO23/$CE$23","v":0},null,{"$f":"$G23*BR23","v":0},{"$f":"BR23/$CE$23","v":0},null,{"$f":"$G23*BU23","v":0},{"$f":"BU23/$CE$23","v":0},null,{"$f":"$G23*BX23","v":0},{"$f":"BX23/$CE$23","v":0},null,{"$f":"$G23*CA23","v":0},{"$f":"CA23/$CE$23","v":0},null,7.4]
["1.5","O",5,"Armaturna betonska mreža \ndim. (dxš) 6000 x 2150 = 12,9 m2/kom","Reinforcement mesh\ndim. (lxw) 6000 x 2150 = 12,9 m2/pcs","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["1.5.1",null,"A","Q84    /4x4/150x150/ ","Q84    /4x4/150x150/ ","kg",{"$f":"CENA!G16","v":0},{"$f":"J25+M25+P25+S25+V25+Y25+AB25+AE25+AH25+AK25+AN25+AQ25+AT25+AW25+AZ25+BC25+BF25+BI25+BL25+BO25+BR25+BU25+BX25+CA25","v":1408},{"$f":"G25*H25","v":0},0,{"$f":"$G25*J25","v":0},{"$f":"J25/$CE$25","v":0},176,{"$f":"$G25*M25","v":0},{"$f":"M25/$CE$25","v":10},0,{"$f":"$G25*P25","v":0},{"$f":"P25/$CE$25","v":0},176,{"$f":"$G25*S25","v":0},{"$f":"S25/$CE$25","v":10},0,{"$f":"$G25*V25","v":0},{"$f":"V25/$CE$25","v":0},176,{"$f":"$G25*Y25","v":0},{"$f":"Y25/$CE$25","v":10},0,{"$f":"$G25*AB25","v":0},{"$f":"AB25/$CE$25","v":0},0,{"$f":"$G25*AE25","v":0},{"$f":"AE25/$CE$25","v":0},176,{"$f":"$G25*AH25","v":0},{"$f":"AH25/$CE$25","v":10},0,{"$f":"$G25*AK25","v":0},{"$f":"AK25/$CE$25","v":0},0,{"$f":"$G25*AN25","v":0},{"$f":"AN25/$CE$25","v":0},176,{"$f":"$G25*AQ25","v":0},{"$f":"AQ25/$CE$25","v":10},0,{"$f":"$G25*AT25","v":0},{"$f":"AT25/$CE$25","v":0},0,{"$f":"$G25*AW25","v":0},{"$f":"AW25/$CE$25","v":0},0,{"$f":"$G25*AZ25","v":0},{"$f":"AZ25/$CE$25","v":0},0,{"$f":"$G25*BC25","v":0},{"$f":"BC25/$CE$25","v":0},176,{"$f":"$G25*BF25","v":0},{"$f":"BF25/$CE$25","v":10},176,{"$f":"$G25*BI25","v":0},{"$f":"BI25/$CE$25","v":10},0,{"$f":"$G25*BL25","v":0},{"$f":"BL25/$CE$25","v":0},0,{"$f":"$G25*BO25","v":0},{"$f":"BO25/$CE$25","v":0},0,{"$f":"$G25*BR25","v":0},{"$f":"BR25/$CE$25","v":0},0,{"$f":"$G25*BU25","v":0},{"$f":"BU25/$CE$25","v":0},176,{"$f":"$G25*BX25","v":0},{"$f":"BX25/$CE$25","v":10},0,{"$f":"$G25*CA25","v":0},{"$f":"CA25/$CE$25","v":0},null,17.600000000000001]
["1.5.2",null,"B","Q131  /5x5/150x150/ ","Q131  /5x5/150x150/ ","kg",{"$f":"CENA!G17","v":0},{"$f":"J26+M26+P26+S26+V26+Y26+AB26+AE26+AH26+AK26+AN26+AQ26+AT26+AW26+AZ26+BC26+BF26+BI26+BL26+BO26+BR26+BU26+BX26+CA26","v":2299.92},{"$f":"G26*H26","v":0},383.32,{"$f":"$G26*J26","v":0},{"$f":"J26/$CE$26","v":14},0,0,{"$f":"M26/$CE$26","v":0},438.08,{"$f":"$G26*P26","v":0},{"$f":"P26/$CE$26","v":16},0,{"$f":"$G26*S26","v":0},{"$f":"S26/$CE$26","v":0},null,{"$f":"$G26*V26","v":0},{"$f":"V26/$CE$26","v":0},0,{"$f":"$G26*Y26","v":0},{"$f":"Y26/$CE$26","v":0},136.9,{"$f":"$G26*AB26","v":0},{"$f":"AB26/$CE$26","v":5},383.32,{"$f":"$G26*AE26","v":0},{"$f":"AE26/$CE$26","v":14},0,{"$f":"$G26*AH26","v":0},{"$f":"AH26/$CE$26","v":0},0,{"$f":"$G26*AK26","v":0},{"$f":"AK26/$CE$26","v":0},0,{"$f":"$G26*AN26","v":0},{"$f":"AN26/$CE$26","v":0},0,{"$f":"$G26*AQ26","v":0},{"$f":"AQ26/$CE$26","v":0},0,{"$f":"$G26*AT26","v":0},{"$f":"AT26/$CE$26","v":0},164.28,{"$f":"$G26*AW26","v":0},{"$f":"AW26/$CE$26","v":6},0,{"$f":"$G26*AZ26","v":0},{"$f":"AZ26/$CE$26","v":0},0,{"$f":"$G26*BC26","v":0},{"$f":"BC26/$CE$26","v":0},0,{"$f":"$G26*BF26","v":0},{"$f":"BF26/$CE$26","v":0},0,{"$f":"$G26*BI26","v":0},{"$f":"BI26/$CE$26","v":0},191.66,{"$f":"$G26*BL26","v":0},{"$f":"BL26/$CE$26","v":7},109.52,{"$f":"$G26*BO26","v":0},{"$f":"BO26/$CE$26","v":4},273.8,{"$f":"$G26*BR26","v":0},{"$f":"BR26/$CE$26","v":10},219.04,{"$f":"$G26*BU26","v":0},{"$f":"BU26/$CE$26","v":8},null,{"$f":"$G26*BX26","v":0},{"$f":"BX26/$CE$26","v":0},0,{"$f":"$G26*CA26","v":0},{"$f":"CA26/$CE$26","v":0},null,27.38]
["1.5.3",null,"C","Q188  /6x6/150x150/ ","Q188  /6x6/150x150/ ","kg",{"$f":"CENA!G18","v":0},{"$f":"J27+M27+P27+S27+V27+Y27+AB27+AE27+AH27+AK27+AN27+AQ27+AT27+AW27+AZ27+BC27+BF27+BI27+BL27+BO27+BR27+BU27+BX27+CA27","v":315.68},{"$f":"G27*H27","v":0},0,{"$f":"$G27*J27","v":0},{"$f":"J27/$CE$27","v":0},0,0,{"$f":"M27/$CE$27","v":0},0,{"$f":"$G27*P27","v":0},{"$f":"P27/$CE$27","v":0},0,{"$f":"$G27*S27","v":0},{"$f":"S27/$CE$27","v":0},315.68,{"$f":"$G27*V27","v":0},{"$f":"V27/$CE$27","v":8},0,{"$f":"$G27*Y27","v":0},{"$f":"Y27/$CE$27","v":0},0,{"$f":"$G27*AB27","v":0},{"$f":"AB27/$CE$27","v":0},0,{"$f":"$G27*AE27","v":0},{"$f":"AE27/$CE$27","v":0},0,{"$f":"$G27*AH27","v":0},{"$f":"AH27/$CE$27","v":0},0,{"$f":"$G27*AK27","v":0},{"$f":"AK27/$CE$27","v":0},0,{"$f":"$G27*AN27","v":0},{"$f":"AN27/$CE$27","v":0},0,{"$f":"$G27*AQ27","v":0},{"$f":"AQ27/$CE$27","v":0},0,{"$f":"$G27*AT27","v":0},{"$f":"AT27/$CE$27","v":0},0,{"$f":"$G27*AW27","v":0},{"$f":"AW27/$CE$27","v":0},0,{"$f":"$G27*AZ27","v":0},{"$f":"AZ27/$CE$27","v":0},0,{"$f":"$G27*BC27","v":0},{"$f":"BC27/$CE$27","v":0},0,{"$f":"$G27*BF27","v":0},{"$f":"BF27/$CE$27","v":0},0,{"$f":"$G27*BI27","v":0},{"$f":"BI27/$CE$27","v":0},0,{"$f":"$G27*BL27","v":0},{"$f":"BL27/$CE$27","v":0},0,{"$f":"$G27*BO27","v":0},{"$f":"BO27/$CE$27","v":0},0,{"$f":"$G27*BR27","v":0},{"$f":"BR27/$CE$27","v":0},0,{"$f":"$G27*BU27","v":0},{"$f":"BU27/$CE$27","v":0},0,{"$f":"$G27*BX27","v":0},{"$f":"BX27/$CE$27","v":0},0,{"$f":"$G27*CA27","v":0},{"$f":"CA27/$CE$27","v":0},null,39.46]
["1.5.4",null,"D","Q283  /6x6/100x100/","Q283  /6x6/100x100/","kg",{"$f":"CENA!G19","v":0},{"$f":"J28+M28+P28+S28+V28+Y28+AB28+AE28+AH28+AK28+AN28+AQ28+AT28+AW28+AZ28+BC28+BF28+BI28+BL28+BO28+BR28+BU28+BX28+CA28","v":0},{"$f":"G28*H28","v":0},null,{"$f":"$G28*J28","v":0},{"$f":"J28/$CE$28","v":0},null,0,{"$f":"M28/$CE$28","v":0},null,{"$f":"$G28*P28","v":0},{"$f":"P28/$CE$28","v":0},null,{"$f":"$G28*S28","v":0},{"$f":"S28/$CE$28","v":0},null,{"$f":"$G28*V28","v":0},{"$f":"V28/$CE$28","v":0},null,{"$f":"$G28*Y28","v":0},{"$f":"Y28/$CE$28","v":0},null,{"$f":"$G28*AB28","v":0},{"$f":"AB28/$CE$28","v":0},null,{"$f":"$G28*AE28","v":0},{"$f":"AE28/$CE$28","v":0},null,{"$f":"$G28*AH28","v":0},{"$f":"AH28/$CE$28","v":0},null,{"$f":"$G28*AK28","v":0},{"$f":"AK28/$CE$28","v":0},null,{"$f":"$G28*AN28","v":0},{"$f":"AN28/$CE$28","v":0},null,{"$f":"$G28*AQ28","v":0},{"$f":"AQ28/$CE$28","v":0},null,{"$f":"$G28*AT28","v":0},{"$f":"AT28/$CE$28","v":0},null,{"$f":"$G28*AW28","v":0},{"$f":"AW28/$CE$28","v":0},null,{"$f":"$G28*AZ28","v":0},{"$f":"AZ28/$CE$28","v":0},null,{"$f":"$G28*BC28","v":0},{"$f":"BC28/$CE$28","v":0},null,{"$f":"$G28*BF28","v":0},{"$f":"BF28/$CE$28","v":0},null,{"$f":"$G28*BI28","v":0},{"$f":"BI28/$CE$28","v":0},null,{"$f":"$G28*BL28","v":0},{"$f":"BL28/$CE$28","v":0},null,{"$f":"$G28*BO28","v":0},{"$f":"BO28/$CE$28","v":0},null,{"$f":"$G28*BR28","v":0},{"$f":"BR28/$CE$28","v":0},null,{"$f":"$G28*BU28","v":0},{"$f":"BU28/$CE$28","v":0},null,{"$f":"$G28*BX28","v":0},{"$f":"BX28/$CE$28","v":0},null,{"$f":"$G28*CA28","v":0},{"$f":"CA28/$CE$28","v":0},null,58.21]
["1.5.5",null,"E","Q335  /8x8/150x150/","Q335  /8x8/150x150/","kg",{"$f":"CENA!G20","v":0},{"$f":"J29+M29+P29+S29+V29+Y29+AB29+AE29+AH29+AK29+AN29+AQ29+AT29+AW29+AZ29+BC29+BF29+BI29+BL29+BO29+BR29+BU29+BX29+CA29","v":631.98},{"$f":"G29*H29","v":0},null,{"$f":"$G29*J29","v":0},{"$f":"J29/$CE$29","v":0},null,0,{"$f":"M29/$CE$29","v":0},null,{"$f":"$G29*P29","v":0},{"$f":"P29/$CE$29","v":0},null,{"$f":"$G29*S29","v":0},{"$f":"S29/$CE$29","v":0},561.76,{"$f":"$G29*V29","v":0},{"$f":"V29/$CE$29","v":8},null,{"$f":"$G29*Y29","v":0},{"$f":"Y29/$CE$29","v":0},null,{"$f":"$G29*AB29","v":0},{"$f":"AB29/$CE$29","v":0},null,{"$f":"$G29*AE29","v":0},{"$f":"AE29/$CE$29","v":0},null,{"$f":"$G29*AH29","v":0},{"$f":"AH29/$CE$29","v":0},null,{"$f":"$G29*AK29","v":0},{"$f":"AK29/$CE$29","v":0},70.22,{"$f":"$G29*AN29","v":0},{"$f":"AN29/$CE$29","v":1},null,{"$f":"$G29*AQ29","v":0},{"$f":"AQ29/$CE$29","v":0},null,{"$f":"$G29*AT29","v":0},{"$f":"AT29/$CE$29","v":0},null,{"$f":"$G29*AW29","v":0},{"$f":"AW29/$CE$29","v":0},null,{"$f":"$G29*AZ29","v":0},{"$f":"AZ29/$CE$29","v":0},null,{"$f":"$G29*BC29","v":0},{"$f":"BC29/$CE$29","v":0},null,{"$f":"$G29*BF29","v":0},{"$f":"BF29/$CE$29","v":0},null,{"$f":"$G29*BI29","v":0},{"$f":"BI29/$CE$29","v":0},null,{"$f":"$G29*BL29","v":0},{"$f":"BL29/$CE$29","v":0},null,{"$f":"$G29*BO29","v":0},{"$f":"BO29/$CE$29","v":0},null,{"$f":"$G29*BR29","v":0},{"$f":"BR29/$CE$29","v":0},null,{"$f":"$G29*BU29","v":0},{"$f":"BU29/$CE$29","v":0},null,{"$f":"$G29*BX29","v":0},{"$f":"BX29/$CE$29","v":0},null,{"$f":"$G29*CA29","v":0},{"$f":"CA29/$CE$29","v":0},null,70.22]
[]
[2,"Z",null,"MATERIJAL ZA ZIDANJE, MALTERISANJE, GLETOVANJE I FARBANJE","MASONRY, PLASTERING FAIRING AND PAINTING MATERIAL"]
["2.1","Z",1,"Giter blok (d/š/v) 250x190x190 mm","Gitter block (l/w/h) 250x190x190 mm","kom/pcs",{"$f":"CENA!G23","v":0},{"$f":"J32+M32+P32+S32+V32+Y32+AB32+AE32+AH32+AK32+AN32+AQ32+AT32+AW32+AZ32+BC32+BF32+BI32+BL32+BO32+BR32+BU32+BX32+CA32","v":20480},{"$f":"G32*H32","v":0},4000,{"$f":"$G32*J32","v":0},null,1120,{"$f":"$G32*M32","v":0},null,2080,{"$f":"$G32*P32","v":0},null,0,{"$f":"$G32*S32","v":0},null,2880,{"$f":"$G32*V32","v":0},null,1600,{"$f":"$G32*Y32","v":0},null,0,{"$f":"$G32*AB32","v":0},null,5120,{"$f":"$G32*AE32","v":0},null,0,{"$f":"$G32*AH32","v":0},null,0,{"$f":"$G32*AK32","v":0},null,0,{"$f":"$G32*AN32","v":0},null,0,{"$f":"$G32*AQ32","v":0},null,1600,{"$f":"$G32*AT32","v":0},null,0,{"$f":"$G32*AW32","v":0},null,0,{"$f":"$G32*AZ32","v":0},null,0,{"$f":"$G32*BC32","v":0},null,0,{"$f":"$G32*BF32","v":0},null,800,{"$f":"$G32*BI32","v":0},null,0,{"$f":"$G32*BL32","v":0},null,0,{"$f":"$G32*BO32","v":0},null,0,{"$f":"$G32*BR32","v":0},null,1280,{"$f":"$G32*BU32","v":0},null,0,{"$f":"$G32*BX32","v":0},null,0,{"$f":"$G32*CA32","v":0}]
["2.2","Z",2,"Giter polublok (12cm) (d/š/v) 250x120x190mm","Gitter half block (12cm) (l/w/h) 250x120x190mm","kom/pcs",{"$f":"CENA!G24","v":0},{"$f":"J33+M33+P33+S33+V33+Y33+AB33+AE33+AH33+AK33+AN33+AQ33+AT33+AW33+AZ33+BC33+BF33+BI33+BL33+BO33+BR33+BU33+BX33+CA33","v":3990},{"$f":"G33*H33","v":0},1470,{"$f":"$G33*J33","v":0},null,0,0,null,0,{"$f":"$G33*P33","v":0},null,0,{"$f":"$G33*S33","v":0},null,0,{"$f":"$G33*V33","v":0},null,0,{"$f":"$G33*Y33","v":0},null,0,{"$f":"$G33*AB33","v":0},null,1050,{"$f":"$G33*AE33","v":0},null,0,{"$f":"$G33*AH33","v":0},null,0,{"$f":"$G33*AK33","v":0},null,0,{"$f":"$G33*AN33","v":0},null,0,{"$f":"$G33*AQ33","v":0},null,0,{"$f":"$G33*AT33","v":0},null,0,{"$f":"$G33*AW33","v":0},null,0,{"$f":"$G33*AZ33","v":0},null,1470,{"$f":"$G33*BC33","v":0},null,0,{"$f":"$G33*BF33","v":0},null,0,{"$f":"$G33*BI33","v":0},null,0,{"$f":"$G33*BL33","v":0},null,0,{"$f":"$G33*BO33","v":0},null,0,{"$f":"$G33*BR33","v":0},null,0,{"$f":"$G33*BU33","v":0},null,0,{"$f":"$G33*BX33","v":0},null,0,{"$f":"$G33*CA33","v":0}]
["2.3","Z",3,"Opeka puna (d/š/v) 250x120x65 mm","Brick (full-without holes) (l/w/h) 250x120x65 mm","kom/pcs",{"$f":"CENA!G25","v":0},{"$f":"J34+M34+P34+S34+V34+Y34+AB34+AE34+AH34+AK34+AN34+AQ34+AT34+AW34+AZ34+BC34+BF34+BI34+BL34+BO34+BR34+BU34+BX34+CA34","v":30720},{"$f":"G34*H34","v":0},0,{"$f":"$G34*J34","v":0},null,0,0,null,0,{"$f":"$G34*P34","v":0},null,2048,{"$f":"$G34*S34","v":0},null,3072,{"$f":"$G34*V34","v":0},null,0,{"$f":"$G34*Y34","v":0},null,3072,{"$f":"$G34*AB34","v":0},null,0,{"$f":"$G34*AE34","v":0},null,0,{"$f":"$G34*AH34","v":0},null,0,{"$f":"$G34*AK34","v":0},null,2048,{"$f":"$G34*AN34","v":0},null,3072,{"$f":"$G34*AQ34","v":0},null,0,{"$f":"$G34*AT34","v":0},null,0,{"$f":"$G34*AW34","v":0},null,0,{"$f":"$G34*AZ34","v":0},null,0,{"$f":"$G34*BC34","v":0},null,6144,{"$f":"$G34*BF34","v":0},null,0,{"$f":"$G34*BI34","v":0},null,5120,{"$f":"$G34*BL34","v":0},null,6144,{"$f":"$G34*BO34","v":0},null,0,{"$f":"$G34*BR34","v":0},null,0,{"$f":"$G34*BU34","v":0},null,0,{"$f":"$G34*BX34","v":0},null,0,{"$f":"$G34*CA34","v":0}]
["2.4","Z",4,"Blok od porobetona za pregradni zid\n(d/š/v) 625x200x200 mm","Aerated concrete block for partition wall\n(l/w/h) 625x200x200 mm","kom/pcs",{"$f":"CENA!G26","v":0},{"$f":"J35+M35+P35+S35+V35+Y35+AB35+AE35+AH35+AK35+AN35+AQ35+AT35+AW35+AZ35+BC35+BF35+BI35+BL35+BO35+BR35+BU35+BX35+CA35","v":0},{"$f":"G35*H35","v":0},0,{"$f":"$G35*J35","v":0},null,0,0,null,0,{"$f":"$G35*P35","v":0},null,0,{"$f":"$G35*S35","v":0},null,0,{"$f":"$G35*V35","v":0},null,0,{"$f":"$G35*Y35","v":0},null,0,{"$f":"$G35*AB35","v":0},null,0,{"$f":"$G35*AE35","v":0},null,0,{"$f":"$G35*AH35","v":0},null,0,{"$f":"$G35*AK35","v":0},null,0,{"$f":"$G35*AN35","v":0},null,0,{"$f":"$G35*AQ35","v":0},null,0,{"$f":"$G35*AT35","v":0},null,0,{"$f":"$G35*AW35","v":0},null,0,{"$f":"$G35*AZ35","v":0},null,0,{"$f":"$G35*BC35","v":0},null,0,{"$f":"$G35*BF35","v":0},null,0,{"$f":"$G35*BI35","v":0},null,0,{"$f":"$G35*BL35","v":0},null,0,{"$f":"$G35*BO35","v":0},null,0,{"$f":"$G35*BR35","v":0},null,0,{"$f":"$G35*BU35","v":0},null,0,{"$f":"$G35*BX35","v":0},null,0,{"$f":"$G35*CA35","v":0}]
["2.5","Z",5,"Fert nosači (gredice)\nDužina nosača je jednaka dužini binora = \nširina otvora između zidova + 30 cm.\nBroj gredica = dužina prostorije x 0,40","Fert beams\nBoom length is equal to the length of Binor =\nwidth of the openings between the walls + 30 cm.\nNumber of beams = length of room x 0.40","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["2.5.1",null,"A","0,00-3,90 m ","0,00-3,90 m ","m1",{"$f":"CENA!G28","v":0},{"$f":"J37+M37+P37+S37+V37+Y37+AB37+AE37+AH37+AK37+AN37+AQ37+AT37+AW37+AZ37+BC37+BF37+BI37+BL37+BO37+BR37+BU37+BX37+CA37","v":737.09999999999991},{"$f":"G37*H37","v":0},70.2,{"$f":"$G37*J37","v":0},{"$f":"J37/3.9","v":18},0,{"$f":"$G37*M37","v":0},{"$f":"M37/3.9","v":0},128.69999999999999,{"$f":"$G37*P37","v":0},null,0,{"$f":"$G37*S37","v":0},null,0,{"$f":"$G37*V37","v":0},null,0,{"$f":"$G37*Y37","v":0},null,0,{"$f":"$G37*AB37","v":0},null,234,{"$f":"$G37*AE37","v":0},{"$f":"AE37/3.9","v":60},0,{"$f":"$G37*AH37","v":0},null,0,{"$f":"$G37*AK37","v":0},null,0,{"$f":"$G37*AN37","v":0},{"$f":"AN37/3.9","v":0},0,{"$f":"$G37*AQ37","v":0},{"$f":"AQ37/3.9","v":0},0,{"$f":"$G37*AT37","v":0},null,0,{"$f":"$G37*AW37","v":0},null,0,{"$f":"$G37*AZ37","v":0},null,0,{"$f":"$G37*BC37","v":0},null,0,{"$f":"$G37*BF37","v":0},null,0,{"$f":"$G37*BI37","v":0},null,null,{"$f":"$G37*BL37","v":0},null,0,{"$f":"$G37*BO37","v":0},null,136.5,{"$f":"$G37*BR37","v":0},null,167.7,{"$f":"$G37*BU37","v":0},null,0,{"$f":"$G37*BX37","v":0},null,0,{"$f":"$G37*CA37","v":0}]
["2.5.2",null,"B","3,91-4,50 m ","3,91-4,50 m ","m1",{"$f":"CENA!G29","v":0},445.5,0,126,{"$f":"$G38*J38","v":0},{"$f":"J38/4.5","v":28},0,0,{"$f":"M38/4.5","v":0},148.5,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,{"$f":"AE38/4.5","v":0},0,0,null,0,0,null,0,0,{"$f":"AN38/4.5","v":0},0,0,{"$f":"AQ38/4.5","v":0},0,0,null,90,0,null,0,0,null,0,0,null,0,0,null,0,0,null,null,0,null,81,0,null,0,0,null,0,0,null,0,0,null,0,0]
["2.5.3",null,"C","4,51-4,90 m ","4,51-4,90 m ","m1",{"$f":"CENA!G30","v":0},406.7,0,0,{"$f":"$G39*J39","v":0},{"$f":"J39/4.9","v":0},0,0,{"$f":"M39/4.9","v":0},0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,112.7,0,{"$f":"AE39/4.9","v":23},0,0,null,0,0,null,0,0,{"$f":"AN39/4.9","v":0},0,0,{"$f":"AQ39/4.9","v":0},0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,147,0,null,147,0,null,0,0,null,0,0]
["2.5.4",null,"D","4,91-5,30 m ","4,91-5,30 m ","m1",{"$f":"CENA!G31","v":0},0,0,0,{"$f":"$G40*J40","v":0},{"$f":"J40/5.3","v":0},0,0,{"$f":"M40/5.3","v":0},0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,{"$f":"AE40/5.3","v":0},0,0,null,0,0,null,0,0,{"$f":"AN40/5.3","v":0},0,0,{"$f":"AQ40/5.3","v":0},0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0]
["2.5.5",null,"E","5,31-5,90 m ","5,31-5,90 m ","m1",{"$f":"CENA!G32","v":0},165.20000000000002,0,0,{"$f":"$G41*J41","v":0},{"$f":"J41/5.9","v":0},0,0,{"$f":"M41/5.9","v":0},0,0,null,0,0,null,165.20000000000002,0,null,0,0,null,0,0,null,0,0,{"$f":"AE41/5.9","v":0},0,0,null,0,0,null,0,0,{"$f":"AN41/5.9","v":0},0,0,{"$f":"AQ41/5.9","v":0},0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0]
["2.5.6",null,"F","5,91-6,30 m ","5,91-6,30 m ","m1",{"$f":"CENA!G33","v":0},176.4,0,0,{"$f":"$G42*J42","v":0},{"$f":"J42/6.3","v":0},0,0,{"$f":"M42/6.3","v":0},0,0,null,0,0,null,176.4,0,null,0,0,null,0,0,null,0,0,{"$f":"AE42/6.3","v":0},0,0,null,0,0,null,0,0,{"$f":"AN42/6.3","v":0},0,0,{"$f":"AQ42/6.3","v":0},0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0]
["2.6","Z",6,"Fert ispuna (d/š/v) 245x285/275x160 mm ","Fert fillings (l/w/h) 245x285/275x160 mm ","kom/pcs",{"$f":"CENA!G34","v":0},5670,0,0,{"$f":"$G43*J43","v":0},null,0,0,null,1008,0,null,0,0,null,1260,0,null,0,0,null,0,0,null,882,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,252,0,null,0,0,null,0,0,null,0,0,null,0,0,null,null,0,null,252,0,null,1008,0,null,1008,0,null,0,0,null,0,0]
["2.7","Z",7,"Malter za zidanje \nPripremljeno krečno - cementno vezivo","Mortar for masonry\nPrepared lime - cement binder","kg",{"$f":"CENA!G35","v":0},0,0,null,{"$f":"$G44*J44","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["2.8","Z",8,"Malter za malterisanje \nPripremljeno krečno - cementno vezivo","Mortar for plastering\nPrepared lime - cement binder","kg",{"$f":"CENA!G36","v":0},2600,0,null,{"$f":"$G45*J45","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,2600,0,null,null,0]
["2.9","Z",9,"Krečna glet masa\nBezcementna krečna masa za gletovanje","Lime smoothing mass\nNo cement lime compound for smoothing","kg",{"$f":"CENA!G37","v":0},7325,0,null,{"$f":"$G46*J46","v":0},null,600,0,null,null,0,null,300,0,null,null,0,null,300,0,null,275,0,null,null,0,null,600,0,null,300,0,null,500,0,null,500,0,null,300,0,null,0,0,null,200,0,null,600,0,null,null,0,null,550,0,null,300,0,null,300,0,null,300,0,null,400,0,null,700,0,null,300,0]
["2.10","Z",10,"Poludisperzivna boja \nPoludisperziona boja  razrediva vodom","Semi dispersion paint","kg",{"$f":"CENA!G38","v":0},1100,0,100,{"$f":"$G47*J47","v":0},null,50,0,null,null,0,null,50,0,null,null,0,null,50,0,null,25,0,null,100,0,null,50,0,null,50,0,null,25,0,null,50,0,null,50,0,null,0,0,null,50,0,null,50,0,null,50,0,null,50,0,null,50,0,null,50,0,null,50,0,null,50,0,null,50,0,null,50,0]
[]
["3","K",null,"MATERIJAL ZA KROVNU KONSTRUKCIJU, KROVNI POKRIVAČ, OSB I GIPS KARONSKE TABLE","ROOF CONSTRUCTION AND ROOFING MATERIAL, OSB AND PLASTERBOARD TABLE"]
["3.1","K",1,"Presovani glineni crep I klase\ndimenzija: 400-450x245-275 mm","Pressed clay tiles class 1\ndim: 400-450x245-275 mm","kom/pcs",{"$f":"CENA!G41","v":0},{"$f":"J50+M50+P50+S50+V50+Y50+AB50+AE50+AH50+AK50+AN50+AQ50+AT50+AW50+AZ50+BC50+BF50+BI50+BL50+BO50+BR50+BU50+BX50+CA50","v":59840},{"$f":"G50*H50","v":0},1920,{"$f":"$G50*J50","v":0},null,2240,{"$f":"$G50*M50","v":0},null,2560,{"$f":"$G50*P50","v":0},null,2240,{"$f":"$G50*S50","v":0},null,2560,{"$f":"$G50*V50","v":0},null,2560,{"$f":"$G50*Y50","v":0},null,1920,{"$f":"$G50*AB50","v":0},null,2560,{"$f":"$G50*AE50","v":0},null,null,{"$f":"$G50*AH50","v":0},null,2560,{"$f":"$G50*AK50","v":0},null,1920,{"$f":"$G50*AN50","v":0},null,2240,{"$f":"$G50*AQ50","v":0},null,2560,{"$f":"$G50*AT50","v":0},null,3520,{"$f":"$G50*AW50","v":0},null,2880,{"$f":"$G50*AZ50","v":0},null,2240,{"$f":"$G50*BC50","v":0},null,3520,{"$f":"$G50*BF50","v":0},null,2880,{"$f":"$G50*BI50","v":0},null,2240,{"$f":"$G50*BL50","v":0},null,2240,{"$f":"$G50*BO50","v":0},null,3520,{"$f":"$G50*BR50","v":0},null,2560,{"$f":"$G50*BU50","v":0},null,3200,{"$f":"$G50*BX50","v":0},null,3200,{"$f":"$G50*CA50","v":0}]
["3.2","K",3,"Biber crep I klase dimenzija: 180x380 mm","Biber clay tiles class 1 dim: 180x380 mm","kom/pcs",{"$f":"CENA!G42","v":0},{"$f":"J51+M51+P51+S51+V51+Y51+AB51+AE51+AH51+AK51+AN51+AQ51+AT51+AW51+AZ51+BC51+BF51+BI51+BL51+BO51+BR51+BU51+BX51+CA51","v":0},{"$f":"G51*H51","v":0},null,{"$f":"$G51*J51","v":0},null,null,0,null,null,{"$f":"$G51*P51","v":0},null,null,{"$f":"$G51*S51","v":0},null,null,{"$f":"$G51*V51","v":0},null,null,{"$f":"$G51*Y51","v":0},null,null,{"$f":"$G51*AB51","v":0},null,null,{"$f":"$G51*AE51","v":0},null,null,{"$f":"$G51*AH51","v":0},null,null,{"$f":"$G51*AK51","v":0},null,null,{"$f":"$G51*AN51","v":0},null,null,{"$f":"$G51*AQ51","v":0},null,null,{"$f":"$G51*AT51","v":0},null,null,{"$f":"$G51*AW51","v":0},null,null,{"$f":"$G51*AZ51","v":0},null,null,{"$f":"$G51*BC51","v":0},null,null,{"$f":"$G51*BF51","v":0},null,null,{"$f":"$G51*BI51","v":0},null,null,{"$f":"$G51*BL51","v":0},null,null,{"$f":"$G51*BO51","v":0},null,null,{"$f":"$G51*BR51","v":0},null,null,{"$f":"$G51*BU51","v":0},null,null,{"$f":"$G51*BX51","v":0},null,null,{"$f":"$G51*CA51","v":0}]
["3.3","K",2,"Slemeni crep I klase (žljebnjak)","Ridge clay tiles class 1","kom/pcs",{"$f":"CENA!G43","v":0},{"$f":"J52+M52+P52+S52+V52+Y52+AB52+AE52+AH52+AK52+AN52+AQ52+AT52+AW52+AZ52+BC52+BF52+BI52+BL52+BO52+BR52+BU52+BX52+CA52","v":870},{"$f":"G52*H52","v":0},39,{"$f":"$G52*J52","v":0},null,39,0,null,42,{"$f":"$G52*P52","v":0},null,42,{"$f":"$G52*S52","v":0},null,36,{"$f":"$G52*V52","v":0},null,48,{"$f":"$G52*Y52","v":0},null,0,{"$f":"$G52*AB52","v":0},null,36,{"$f":"$G52*AE52","v":0},null,0,{"$f":"$G52*AH52","v":0},null,36,{"$f":"$G52*AK52","v":0},null,36,{"$f":"$G52*AN52","v":0},null,42,{"$f":"$G52*AQ52","v":0},null,36,{"$f":"$G52*AT52","v":0},null,60,{"$f":"$G52*AW52","v":0},null,48,{"$f":"$G52*AZ52","v":0},null,0,{"$f":"$G52*BC52","v":0},null,54,{"$f":"$G52*BF52","v":0},null,45,{"$f":"$G52*BI52","v":0},null,27,{"$f":"$G52*BL52","v":0},null,42,{"$f":"$G52*BO52","v":0},null,60,{"$f":"$G52*BR52","v":0},null,42,{"$f":"$G52*BU52","v":0},null,0,{"$f":"$G52*BX52","v":0},null,60,{"$f":"$G52*CA52","v":0}]
["3.4","K",4,"Paropropusna i vodonepropusna krovna  folija kontrola vodene pare iznad termoizolacije","Vapour permeable and waterproof roof sheeting control of water vapor above the insulation","m2",{"$f":"CENA!G44","v":0},{"$f":"J53+M53+P53+S53+V53+Y53+AB53+AE53+AH53+AK53+AN53+AQ53+AT53+AW53+AZ53+BC53+BF53+BI53+BL53+BO53+BR53+BU53+BX53+CA53","v":3825},{"$f":"G53*H53","v":0},150,{"$f":"$G53*J53","v":0},null,150,0,null,150,{"$f":"$G53*P53","v":0},null,null,{"$f":"$G53*S53","v":0},null,150,{"$f":"$G53*V53","v":0},null,150,{"$f":"$G53*Y53","v":0},null,150,{"$f":"$G53*AB53","v":0},null,150,{"$f":"$G53*AE53","v":0},null,150,{"$f":"$G53*AH53","v":0},null,150,{"$f":"$G53*AK53","v":0},null,150,{"$f":"$G53*AN53","v":0},null,150,{"$f":"$G53*AQ53","v":0},null,150,{"$f":"$G53*AT53","v":0},null,225,{"$f":"$G53*AW53","v":0},null,225,{"$f":"$G53*AZ53","v":0},null,150,{"$f":"$G53*BC53","v":0},null,225,{"$f":"$G53*BF53","v":0},null,225,{"$f":"$G53*BI53","v":0},null,150,{"$f":"$G53*BL53","v":0},null,150,{"$f":"$G53*BO53","v":0},null,225,{"$f":"$G53*BR53","v":0},null,225,{"$f":"$G53*BU53","v":0},null,null,{"$f":"$G53*BX53","v":0},null,225,{"$f":"$G53*CA53","v":0}]
["3.5","K",5,"Staklena mineralna vuna \ntermoizolacija potkrovlja između rogova","Glass Mineral Wool \nloft insulation between the rafters","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["3.5.1",null,"A","debljina d=10 cm  ","thickness d=10 cm  ","m2",{"$f":"CENA!G46","v":0},{"$f":"J55+M55+P55+S55+V55+Y55+AB55+AE55+AH55+AK55+AN55+AQ55+AT55+AW55+AZ55+BC55+BF55+BI55+BL55+BO55+BR55+BU55+BX55+CA55","v":2226},{"$f":"G55*H55","v":0},null,{"$f":"$G55*J55","v":0},null,134.4,{"$f":"$G55*M55","v":0},null,null,{"$f":"$G55*P55","v":0},null,null,{"$f":"$G55*S55","v":0},null,null,{"$f":"$G55*V55","v":0},null,126,{"$f":"$G55*Y55","v":0},null,84,{"$f":"$G55*AB55","v":0},null,null,{"$f":"$G55*AE55","v":0},null,134.4,{"$f":"$G55*AH55","v":0},null,151.20000000000002,{"$f":"$G55*AK55","v":0},null,126,{"$f":"$G55*AN55","v":0},null,142.80000000000001,{"$f":"$G55*AQ55","v":0},null,151.20000000000002,{"$f":"$G55*AT55","v":0},null,210,{"$f":"$G55*AW55","v":0},null,null,{"$f":"$G55*AZ55","v":0},null,134.4,{"$f":"$G55*BC55","v":0},null,null,{"$f":"$G55*BF55","v":0},null,184.8,{"$f":"$G55*BI55","v":0},null,142.80000000000001,{"$f":"$G55*BL55","v":0},null,134.4,{"$f":"$G55*BO55","v":0},null,null,{"$f":"$G55*BR55","v":0},null,168,{"$f":"$G55*BU55","v":0},null,null,{"$f":"$G55*BX55","v":0},null,201.60000000000002,{"$f":"$G55*CA55","v":0}]
["3.5.2",null,"B","debljina d=12 cm  ","thickness d=12 cm  ","m2",{"$f":"CENA!G47","v":0},{"$f":"J56+M56+P56+S56+V56+Y56+AB56+AE56+AH56+AK56+AN56+AQ56+AT56+AW56+AZ56+BC56+BF56+BI56+BL56+BO56+BR56+BU56+BX56+CA56","v":0},{"$f":"G56*H56","v":0},null,{"$f":"$G56*J56","v":0},null,null,0,null,null,{"$f":"$G56*P56","v":0},null,null,{"$f":"$G56*S56","v":0},null,null,{"$f":"$G56*V56","v":0},null,null,{"$f":"$G56*Y56","v":0},null,null,{"$f":"$G56*AB56","v":0},null,null,{"$f":"$G56*AE56","v":0},null,null,{"$f":"$G56*AH56","v":0},null,null,{"$f":"$G56*AK56","v":0},null,null,{"$f":"$G56*AN56","v":0},null,null,{"$f":"$G56*AQ56","v":0},null,null,{"$f":"$G56*AT56","v":0},null,null,{"$f":"$G56*AW56","v":0},null,null,{"$f":"$G56*AZ56","v":0},null,null,{"$f":"$G56*BC56","v":0},null,null,{"$f":"$G56*BF56","v":0},null,null,{"$f":"$G56*BI56","v":0},null,null,{"$f":"$G56*BL56","v":0},null,null,{"$f":"$G56*BO56","v":0},null,null,{"$f":"$G56*BR56","v":0},null,null,{"$f":"$G56*BU56","v":0},null,null,{"$f":"$G56*BX56","v":0},null,null,{"$f":"$G56*CA56","v":0}]
["3.5.3",null,"C","debljina d=14 cm  ","thickness d=14 cm  ","m2",{"$f":"CENA!G48","v":0},{"$f":"J57+M57+P57+S57+V57+Y57+AB57+AE57+AH57+AK57+AN57+AQ57+AT57+AW57+AZ57+BC57+BF57+BI57+BL57+BO57+BR57+BU57+BX57+CA57","v":0},{"$f":"G57*H57","v":0},null,{"$f":"$G57*J57","v":0},null,null,0,null,null,{"$f":"$G57*P57","v":0},null,null,{"$f":"$G57*S57","v":0},null,null,{"$f":"$G57*V57","v":0},null,null,{"$f":"$G57*Y57","v":0},null,null,{"$f":"$G57*AB57","v":0},null,null,{"$f":"$G57*AE57","v":0},null,null,{"$f":"$G57*AH57","v":0},null,null,{"$f":"$G57*AK57","v":0},null,null,{"$f":"$G57*AN57","v":0},null,null,{"$f":"$G57*AQ57","v":0},null,null,{"$f":"$G57*AT57","v":0},null,null,{"$f":"$G57*AW57","v":0},null,null,{"$f":"$G57*AZ57","v":0},null,null,{"$f":"$G57*BC57","v":0},null,null,{"$f":"$G57*BF57","v":0},null,null,{"$f":"$G57*BI57","v":0},null,null,{"$f":"$G57*BL57","v":0},null,null,{"$f":"$G57*BO57","v":0},null,null,{"$f":"$G57*BR57","v":0},null,null,{"$f":"$G57*BU57","v":0},null,null,{"$f":"$G57*BX57","v":0},null,null,{"$f":"$G57*CA57","v":0}]
["3.6","K",6,"Parna brana\nkontrola vodene pare ispod termoizolacije","Vapor barrier \ncontrol of water vapor below the insulation","m2",{"$f":"CENA!G49","v":0},{"$f":"J58+M58+P58+S58+V58+Y58+AB58+AE58+AH58+AK58+AN58+AQ58+AT58+AW58+AZ58+BC58+BF58+BI58+BL58+BO58+BR58+BU58+BX58+CA58","v":2550},{"$f":"G58*H58","v":0},null,{"$f":"$G58*J58","v":0},null,150,0,null,null,{"$f":"$G58*P58","v":0},null,null,{"$f":"$G58*S58","v":0},null,null,{"$f":"$G58*V58","v":0},null,150,{"$f":"$G58*Y58","v":0},null,150,{"$f":"$G58*AB58","v":0},null,null,{"$f":"$G58*AE58","v":0},null,150,{"$f":"$G58*AH58","v":0},null,150,{"$f":"$G58*AK58","v":0},null,150,{"$f":"$G58*AN58","v":0},null,150,{"$f":"$G58*AQ58","v":0},null,150,{"$f":"$G58*AT58","v":0},null,225,{"$f":"$G58*AW58","v":0},null,null,{"$f":"$G58*AZ58","v":0},null,150,{"$f":"$G58*BC58","v":0},null,null,{"$f":"$G58*BF58","v":0},null,225,{"$f":"$G58*BI58","v":0},null,150,{"$f":"$G58*BL58","v":0},null,150,{"$f":"$G58*BO58","v":0},null,null,{"$f":"$G58*BR58","v":0},null,225,{"$f":"$G58*BU58","v":0},null,null,{"$f":"$G58*BX58","v":0},null,225,{"$f":"$G58*CA58","v":0}]
["3.7","K",7,"Čamova rezana građa različitog preseka\ndužine 400 cm","Fir lumber of different cross-section\nlength 400 cm","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["3.7.1",null,"A","Rog/Venčanica/Raspinjača           10/12 cm","rafters / wall plate / ridge collar 10/12 cm","m3",{"$f":"CENA!G51","v":0},{"$f":"J60+M60+P60+S60+V60+Y60+AB60+AE60+AH60+AK60+AN60+AQ60+AT60+AW60+AZ60+BC60+BF60+BI60+BL60+BO60+BR60+BU60+BX60+CA60","v":0},{"$f":"G60*H60","v":0},null,{"$f":"$G60*J60","v":0},{"$f":"J60/$CE$60","v":0},null,{"$f":"$G60*M60","v":0},{"$f":"M60/$CE$60","v":0},null,{"$f":"$G60*P60","v":0},{"$f":"P60/$CE$60","v":0},null,{"$f":"$G60*S60","v":0},{"$f":"S60/$CE$60","v":0},null,{"$f":"$G60*V60","v":0},{"$f":"V60/$CE$60","v":0},null,{"$f":"$G60*Y60","v":0},{"$f":"Y60/$CE$60","v":0},null,{"$f":"$G60*AB60","v":0},{"$f":"AB60/$CE$60","v":0},null,{"$f":"$G60*AE60","v":0},{"$f":"AE60/$CE$60","v":0},null,{"$f":"$G60*AH60","v":0},{"$f":"AH60/$CE$60","v":0},null,{"$f":"$G60*AK60","v":0},{"$f":"AK60/$CE$60","v":0},null,{"$f":"$G60*AN60","v":0},{"$f":"AN60/$CE$60","v":0},null,{"$f":"$G60*AQ60","v":0},{"$f":"AQ60/$CE$60","v":0},null,{"$f":"$G60*AT60","v":0},{"$f":"AT60/$CE$60","v":0},null,{"$f":"$G60*AW60","v":0},{"$f":"AW60/$CE$60","v":0},null,{"$f":"$G60*AZ60","v":0},{"$f":"AZ60/$CE$60","v":0},null,{"$f":"$G60*BC60","v":0},{"$f":"BC60/$CE$60","v":0},null,{"$f":"$G60*BF60","v":0},{"$f":"BF60/$CE$60","v":0},null,{"$f":"$G60*BI60","v":0},{"$f":"BI60/$CE$60","v":0},null,{"$f":"$G60*BL60","v":0},{"$f":"BL60/$CE$60","v":0},null,{"$f":"$G60*BO60","v":0},{"$f":"BO60/$CE$60","v":0},null,{"$f":"$G60*BR60","v":0},{"$f":"BR60/$CE$60","v":0},null,{"$f":"$G60*BU60","v":0},{"$f":"BU60/$CE$60","v":0},null,{"$f":"$G60*BX60","v":0},{"$f":"BX60/$CE$60","v":0},null,{"$f":"$G60*CA60","v":0},{"$f":"CA60/$CE$60","v":0},null,4.8000000000000001E-2]
["3.7.2",null,"B","Rog/Stub/Grebenjača/Slemenja.   12/14 cm","column / pile / hip rafter / ridge 12/14 cm","m3",{"$f":"CENA!G52","v":0},{"$f":"J61+M61+P61+S61+V61+Y61+AB61+AE61+AH61+AK61+AN61+AQ61+AT61+AW61+AZ61+BC61+BF61+BI61+BL61+BO61+BR61+BU61+BX61+CA61","v":0},{"$f":"G61*H61","v":0},null,{"$f":"$G61*J61","v":0},{"$f":"J61/$CE$61","v":0},null,0,{"$f":"M61/$CE$61","v":0},null,{"$f":"$G61*P61","v":0},{"$f":"P61/$CE$61","v":0},null,{"$f":"$G61*S61","v":0},{"$f":"S61/$CE$61","v":0},null,{"$f":"$G61*V61","v":0},{"$f":"V61/$CE$61","v":0},null,{"$f":"$G61*Y61","v":0},{"$f":"Y61/$CE$61","v":0},null,{"$f":"$G61*AB61","v":0},{"$f":"AB61/$CE$61","v":0},null,{"$f":"$G61*AE61","v":0},{"$f":"AE61/$CE$61","v":0},null,{"$f":"$G61*AH61","v":0},{"$f":"AH61/$CE$61","v":0},null,{"$f":"$G61*AK61","v":0},{"$f":"AK61/$CE$61","v":0},null,{"$f":"$G61*AN61","v":0},{"$f":"AN61/$CE$61","v":0},null,{"$f":"$G61*AQ61","v":0},{"$f":"AQ61/$CE$61","v":0},null,{"$f":"$G61*AT61","v":0},{"$f":"AT61/$CE$61","v":0},null,{"$f":"$G61*AW61","v":0},{"$f":"AW61/$CE$61","v":0},null,{"$f":"$G61*AZ61","v":0},{"$f":"AZ61/$CE$61","v":0},null,{"$f":"$G61*BC61","v":0},{"$f":"BC61/$CE$61","v":0},null,{"$f":"$G61*BF61","v":0},{"$f":"BF61/$CE$61","v":0},null,{"$f":"$G61*BI61","v":0},{"$f":"BI61/$CE$61","v":0},null,{"$f":"$G61*BL61","v":0},{"$f":"BL61/$CE$61","v":0},null,{"$f":"$G61*BO61","v":0},{"$f":"BO61/$CE$61","v":0},null,{"$f":"$G61*BR61","v":0},{"$f":"BR61/$CE$61","v":0},null,{"$f":"$G61*BU61","v":0},{"$f":"BU61/$CE$61","v":0},null,{"$f":"$G61*BX61","v":0},{"$f":"BX61/$CE$61","v":0},null,{"$f":"$G61*CA61","v":0},{"$f":"CA61/$CE$61","v":0},null,6.7199999999999996E-2]
["3.7.3",null,"C","Stub/Grebenjača                         14/14 cm","column / hip rafter 14/14 cm","m3",{"$f":"CENA!G53","v":0},{"$f":"J62+M62+P62+S62+V62+Y62+AB62+AE62+AH62+AK62+AN62+AQ62+AT62+AW62+AZ62+BC62+BF62+BI62+BL62+BO62+BR62+BU62+BX62+CA62","v":14.975999999999999},{"$f":"G62*H62","v":0},0.78,{"$f":"$G62*J62","v":0},{"$f":"J62/$CE$62","v":9.9489795918367356},0.78,0,{"$f":"M62/$CE$62","v":9.9489795918367356},0.78,{"$f":"$G62*P62","v":0},{"$f":"P62/$CE$62","v":9.9489795918367356},0.78,{"$f":"$G62*S62","v":0},{"$f":"S62/$CE$62","v":9.9489795918367356},0.93599999999999994,{"$f":"$G62*V62","v":0},{"$f":"V62/$CE$62","v":11.938775510204081},0.93599999999999994,{"$f":"$G62*Y62","v":0},{"$f":"Y62/$CE$62","v":11.938775510204081},0,{"$f":"$G62*AB62","v":0},{"$f":"AB62/$CE$62","v":0},null,{"$f":"$G62*AE62","v":0},{"$f":"AE62/$CE$62","v":0},0,{"$f":"$G62*AH62","v":0},{"$f":"AH62/$CE$62","v":0},0.624,{"$f":"$G62*AK62","v":0},{"$f":"AK62/$CE$62","v":7.9591836734693882},null,{"$f":"$G62*AN62","v":0},{"$f":"AN62/$CE$62","v":0},0.78,{"$f":"$G62*AQ62","v":0},{"$f":"AQ62/$CE$62","v":9.9489795918367356},0.624,{"$f":"$G62*AT62","v":0},{"$f":"AT62/$CE$62","v":7.9591836734693882},1.0920000000000001,{"$f":"$G62*AW62","v":0},{"$f":"AW62/$CE$62","v":13.928571428571431},0.93599999999999994,{"$f":"$G62*AZ62","v":0},{"$f":"AZ62/$CE$62","v":11.938775510204081},0,{"$f":"$G62*BC62","v":0},{"$f":"BC62/$CE$62","v":0},0.93599999999999994,{"$f":"$G62*BF62","v":0},{"$f":"BF62/$CE$62","v":11.938775510204081},0.78,{"$f":"$G62*BI62","v":0},{"$f":"BI62/$CE$62","v":9.9489795918367356},0.624,{"$f":"$G62*BL62","v":0},{"$f":"BL62/$CE$62","v":7.9591836734693882},0.78,{"$f":"$G62*BO62","v":0},{"$f":"BO62/$CE$62","v":9.9489795918367356},0.93599999999999994,{"$f":"$G62*BR62","v":0},{"$f":"BR62/$CE$62","v":11.938775510204081},0.78,{"$f":"$G62*BU62","v":0},{"$f":"BU62/$CE$62","v":9.9489795918367356},0,{"$f":"$G62*BX62","v":0},{"$f":"BX62/$CE$62","v":0},1.0920000000000001,{"$f":"$G62*CA62","v":0},{"$f":"CA62/$CE$62","v":13.928571428571431},null,7.8399999999999997E-2]
["3.7.4",null,"H","Tavanjače                                   18/26 cm","attic beams 18/26 cm","m3",{"$f":"CENA!G54","v":0},{"$f":"J63+M63+P63+S63+V63+Y63+AB63+AE63+AH63+AK63+AN63+AQ63+AT63+AW63+AZ63+BC63+BF63+BI63+BL63+BO63+BR63+BU63+BX63+CA63","v":0},{"$f":"G63*H63","v":0},null,{"$f":"$G63*J63","v":0},{"$f":"J63/$CE$63","v":0},null,0,{"$f":"M63/$CE$63","v":0},null,{"$f":"$G63*P63","v":0},{"$f":"P63/$CE$63","v":0},null,{"$f":"$G63*S63","v":0},{"$f":"S63/$CE$63","v":0},null,{"$f":"$G63*V63","v":0},{"$f":"V63/$CE$63","v":0},null,{"$f":"$G63*Y63","v":0},{"$f":"Y63/$CE$63","v":0},null,{"$f":"$G63*AB63","v":0},{"$f":"AB63/$CE$63","v":0},null,{"$f":"$G63*AE63","v":0},{"$f":"AE63/$CE$63","v":0},null,{"$f":"$G63*AH63","v":0},{"$f":"AH63/$CE$63","v":0},null,{"$f":"$G63*AK63","v":0},{"$f":"AK63/$CE$63","v":0},null,{"$f":"$G63*AN63","v":0},{"$f":"AN63/$CE$63","v":0},null,{"$f":"$G63*AQ63","v":0},{"$f":"AQ63/$CE$63","v":0},null,{"$f":"$G63*AT63","v":0},{"$f":"AT63/$CE$63","v":0},null,{"$f":"$G63*AW63","v":0},{"$f":"AW63/$CE$63","v":0},null,{"$f":"$G63*AZ63","v":0},{"$f":"AZ63/$CE$63","v":0},null,{"$f":"$G63*BC63","v":0},{"$f":"BC63/$CE$63","v":0},null,{"$f":"$G63*BF63","v":0},{"$f":"BF63/$CE$63","v":0},null,{"$f":"$G63*BI63","v":0},{"$f":"BI63/$CE$63","v":0},null,{"$f":"$G63*BL63","v":0},{"$f":"BL63/$CE$63","v":0},null,{"$f":"$G63*BO63","v":0},{"$f":"BO63/$CE$63","v":0},null,{"$f":"$G63*BR63","v":0},{"$f":"BR63/$CE$63","v":0},null,{"$f":"$G63*BU63","v":0},{"$f":"BU63/$CE$63","v":0},null,{"$f":"$G63*BX63","v":0},{"$f":"BX63/$CE$63","v":0},null,{"$f":"$G63*CA63","v":0},{"$f":"CA63/$CE$63","v":0},null,0.18720000000000001]
["3.8","K",8,"Čamova rezana građa različitog preseka\ndužine 600 cm","Fir lumber of different cross-section\nlength 600 cm","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,null,"/"]
["3.8.1",null,"A","Rog/Venčanica/Raspinjača          10/12 cm","rafters / wall plate / ridge collar 10/12 cm","m3",{"$f":"CENA!G56","v":0},{"$f":"J65+M65+P65+S65+V65+Y65+AB65+AE65+AH65+AK65+AN65+AQ65+AT65+AW65+AZ65+BC65+BF65+BI65+BL65+BO65+BR65+BU65+BX65+CA65","v":67.24799999999999},{"$f":"G65*H65","v":0},3.1679999999999997,{"$f":"$G65*J65","v":0},{"$f":"J65/$CE$65","v":44},3.1679999999999997,{"$f":"$G65*M65","v":0},{"$f":"M65/$CE$65","v":44},3.4559999999999995,{"$f":"$G65*P65","v":0},{"$f":"P65/$CE$65","v":48},3.4559999999999995,{"$f":"$G65*S65","v":0},{"$f":"S65/$CE$65","v":48},2.3039999999999998,{"$f":"$G65*V65","v":0},{"$f":"V65/$CE$65","v":32},3.8879999999999999,{"$f":"$G65*Y65","v":0},{"$f":"Y65/$CE$65","v":54},0.72,{"$f":"$G65*AB65","v":0},{"$f":"AB65/$CE$65","v":10},2.88,{"$f":"$G65*AE65","v":0},{"$f":"AE65/$CE$65","v":40},0,{"$f":"$G65*AH65","v":0},{"$f":"AH65/$CE$65","v":0},2.88,{"$f":"$G65*AK65","v":0},{"$f":"AK65/$CE$65","v":40},null,{"$f":"$G65*AN65","v":0},{"$f":"AN65/$CE$65","v":0},3.4559999999999995,{"$f":"$G65*AQ65","v":0},{"$f":"AQ65/$CE$65","v":48},2.88,{"$f":"$G65*AT65","v":0},{"$f":"AT65/$CE$65","v":40},4.8959999999999999,{"$f":"$G65*AW65","v":0},{"$f":"AW65/$CE$65","v":68},3.8879999999999999,{"$f":"$G65*AZ65","v":0},{"$f":"AZ65/$CE$65","v":54},0.72,{"$f":"$G65*BC65","v":0},{"$f":"BC65/$CE$65","v":10},4.3199999999999994,{"$f":"$G65*BF65","v":0},{"$f":"BF65/$CE$65","v":59.999999999999993},3.5999999999999996,{"$f":"$G65*BI65","v":0},{"$f":"BI65/$CE$65","v":50},2.448,{"$f":"$G65*BL65","v":0},{"$f":"BL65/$CE$65","v":34},3.4559999999999995,{"$f":"$G65*BO65","v":0},{"$f":"BO65/$CE$65","v":48},3.3119999999999998,{"$f":"$G65*BR65","v":0},{"$f":"BR65/$CE$65","v":46},3.4559999999999995,{"$f":"$G65*BU65","v":0},{"$f":"BU65/$CE$65","v":48},0,{"$f":"$G65*BX65","v":0},{"$f":"BX65/$CE$65","v":0},4.8959999999999999,{"$f":"$G65*CA65","v":0},{"$f":"CA65/$CE$65","v":68},null,7.1999999999999995E-2]
["3.8.2",null,"B","Rog/Stub/Grebenjača/Slemenja.   12/14 cm","column / pile / hip rafter / ridge 12/14 cm","m3",{"$f":"CENA!G57","v":0},0.2016,0,null,{"$f":"$G66*J66","v":0},{"$f":"J66/$CE$66","v":0},null,0,{"$f":"M66/$CE$66","v":0},null,0,{"$f":"P66/$CE$66","v":0},null,0,{"$f":"S66/$CE$66","v":0},null,0,{"$f":"V66/$CE$66","v":0},null,0,{"$f":"Y66/$CE$66","v":0},0.2016,0,{"$f":"AB66/$CE$66","v":2},null,0,{"$f":"AE66/$CE$66","v":0},null,0,{"$f":"AH66/$CE$66","v":0},null,0,{"$f":"AK66/$CE$66","v":0},null,0,{"$f":"AN66/$CE$66","v":0},null,0,{"$f":"AQ66/$CE$66","v":0},null,0,{"$f":"AT66/$CE$66","v":0},null,0,{"$f":"AW66/$CE$66","v":0},null,0,{"$f":"AZ66/$CE$66","v":0},null,0,{"$f":"BC66/$CE$66","v":0},null,0,{"$f":"BF66/$CE$66","v":0},null,0,{"$f":"BI66/$CE$66","v":0},null,0,{"$f":"BL66/$CE$66","v":0},null,0,{"$f":"BO66/$CE$66","v":0},null,0,{"$f":"BR66/$CE$66","v":0},null,0,{"$f":"BU66/$CE$66","v":0},null,0,{"$f":"BX66/$CE$66","v":0},null,0,{"$f":"CA66/$CE$66","v":0},null,0.1008]
["3.8.3",null,"C","Stub/Grebenjača                         14/14 cm","column / hip rafter 14/14 cm","m3",{"$f":"CENA!G58","v":0},12.870000000000001,0,0.70200000000000007,{"$f":"$G67*J67","v":0},{"$f":"J67/$CE$67","v":5.9693877551020416},0.70200000000000007,0,{"$f":"M67/$CE$67","v":5.9693877551020416},0.70200000000000007,0,{"$f":"P67/$CE$67","v":5.9693877551020416},0.70200000000000007,0,{"$f":"S67/$CE$67","v":5.9693877551020416},null,0,{"$f":"V67/$CE$67","v":0},0.70200000000000007,0,{"$f":"Y67/$CE$67","v":5.9693877551020416},0.46800000000000003,0,{"$f":"AB67/$CE$67","v":3.9795918367346941},0.46800000000000003,0,{"$f":"AE67/$CE$67","v":3.9795918367346941},0,0,{"$f":"AH67/$CE$67","v":0},0.46800000000000003,0,{"$f":"AK67/$CE$67","v":3.9795918367346941},null,0,{"$f":"AN67/$CE$67","v":0},0.70200000000000007,0,{"$f":"AQ67/$CE$67","v":5.9693877551020416},0.46800000000000003,0,{"$f":"AT67/$CE$67","v":3.9795918367346941},0.93600000000000005,0,{"$f":"AW67/$CE$67","v":7.9591836734693882},0.70200000000000007,0,{"$f":"AZ67/$CE$67","v":5.9693877551020416},0,0,{"$f":"BC67/$CE$67","v":0},0.70200000000000007,0,{"$f":"BF67/$CE$67","v":5.9693877551020416},0.70200000000000007,0,{"$f":"BI67/$CE$67","v":5.9693877551020416},0.70199999999999996,0,{"$f":"BL67/$CE$67","v":5.9693877551020407},0.70200000000000007,0,{"$f":"BO67/$CE$67","v":5.9693877551020416},0.70200000000000007,0,{"$f":"BR67/$CE$67","v":5.9693877551020416},0.70200000000000007,0,{"$f":"BU67/$CE$67","v":5.9693877551020416},0,0,{"$f":"BX67/$CE$67","v":0},0.93600000000000005,0,{"$f":"CA67/$CE$67","v":7.9591836734693882},null,0.1176]
["3.8.4",null,"D","Rožnjača                                    14/16 cm","Purlin 14/16 cm","m3",{"$f":"CENA!G59","v":0},15.276000000000003,0,0.80400000000000005,{"$f":"$G68*J68","v":0},{"$f":"J68/$CE$68","v":5.9821428571428577},0.80400000000000005,0,{"$f":"M68/$CE$68","v":5.9821428571428577},0.80400000000000005,0,{"$f":"P68/$CE$68","v":5.9821428571428577},0.80400000000000005,0,{"$f":"S68/$CE$68","v":5.9821428571428577},1.0720000000000001,0,{"$f":"V68/$CE$68","v":7.9761904761904772},0.80400000000000005,0,{"$f":"Y68/$CE$68","v":5.9821428571428577},0,0,{"$f":"AB68/$CE$68","v":0},0.53600000000000003,0,{"$f":"AE68/$CE$68","v":3.9880952380952386},0,0,{"$f":"AH68/$CE$68","v":0},0.53600000000000003,0,{"$f":"AK68/$CE$68","v":3.9880952380952386},null,0,{"$f":"AN68/$CE$68","v":0},0.80400000000000005,0,{"$f":"AQ68/$CE$68","v":5.9821428571428577},0.53600000000000003,0,{"$f":"AT68/$CE$68","v":3.9880952380952386},1.0720000000000001,0,{"$f":"AW68/$CE$68","v":7.9761904761904772},0.80400000000000005,0,{"$f":"AZ68/$CE$68","v":5.9821428571428577},0,0,{"$f":"BC68/$CE$68","v":0},0.80400000000000005,0,{"$f":"BF68/$CE$68","v":5.9821428571428577},0.80400000000000005,0,{"$f":"BI68/$CE$68","v":5.9821428571428577},0.80400000000000005,0,{"$f":"BL68/$CE$68","v":5.9821428571428577},0.80400000000000005,0,{"$f":"BO68/$CE$68","v":5.9821428571428577},0.80400000000000005,0,{"$f":"BR68/$CE$68","v":5.9821428571428577},0.80400000000000005,0,{"$f":"BU68/$CE$68","v":5.9821428571428577},0,0,{"$f":"BX68/$CE$68","v":0},1.0720000000000001,0,{"$f":"CA68/$CE$68","v":7.9761904761904772},null,0.13439999999999999]
["3.8.5",null,"E","Kosnik/Pajanta                           10/10 cm","Strut 10/10 cm","m3",{"$f":"CENA!G60","v":0},11.04,0,0.6,{"$f":"$G69*J69","v":0},{"$f":"J69/$CE$69","v":10},0.6,0,{"$f":"M69/$CE$69","v":10},0.6,0,{"$f":"P69/$CE$69","v":10},0.6,0,{"$f":"S69/$CE$69","v":10},null,0,{"$f":"V69/$CE$69","v":0},0.72,0,{"$f":"Y69/$CE$69","v":12},0.24,0,{"$f":"AB69/$CE$69","v":4},null,0,{"$f":"AE69/$CE$69","v":0},0,0,{"$f":"AH69/$CE$69","v":0},0.48,0,{"$f":"AK69/$CE$69","v":8},null,0,{"$f":"AN69/$CE$69","v":0},0.6,0,{"$f":"AQ69/$CE$69","v":10},0.48,0,{"$f":"AT69/$CE$69","v":8},0.84,0,{"$f":"AW69/$CE$69","v":14},0.72,0,{"$f":"AZ69/$CE$69","v":12},0,0,{"$f":"BC69/$CE$69","v":0},0.72,0,{"$f":"BF69/$CE$69","v":12},0.6,0,{"$f":"BI69/$CE$69","v":10},0.48,0,{"$f":"BL69/$CE$69","v":8},0.6,0,{"$f":"BO69/$CE$69","v":10},0.72,0,{"$f":"BR69/$CE$69","v":12},0.6,0,{"$f":"BU69/$CE$69","v":10},0,0,{"$f":"BX69/$CE$69","v":0},0.84,0,{"$f":"CA69/$CE$69","v":14},null,0.06]
["3.8.6",null,"F","Klešta                                         6/12 cm","Collar tie 6/12 cm","m3",{"$f":"CENA!G61","v":0},8.0839999999999979,0,0.42999999999999994,{"$f":"$G70*J70","v":0},{"$f":"J70/$CE$70","v":9.9537037037037024},0.42999999999999994,0,{"$f":"M70/$CE$70","v":9.9537037037037024},0.42999999999999994,0,{"$f":"P70/$CE$70","v":9.9537037037037024},0.42999999999999994,0,{"$f":"S70/$CE$70","v":9.9537037037037024},null,0,{"$f":"V70/$CE$70","v":0},0.51600000000000001,0,{"$f":"Y70/$CE$70","v":11.944444444444445},0,0,{"$f":"AB70/$CE$70","v":0},0.34399999999999997,0,{"$f":"AE70/$CE$70","v":7.9629629629629619},0,0,{"$f":"AH70/$CE$70","v":0},0.34399999999999997,0,{"$f":"AK70/$CE$70","v":7.9629629629629619},null,0,{"$f":"AN70/$CE$70","v":0},0.42999999999999994,0,{"$f":"AQ70/$CE$70","v":9.9537037037037024},0.34399999999999997,0,{"$f":"AT70/$CE$70","v":7.9629629629629619},0.60199999999999998,0,{"$f":"AW70/$CE$70","v":13.935185185185183},0.51600000000000001,0,{"$f":"AZ70/$CE$70","v":11.944444444444445},0,0,{"$f":"BC70/$CE$70","v":0},0.51600000000000001,0,{"$f":"BF70/$CE$70","v":11.944444444444445},0.42999999999999994,0,{"$f":"BI70/$CE$70","v":9.9537037037037024},0.34399999999999997,0,{"$f":"BL70/$CE$70","v":7.9629629629629619},0.42999999999999994,0,{"$f":"BO70/$CE$70","v":9.9537037037037024},0.51600000000000001,0,{"$f":"BR70/$CE$70","v":11.944444444444445},0.42999999999999994,0,{"$f":"BU70/$CE$70","v":9.9537037037037024},0,0,{"$f":"BX70/$CE$70","v":0},0.60199999999999998,0,{"$f":"CA70/$CE$70","v":13.935185185185183},null,4.3200000000000002E-2]
["3.8.7",null,"G","Krovna štafla                                5/8  cm","Roof battens 5/8  cm","m3",{"$f":"CENA!G62","v":0},2.4,0,0,{"$f":"$G71*J71","v":0},{"$f":"J71/$CE$71","v":0},0.48,0,{"$f":"M71/$CE$71","v":20},0,0,{"$f":"P71/$CE$71","v":0},0,0,{"$f":"S71/$CE$71","v":0},0,0,{"$f":"V71/$CE$71","v":0},0,0,{"$f":"Y71/$CE$71","v":0},0.24,0,{"$f":"AB71/$CE$71","v":10},0,0,{"$f":"AE71/$CE$71","v":0},0,0,{"$f":"AH71/$CE$71","v":0},0,0,{"$f":"AK71/$CE$71","v":0},0.96,0,{"$f":"AN71/$CE$71","v":40},0,0,{"$f":"AQ71/$CE$71","v":0},0,0,{"$f":"AT71/$CE$71","v":0},0,0,{"$f":"AW71/$CE$71","v":0},0,0,{"$f":"AZ71/$CE$71","v":0},0.72,0,{"$f":"BC71/$CE$71","v":30},0,0,{"$f":"BF71/$CE$71","v":0},0,0,{"$f":"BI71/$CE$71","v":0},0,0,{"$f":"BL71/$CE$71","v":0},0,0,{"$f":"BO71/$CE$71","v":0},0,0,{"$f":"BR71/$CE$71","v":0},0,0,{"$f":"BU71/$CE$71","v":0},0,0,{"$f":"BX71/$CE$71","v":0},0,0,{"$f":"CA71/$CE$71","v":0},null,2.4E-2]
["3.8.8",null,"H","Tavanjače                                   18/26 cm","attic beams 18/26 cm","m3",{"$f":"CENA!G63","v":0},6.7439999999999998,0,0,{"$f":"$G72*J72","v":0},{"$f":"J72/$CE$72","v":0},5.62,0,{"$f":"M72/$CE$72","v":20.014245014245017},0,0,{"$f":"P72/$CE$72","v":0},1.1240000000000001,0,{"$f":"S72/$CE$72","v":4.0028490028490031},0,0,{"$f":"V72/$CE$72","v":0},0,0,{"$f":"Y72/$CE$72","v":0},0,0,{"$f":"AB72/$CE$72","v":0},0,0,{"$f":"AE72/$CE$72","v":0},0,0,{"$f":"AH72/$CE$72","v":0},0,0,{"$f":"AK72/$CE$72","v":0},null,0,{"$f":"AN72/$CE$72","v":0},0,0,{"$f":"AQ72/$CE$72","v":0},0,0,{"$f":"AT72/$CE$72","v":0},0,0,{"$f":"AW72/$CE$72","v":0},0,0,{"$f":"AZ72/$CE$72","v":0},0,0,{"$f":"BC72/$CE$72","v":0},0,0,{"$f":"BF72/$CE$72","v":0},0,0,{"$f":"BI72/$CE$72","v":0},0,0,{"$f":"BL72/$CE$72","v":0},0,0,{"$f":"BO72/$CE$72","v":0},0,0,{"$f":"BR72/$CE$72","v":0},0,0,{"$f":"BU72/$CE$72","v":0},0,0,{"$f":"BX72/$CE$72","v":0},0,0,{"$f":"CA72/$CE$72","v":0},null,0.28079999999999999]
["3.9","K",9,"Građevinska daska - fosna\n4,8/25/400 cm","Fir board\n4,8/25/400 cm","m3",{"$f":"CENA!G64","v":0},2.016,0,null,{"$f":"$G73*J73","v":0},{"$f":"J73/$CE$73","v":0},null,0,{"$f":"M73/$CE$73","v":0},null,0,{"$f":"P73/$CE$73","v":0},null,0,{"$f":"S73/$CE$73","v":0},2.016,0,{"$f":"V73/$CE$73","v":42},null,0,{"$f":"Y73/$CE$73","v":0},null,0,{"$f":"AB73/$CE$73","v":0},null,0,{"$f":"AE73/$CE$73","v":0},null,0,{"$f":"AH73/$CE$73","v":0},null,0,{"$f":"AK73/$CE$73","v":0},null,0,{"$f":"AN73/$CE$73","v":0},null,0,{"$f":"AQ73/$CE$73","v":0},null,0,{"$f":"AT73/$CE$73","v":0},null,0,{"$f":"AW73/$CE$73","v":0},null,0,{"$f":"AZ73/$CE$73","v":0},null,0,{"$f":"BC73/$CE$73","v":0},null,0,{"$f":"BF73/$CE$73","v":0},null,0,{"$f":"BI73/$CE$73","v":0},null,0,{"$f":"BL73/$CE$73","v":0},null,0,{"$f":"BO73/$CE$73","v":0},null,0,{"$f":"BR73/$CE$73","v":0},null,0,{"$f":"BU73/$CE$73","v":0},null,0,{"$f":"BX73/$CE$73","v":0},null,0,{"$f":"CA73/$CE$73","v":0},null,4.8000000000000001E-2]
["3.10","K",10,"Krovna daska od čamove rezane građe \n2,4-2,5/15 cm, isporučuje se dužine l=3,0 metra","Roof fir board\n2,4-2,5/15 cm, lenght l=3,0 m","m3",{"$f":"CENA!G65","v":0},84.900797029702986,0,2.9702970297029703,{"$f":"$G74*J74","v":0},null,4.9504000000000001,0,null,3.7128712871287131,0,null,1.9801,0,null,null,0,null,3.7128712871287131,0,null,2.9702970297029703,0,null,3.7128712871287131,0,null,3.217821782178218,0,null,3.7128712871287131,0,null,2.9702970297029703,0,null,3.4653465346534653,0,null,3.7128712871287131,0,null,5.1980198019801982,0,null,4.4554455445544559,0,null,3.217821782178218,0,null,5.4455445544554459,0,null,4.4554455445544559,0,null,3.4653465346534653,0,null,3.217821782178218,0,null,5.4455445544554459,0,null,3.9603960396039604,0,null,null,0,null,4.9504950495049505,0]
["3.11","K",11,"Krovna letva od čamove rezane građe \n 3 / 5 cm , isporučuje se dužine l=3,0 metra","Fir batten\n 3 / 5 cm , lenght l=3,0 m","m1",{"$f":"CENA!G66","v":0},14364,0,660,{"$f":"$G75*J75","v":0},{"$f":"J75/$CE$75","v":220},660,0,{"$f":"M75/$CE$75","v":220},660,0,{"$f":"P75/$CE$75","v":220},660,0,{"$f":"S75/$CE$75","v":220},null,0,{"$f":"V75/$CE$75","v":0},792,0,{"$f":"Y75/$CE$75","v":264},300,0,402,528,0,{"$f":"AE75/$CE$75","v":176},0,0,{"$f":"AH75/$CE$75","v":0},528,0,{"$f":"AK75/$CE$75","v":176},528,0,{"$f":"AN75/$CE$75","v":176},660,0,{"$f":"AQ75/$CE$75","v":220},528,0,{"$f":"AT75/$CE$75","v":176},924,0,{"$f":"AW75/$CE$75","v":308},792,0,{"$f":"AZ75/$CE$75","v":264},420,0,{"$f":"BC75/$CE$75","v":140},792,0,{"$f":"BF75/$CE$75","v":264},660,0,{"$f":"BI75/$CE$75","v":220},528,0,{"$f":"BL75/$CE$75","v":176},660,0,{"$f":"BO75/$CE$75","v":220},900,0,{"$f":"BR75/$CE$75","v":300},660,0,{"$f":"BU75/$CE$75","v":220},600,0,{"$f":"BX75/$CE$75","v":200},924,0,{"$f":"CA75/$CE$75","v":308},null,3]
["3.12","K",12,"OSB3  vlagootporne konstruktivne ploče\nd=18 mm / dim. 2440 x 1220","OSB3  moisture resistant structural panels\nd=18 mm / dim. 2440 x 1220","kom/pcs",{"$f":"CENA!G67","v":0},26,0,null,{"$f":"$G76*J76","v":0},null,6,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,20,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["3.13","K",13,"Standardne gips kartonske ploče - Tip A\ndimenzije: 1200-1250 x 2000 mm","Standard plasterboard table - Type A\ndim: 1200-1250 x 2000 mm","kom/pcs",{"$f":"CENA!G68","v":0},100,0,null,{"$f":"$G77*J77","v":0},null,null,0,null,null,0,null,30,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,30,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,40,0,null,null,0]
["3.14","K",14,"Vlagootporne gips kartonske ploče - Tip H2\ndimenzije: 1200-1250 x 2000 mm","Moisture resistant Plasterboard - Type H2\ndim: 1200-1250 x 2000 mm","kom/pcs",{"$f":"CENA!G69","v":0},245,0,null,{"$f":"$G78*J78","v":0},null,40,0,null,null,0,null,5,0,null,null,0,null,null,0,null,null,0,null,null,0,null,50,0,null,20,0,null,40,0,null,30,0,null,null,0,null,null,0,null,null,0,null,50,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,10,0]
["3.15","K",15,"Čelični pocinkovani i farbani olučni elementi prečnika: Ø 100 mm dužine 600 cm","Galvanized steel and painted gutter elements diameter: Ø 100 mm length 600 cm","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["3.15.1",null,"A","Horizontalni polukružni","horizontal semicircular gutter","kom/pcs",{"$f":"CENA!G71","v":0},{"$f":"J80+M80+P80+S80+V80+Y80+AB80+AE80+AH80+AK80+AN80+AQ80+AT80+AW80+AZ80+BC80+BF80+BI80+BL80+BO80+BR80+BU80+BX80+CA80","v":109},{"$f":"G80*H80","v":0},5,{"$f":"$G80*J80","v":0},null,5,{"$f":"$G80*M80","v":0},null,5,{"$f":"$G80*P80","v":0},null,5,{"$f":"$G80*S80","v":0},null,6,{"$f":"$G80*V80","v":0},null,6,{"$f":"$G80*Y80","v":0},null,0,{"$f":"$G80*AB80","v":0},null,4,{"$f":"$G80*AE80","v":0},null,0,{"$f":"$G80*AH80","v":0},null,4,{"$f":"$G80*AK80","v":0},null,4,{"$f":"$G80*AN80","v":0},null,5,{"$f":"$G80*AQ80","v":0},null,4,{"$f":"$G80*AT80","v":0},null,7,{"$f":"$G80*AW80","v":0},null,6,{"$f":"$G80*AZ80","v":0},null,0,{"$f":"$G80*BC80","v":0},null,6,{"$f":"$G80*BF80","v":0},null,5,{"$f":"$G80*BI80","v":0},null,4,{"$f":"$G80*BL80","v":0},null,5,{"$f":"$G80*BO80","v":0},null,6,{"$f":"$G80*BR80","v":0},null,5,{"$f":"$G80*BU80","v":0},null,5,{"$f":"$G80*BX80","v":0},null,7,{"$f":"$G80*CA80","v":0}]
["3.15.2",null,"B","Vertikalni kružni oluk","Vertical circular gutter","kom/pcs",{"$f":"CENA!G72","v":0},{"$f":"J81+M81+P81+S81+V81+Y81+AB81+AE81+AH81+AK81+AN81+AQ81+AT81+AW81+AZ81+BC81+BF81+BI81+BL81+BO81+BR81+BU81+BX81+CA81","v":52},{"$f":"G81*H81","v":0},2,{"$f":"$G81*J81","v":0},null,2,0,null,3,{"$f":"$G81*P81","v":0},null,2,{"$f":"$G81*S81","v":0},null,3,{"$f":"$G81*V81","v":0},null,3,{"$f":"$G81*Y81","v":0},null,null,{"$f":"$G81*AB81","v":0},null,2,{"$f":"$G81*AE81","v":0},null,null,{"$f":"$G81*AH81","v":0},null,2,{"$f":"$G81*AK81","v":0},null,3,{"$f":"$G81*AN81","v":0},null,2,{"$f":"$G81*AQ81","v":0},null,2,{"$f":"$G81*AT81","v":0},null,3,{"$f":"$G81*AW81","v":0},null,3,{"$f":"$G81*AZ81","v":0},null,null,{"$f":"$G81*BC81","v":0},null,3,{"$f":"$G81*BF81","v":0},null,3,{"$f":"$G81*BI81","v":0},null,2,{"$f":"$G81*BL81","v":0},null,2,{"$f":"$G81*BO81","v":0},null,3,{"$f":"$G81*BR81","v":0},null,2,{"$f":"$G81*BU81","v":0},null,2,{"$f":"$G81*BX81","v":0},null,3,{"$f":"$G81*CA81","v":0}]
[]
["4","P",null,"MATERIJAL ZA PODOVE, LAMINAT, PLOČICE I XPS","FLOORING, LAMINATE, TILES AND XPS"]
["4.1","P",1,"Unutrašnje podne keramičke pločice\nMin. dimenzije pločica: 200x300 mm","Floor tiles for inside\nMin. tile size: 200x300 mm","m2",{"$f":"CENA!G75","v":0},{"$f":"J84+M84+P84+S84+V84+Y84+AB84+AE84+AH84+AK84+AN84+AQ84+AT84+AW84+AZ84+BC84+BF84+BI84+BL84+BO84+BR84+BU84+BX84+CA84","v":396},{"$f":"G84*H84","v":0},15,{"$f":"$G84*J84","v":0},null,20,{"$f":"$G84*M84","v":0},null,20,{"$f":"$G84*P84","v":0},null,38,{"$f":"$G84*S84","v":0},null,6,{"$f":"$G84*V84","v":0},null,15,{"$f":"$G84*Y84","v":0},null,20,{"$f":"$G84*AB84","v":0},null,null,{"$f":"$G84*AE84","v":0},null,15,{"$f":"$G84*AH84","v":0},null,12,{"$f":"$G84*AK84","v":0},null,30,{"$f":"$G84*AN84","v":0},null,20,{"$f":"$G84*AQ84","v":0},null,10,{"$f":"$G84*AT84","v":0},null,20,{"$f":"$G84*AW84","v":0},null,10,{"$f":"$G84*AZ84","v":0},null,20,{"$f":"$G84*BC84","v":0},null,20,{"$f":"$G84*BF84","v":0},null,10,{"$f":"$G84*BI84","v":0},null,10,{"$f":"$G84*BL84","v":0},null,20,{"$f":"$G84*BO84","v":0},null,10,{"$f":"$G84*BR84","v":0},null,15,{"$f":"$G84*BU84","v":0},null,20,{"$f":"$G84*BX84","v":0},null,20,{"$f":"$G84*CA84","v":0}]
["4.2","P",2,"Unutrašnje zidne keramičke pločice \nMin. dimenzije pločica: 200x300 mm","Wall tiles for inside\nMin. tile size: 200x300 mm","m2",{"$f":"CENA!G76","v":0},605,0,35,{"$f":"$G85*J85","v":0},null,15,0,null,35,0,null,35,0,null,25,0,null,30,0,null,null,0,null,null,0,null,35,0,null,null,0,null,40,0,null,40,0,null,30,0,null,null,0,null,30,0,null,35,0,null,40,0,null,30,0,null,15,0,null,35,0,null,30,0,null,30,0,null,40,0,null,null,0]
["4.3","P",3,"Lepak za keramičke pločice\nFleksibilni, polimer-cementni lepak","Glue for ceramic tiles\nFlexible, polymer-cement glue","kg",{"$f":"CENA!G77","v":0},3550,0,175,{"$f":"$G86*J86","v":0},null,125,0,null,175,0,null,225,0,null,100,0,null,150,0,null,75,0,null,0,0,null,175,0,null,50,0,null,400,0,null,200,0,null,125,0,null,75,0,null,125,0,null,175,0,null,200,0,null,125,0,null,150,0,null,175,0,null,125,0,null,150,0,null,200,0,null,75,0]
["4.4","P",4,"Fleksibilna masa za fugovanje\nVodoodbojna fug masa na bazi cementa","Flexible mass for grouting\nWaterproof grout cement based","kg",{"$f":"CENA!G78","v":0},636,0,32,{"$f":"$G87*J87","v":0},null,22,0,null,34,0,null,44,0,null,20,0,null,28,0,null,14,0,null,0,0,null,32,0,null,8,0,null,44,0,null,38,0,null,26,0,null,14,0,null,26,0,null,34,0,null,38,0,null,26,0,null,16,0,null,34,0,null,26,0,null,28,0,null,38,0,null,14,0]
["4.5","P",5,"Laminat - jakopresovani (HLP)\nsa klik sistemom, dezen: hrast natur (prirodni)","Laminate (HLP)\nwith click system, design: oak natural (natural)","m2",{"$f":"CENA!G79","v":0},1042,0,50,{"$f":"$G88*J88","v":0},null,60,0,null,80,0,null,50,0,null,null,0,null,70,0,null,50,0,null,null,0,null,76,0,null,null,0,null,60,0,null,60,0,null,null,0,null,70,0,null,20,0,null,70,0,null,80,0,null,null,0,null,60,0,null,40,0,null,null,0,null,50,0,null,70,0,null,26,0]
["4.6","P",6,"Lajsne za laminat od medijapana \nmaterijal: medijapan / MDF","Moldings for laminate MDF\nMaterial: MDF / MDF","m1",{"$f":"CENA!G80","v":0},1029.5999999999999,0,62.4,{"$f":"$G89*J89","v":0},{"$f":"J89/2.6","v":24},62.4,0,{"$f":"M89/2.6","v":24},62.4,0,{"$f":"P89/2.6","v":24},62.4,0,{"$f":"S89/2.6","v":24},null,0,{"$f":"V89/2.6","v":0},62.4,0,{"$f":"Y89/2.6","v":24},62.4,0,{"$f":"AB89/2.6","v":24},null,0,{"$f":"AE89/2.6","v":0},62.4,0,{"$f":"AH89/2.6","v":24},null,0,{"$f":"AK89/2.6","v":0},62.4,0,{"$f":"AN89/2.6","v":24},62.4,0,{"$f":"AQ89/2.6","v":24},null,0,{"$f":"AT89/2.6","v":0},62.4,0,{"$f":"AW89/2.6","v":24},31.2,0,{"$f":"AZ89/2.6","v":12},62.4,0,{"$f":"BC89/2.6","v":24},93.6,0,{"$f":"BF89/2.6","v":36},null,0,{"$f":"BI89/2.6","v":0},62.4,0,{"$f":"BL89/2.6","v":24},31.2,0,{"$f":"BO89/2.6","v":12},null,0,{"$f":"BR89/2.6","v":0},31.2,0,{"$f":"BU89/2.6","v":12},62.4,0,{"$f":"BX89/2.6","v":24},31.2,0,{"$f":"CA89/2.6","v":12}]
["4.7","P",7,"Podloga za laminat od polietilenske pene\nSunđerasta podloga za laminat","The base for laminate of polyethylene foam\nFoam base for laminate","m2",{"$f":"CENA!G81","v":0},1221,0,66,{"$f":"$G90*J90","v":0},null,66,0,null,82.5,0,null,66,0,null,0,0,null,82.5,0,null,66,0,null,0,0,null,82.5,0,null,0,0,null,66,0,null,66,0,null,0,0,null,82.5,0,null,33,0,null,82.5,0,null,82.5,0,null,0,0,null,66,0,null,49.5,0,null,0,0,null,66,0,null,82.5,0,null,33,0]
["4.8","P",8,"Cementni suvi estrih (cementna košuljica).\nPripremljeno cementno praškasto vezivo","Cement dry screed (cement screed)\nPrepared cement powder binder","kg",{"$f":"CENA!G82","v":0},0,0,null,{"$f":"$G91*J91","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["4.9","P",9,"Građevinska PVC folija Za razdvajanje cementne košuljice od termo izolacije.","PVC foil for construction. To separate the cement screed of thermal insulation.","m2",{"$f":"CENA!G83","v":0},1960,0,80,{"$f":"$G92*J92","v":0},null,80,0,null,120,0,null,120,0,null,40,0,null,120,0,null,80,0,null,0,0,null,120,0,null,40,0,null,120,0,null,80,0,null,40,0,null,120,0,null,40,0,null,120,0,null,120,0,null,40,0,null,80,0,null,80,0,null,40,0,null,80,0,null,120,0,null,80,0]
["4.10","P",10,"Stirodur (XPS za izolaciju na podovima)\nploča od ekstrudirane polistirenske pene","Stirodur (XPS insulation for floors)\npanel of extruded polystyrene foam","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["4.10.1",null,"A","debljine d=2 cm","d=2 cm","m2",{"$f":"CENA!G85","v":0},{"$f":"J94+M94+P94+S94+V94+Y94+AB94+AE94+AH94+AK94+AN94+AQ94+AT94+AW94+AZ94+BC94+BF94+BI94+BL94+BO94+BR94+BU94+BX94+CA94","v":1455},{"$f":"G94*H94","v":0},75,{"$f":"$G94*J94","v":0},null,90,{"$f":"$G94*M94","v":0},null,105,{"$f":"$G94*P94","v":0},null,null,{"$f":"$G94*S94","v":0},null,15,{"$f":"$G94*V94","v":0},null,90,{"$f":"$G94*Y94","v":0},null,75,{"$f":"$G94*AB94","v":0},null,0,{"$f":"$G94*AE94","v":0},null,105,{"$f":"$G94*AH94","v":0},null,15,{"$f":"$G94*AK94","v":0},null,90,{"$f":"$G94*AN94","v":0},null,90,{"$f":"$G94*AQ94","v":0},null,15,{"$f":"$G94*AT94","v":0},null,90,{"$f":"$G94*AW94","v":0},null,30,{"$f":"$G94*AZ94","v":0},null,90,{"$f":"$G94*BC94","v":0},null,105,{"$f":"$G94*BF94","v":0},null,15,{"$f":"$G94*BI94","v":0},null,75,{"$f":"$G94*BL94","v":0},null,60,{"$f":"$G94*BO94","v":0},null,15,{"$f":"$G94*BR94","v":0},null,75,{"$f":"$G94*BU94","v":0},null,90,{"$f":"$G94*BX94","v":0},null,45,{"$f":"$G94*CA94","v":0}]
["4.10.2",null,"B","debljine d=5 cm","d=5 cm","m2",{"$f":"CENA!G86","v":0},{"$f":"J95+M95+P95+S95+V95+Y95+AB95+AE95+AH95+AK95+AN95+AQ95+AT95+AW95+AZ95+BC95+BF95+BI95+BL95+BO95+BR95+BU95+BX95+CA95","v":0},{"$f":"G95*H95","v":0},null,{"$f":"$G95*J95","v":0},null,null,0,null,null,{"$f":"$G95*P95","v":0},null,null,{"$f":"$G95*S95","v":0},null,null,{"$f":"$G95*V95","v":0},null,null,{"$f":"$G95*Y95","v":0},null,null,{"$f":"$G95*AB95","v":0},null,null,{"$f":"$G95*AE95","v":0},null,null,{"$f":"$G95*AH95","v":0},null,null,{"$f":"$G95*AK95","v":0},null,null,{"$f":"$G95*AN95","v":0},null,null,{"$f":"$G95*AQ95","v":0},null,null,{"$f":"$G95*AT95","v":0},null,null,{"$f":"$G95*AW95","v":0},null,null,{"$f":"$G95*AZ95","v":0},null,null,{"$f":"$G95*BC95","v":0},null,null,{"$f":"$G95*BF95","v":0},null,null,{"$f":"$G95*BI95","v":0},null,null,{"$f":"$G95*BL95","v":0},null,null,{"$f":"$G95*BO95","v":0},null,null,{"$f":"$G95*BR95","v":0},null,null,{"$f":"$G95*BU95","v":0},null,null,{"$f":"$G95*BX95","v":0},null,null,{"$f":"$G95*CA95","v":0}]
[]
["5","F",null,"MATERIJAL ZA IZRADU FASADE","FACADE MATERIAL"]
["5.1","F",1,"EPS za termoizolaciju fasadnih zidova\nploča od ekspandiranog polistirena ","Thermal insulation for facade walls (EPS)\nplates made of expanded polystyrene","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["5.1.1",null,"A","debljina d=8 cm","d=8 cm","m2",{"$f":"CENA!G90","v":0},{"$f":"J99+M99+P99+S99+V99+Y99+AB99+AE99+AH99+AK99+AN99+AQ99+AT99+AW99+AZ99+BC99+BF99+BI99+BL99+BO99+BR99+BU99+BX99+CA99","v":351},{"$f":"G99*H99","v":0},null,{"$f":"$G99*J99","v":0},null,null,{"$f":"$G99*M99","v":0},null,null,{"$f":"$G99*P99","v":0},null,null,{"$f":"$G99*S99","v":0},null,null,{"$f":"$G99*V99","v":0},null,null,{"$f":"$G99*Y99","v":0},null,null,{"$f":"$G99*AB99","v":0},null,null,{"$f":"$G99*AE99","v":0},null,null,{"$f":"$G99*AH99","v":0},null,null,{"$f":"$G99*AK99","v":0},null,null,{"$f":"$G99*AN99","v":0},null,null,{"$f":"$G99*AQ99","v":0},null,null,{"$f":"$G99*AT99","v":0},null,null,{"$f":"$G99*AW99","v":0},null,null,{"$f":"$G99*AZ99","v":0},null,null,{"$f":"$G99*BC99","v":0},null,180,{"$f":"$G99*BF99","v":0},null,null,{"$f":"$G99*BI99","v":0},null,null,{"$f":"$G99*BL99","v":0},null,null,{"$f":"$G99*BO99","v":0},null,171,{"$f":"$G99*BR99","v":0},null,null,{"$f":"$G99*BU99","v":0},null,null,{"$f":"$G99*BX99","v":0},null,null,{"$f":"$G99*CA99","v":0}]
["5.1.2",null,"B","debljina d=10 cm","d=10 cm","m2",{"$f":"CENA!G91","v":0},2000,0,0,{"$f":"$G100*J100","v":0},null,130,0,null,0,0,null,80,0,null,0,0,null,150,0,null,60,0,null,0,0,null,150,0,null,60,0,null,0,0,null,140,0,null,0,0,null,150,0,null,80,0,null,170,0,null,null,0,null,150,0,null,150,0,null,110,0,null,null,0,null,150,0,null,100,0,null,170,0]
["5.1.3",null,"C","debljina d=12 cm","d=12 cm","m2",{"$f":"CENA!G92","v":0},0,0,null,{"$f":"$G101*J101","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["5.1.4",null,"D","debljina d=14 cm","d=14 cm","m2",{"$f":"CENA!G93","v":0},0,0,null,{"$f":"$G102*J102","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["5.2","F",2,"GrađevinskI lepak za EPS ploče \ncementni lepak namenjen za lepljenje ploča od ekspandiranog polistirena (EPS) i armiranje armaturne (rabic) mrežice ","Construction glue for EPS plates\ncement adhesive for gluing plates made of expanded polystyrene (EPS) and reinforcing wire (rabic) net","kg",{"$f":"CENA!G94","v":0},29970,0,0,{"$f":"$G103*J103","v":0},null,1650,0,null,0,0,null,1020,0,null,0,0,null,1890,0,null,750,0,null,0,0,null,1890,0,null,750,0,null,0,0,null,1770,0,null,0,0,null,1890,0,null,1020,0,null,2130,0,null,2250,0,null,1890,0,null,1890,0,null,1770,0,null,2130,0,null,1890,0,null,1260,0,null,2130,0]
["5.3","F",3,"Armaturna (rabic) staklena mrežica.\nVisokokvalitetna alkalno postojana staklena mrežica","Reinforcing (rabic) fiberglass mesh\nHigh quality alkali resistant fiberglass mesh","m2",{"$f":"CENA!G95","v":0},2650,0,0,{"$f":"$G104*J104","v":0},null,150,0,null,0,0,null,100,0,null,0,0,null,150,0,null,100,0,null,0,0,null,150,0,null,100,0,null,0,0,null,150,0,null,0,0,null,150,0,null,100,0,null,200,0,null,200,0,null,150,0,null,150,0,null,150,0,null,200,0,null,150,0,null,100,0,null,200,0]
["5.4","F",4,"Aktivni predpremaz pre nanošenja tankoslojnog fasadnog maltera.\npredpremaz za izjednačavanje upijanja - podloga","Active primer before applying the thin-layer plaster primer for the equalization of absorption surface","kg",{"$f":"CENA!G96","v":0},750,0,0,{"$f":"$G105*J105","v":0},null,50,0,null,0,0,null,25,0,null,0,0,null,50,0,null,25,0,null,0,0,null,50,0,null,25,0,null,0,0,null,50,0,null,0,0,null,50,0,null,25,0,null,50,0,null,50,0,null,50,0,null,50,0,null,25,0,null,50,0,null,50,0,null,25,0,null,50,0]
["5.5","F",5,"Fasadni tankoslojni akrilni malter\nZavršni malter u pastoznom stanju, namenjen za zaštitu fasadnih zidnih površina","Facade thin-layer acrylic plaster\nFinishing plaster in paste-like state, intended for the protection of facade wall surfaces","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["5.5.1",null,"A","boja približna RAL 1034 -kajsija ","color similar to RAL 1034-apricot","kg",{"$f":"CENA!G98","v":0},{"$f":"J107+M107+P107+S107+V107+Y107+AB107+AE107+AH107+AK107+AN107+AQ107+AT107+AW107+AZ107+BC107+BF107+BI107+BL107+BO107+BR107+BU107+BX107+CA107","v":8025},{"$f":"G107*H107","v":0},0,{"$f":"$G107*J107","v":0},null,475,{"$f":"$G107*M107","v":0},null,0,{"$f":"$G107*P107","v":0},null,300,{"$f":"$G107*S107","v":0},null,0,{"$f":"$G107*V107","v":0},null,550,{"$f":"$G107*Y107","v":0},null,225,{"$f":"$G107*AB107","v":0},null,0,{"$f":"$G107*AE107","v":0},null,550,{"$f":"$G107*AH107","v":0},null,325,{"$f":"$G107*AK107","v":0},null,0,{"$f":"$G107*AN107","v":0},null,500,{"$f":"$G107*AQ107","v":0},null,0,{"$f":"$G107*AT107","v":0},null,550,{"$f":"$G107*AW107","v":0},null,600,{"$f":"$G107*AZ107","v":0},null,600,{"$f":"$G107*BC107","v":0},null,null,{"$f":"$G107*BF107","v":0},null,550,{"$f":"$G107*BI107","v":0},null,550,{"$f":"$G107*BL107","v":0},null,500,{"$f":"$G107*BO107","v":0},null,null,{"$f":"$G107*BR107","v":0},null,550,{"$f":"$G107*BU107","v":0},null,600,{"$f":"$G107*BX107","v":0},null,600,{"$f":"$G107*CA107","v":0}]
["5.5.2",null,"B","boja približna RAL 6005 -pastelno zelena","color similar to RAL 6005 pastel-green","kg",{"$f":"CENA!G99","v":0},{"$f":"J108+M108+P108+S108+V108+Y108+AB108+AE108+AH108+AK108+AN108+AQ108+AT108+AW108+AZ108+BC108+BF108+BI108+BL108+BO108+BR108+BU108+BX108+CA108","v":0},{"$f":"G108*H108","v":0},null,{"$f":"$G108*J108","v":0},null,null,0,null,null,{"$f":"$G108*P108","v":0},null,null,0,null,null,{"$f":"$G108*V108","v":0},null,null,{"$f":"$G108*Y108","v":0},null,null,{"$f":"$G108*AB108","v":0},null,null,{"$f":"$G108*AE108","v":0},null,null,{"$f":"$G108*AH108","v":0},null,null,{"$f":"$G108*AK108","v":0},null,null,{"$f":"$G108*AN108","v":0},null,null,{"$f":"$G108*AQ108","v":0},null,null,{"$f":"$G108*AT108","v":0},null,null,{"$f":"$G108*AW108","v":0},null,null,{"$f":"$G108*AZ108","v":0},null,null,{"$f":"$G108*BC108","v":0},null,null,{"$f":"$G108*BF108","v":0},null,null,{"$f":"$G108*BI108","v":0},null,null,{"$f":"$G108*BL108","v":0},null,null,{"$f":"$G108*BO108","v":0},null,null,{"$f":"$G108*BR108","v":0},null,null,{"$f":"$G108*BU108","v":0},null,null,{"$f":"$G108*BX108","v":0},null,null,{"$f":"$G108*CA108","v":0}]
["5.5.3",null,"C","boja približna RAL 5023 -pastelno plava","color similar to RAL 5023 pastel-blue","kg",{"$f":"CENA!G100","v":0},{"$f":"J109+M109+P109+S109+V109+Y109+AB109+AE109+AH109+AK109+AN109+AQ109+AT109+AW109+AZ109+BC109+BF109+BI109+BL109+BO109+BR109+BU109+BX109+CA109","v":0},{"$f":"G109*H109","v":0},null,{"$f":"$G109*J109","v":0},null,null,0,null,null,{"$f":"$G109*P109","v":0},null,null,0,null,null,{"$f":"$G109*V109","v":0},null,null,{"$f":"$G109*Y109","v":0},null,null,{"$f":"$G109*AB109","v":0},null,null,{"$f":"$G109*AE109","v":0},null,null,{"$f":"$G109*AH109","v":0},null,null,{"$f":"$G109*AK109","v":0},null,null,{"$f":"$G109*AN109","v":0},null,null,{"$f":"$G109*AQ109","v":0},null,null,{"$f":"$G109*AT109","v":0},null,null,{"$f":"$G109*AW109","v":0},null,null,{"$f":"$G109*AZ109","v":0},null,null,{"$f":"$G109*BC109","v":0},null,null,{"$f":"$G109*BF109","v":0},null,null,{"$f":"$G109*BI109","v":0},null,null,{"$f":"$G109*BL109","v":0},null,null,{"$f":"$G109*BO109","v":0},null,null,{"$f":"$G109*BR109","v":0},null,null,{"$f":"$G109*BU109","v":0},null,null,{"$f":"$G109*BX109","v":0},null,null,{"$f":"$G109*CA109","v":0}]
["5.5.4",null,"D","boja približna RAL 3011 -pastelno crvena","color similar to RAL 3011 pastel-red","kg",{"$f":"CENA!G101","v":0},{"$f":"J110+M110+P110+S110+V110+Y110+AB110+AE110+AH110+AK110+AN110+AQ110+AT110+AW110+AZ110+BC110+BF110+BI110+BL110+BO110+BR110+BU110+BX110+CA110","v":0},{"$f":"G110*H110","v":0},null,{"$f":"$G110*J110","v":0},null,null,0,null,null,{"$f":"$G110*P110","v":0},null,null,0,null,null,{"$f":"$G110*V110","v":0},null,null,{"$f":"$G110*Y110","v":0},null,null,{"$f":"$G110*AB110","v":0},null,null,{"$f":"$G110*AE110","v":0},null,null,{"$f":"$G110*AH110","v":0},null,null,{"$f":"$G110*AK110","v":0},null,null,{"$f":"$G110*AN110","v":0},null,null,{"$f":"$G110*AQ110","v":0},null,null,{"$f":"$G110*AT110","v":0},null,null,{"$f":"$G110*AW110","v":0},null,null,{"$f":"$G110*AZ110","v":0},null,null,{"$f":"$G110*BC110","v":0},null,null,{"$f":"$G110*BF110","v":0},null,null,{"$f":"$G110*BI110","v":0},null,null,{"$f":"$G110*BL110","v":0},null,null,{"$f":"$G110*BO110","v":0},null,null,{"$f":"$G110*BR110","v":0},null,null,{"$f":"$G110*BU110","v":0},null,null,{"$f":"$G110*BX110","v":0},null,null,{"$f":"$G110*CA110","v":0}]
["5.5.5",null,"E","boja približna RAL 8002 -braon","color similar to RAL 8002 brown","kg",{"$f":"CENA!G102","v":0},{"$f":"J111+M111+P111+S111+V111+Y111+AB111+AE111+AH111+AK111+AN111+AQ111+AT111+AW111+AZ111+BC111+BF111+BI111+BL111+BO111+BR111+BU111+BX111+CA111","v":0},{"$f":"G111*H111","v":0},null,{"$f":"$G111*J111","v":0},null,null,0,null,null,{"$f":"$G111*P111","v":0},null,null,0,null,null,{"$f":"$G111*V111","v":0},null,null,{"$f":"$G111*Y111","v":0},null,null,{"$f":"$G111*AB111","v":0},null,null,{"$f":"$G111*AE111","v":0},null,null,{"$f":"$G111*AH111","v":0},null,null,{"$f":"$G111*AK111","v":0},null,null,{"$f":"$G111*AN111","v":0},null,null,{"$f":"$G111*AQ111","v":0},null,null,{"$f":"$G111*AT111","v":0},null,null,{"$f":"$G111*AW111","v":0},null,null,{"$f":"$G111*AZ111","v":0},null,null,{"$f":"$G111*BC111","v":0},null,null,{"$f":"$G111*BF111","v":0},null,null,{"$f":"$G111*BI111","v":0},null,null,{"$f":"$G111*BL111","v":0},null,null,{"$f":"$G111*BO111","v":0},null,null,{"$f":"$G111*BR111","v":0},null,null,{"$f":"$G111*BU111","v":0},null,null,{"$f":"$G111*BX111","v":0},null,null,{"$f":"$G111*CA111","v":0}]
[]
["6","H",null,"MATERIJAL ZA HIDRO IZOLACIJE","WATERPROOFING MATERIAL"]
["6.1","H",1,"Bitulit (prethodni premaz za hidroizolaciju)\nUpotrebljava se u isporučenom stanju (hladan  postupak ) bez zagrevanja","Bitulit (previous coating for waterproofing)\nIt is used as delivered (cold process) without heating","kg",{"$f":"CENA!G105","v":0},{"$f":"J114+M114+P114+S114+V114+Y114+AB114+AE114+AH114+AK114+AN114+AQ114+AT114+AW114+AZ114+BC114+BF114+BI114+BL114+BO114+BR114+BU114+BX114+CA114","v":135},{"$f":"G114*H114","v":0},18,{"$f":"$G114*J114","v":0},null,null,{"$f":"$G114*M114","v":0},null,18,{"$f":"$G114*P114","v":0},null,null,{"$f":"$G114*S114","v":0},null,null,{"$f":"$G114*V114","v":0},null,null,{"$f":"$G114*Y114","v":0},null,null,{"$f":"$G114*AB114","v":0},null,null,{"$f":"$G114*AE114","v":0},null,9,{"$f":"$G114*AH114","v":0},null,null,{"$f":"$G114*AK114","v":0},null,9,{"$f":"$G114*AN114","v":0},null,9,{"$f":"$G114*AQ114","v":0},null,null,{"$f":"$G114*AT114","v":0},null,null,{"$f":"$G114*AW114","v":0},null,null,{"$f":"$G114*AZ114","v":0},null,null,{"$f":"$G114*BC114","v":0},null,null,{"$f":"$G114*BF114","v":0},null,9,{"$f":"$G114*BI114","v":0},null,18,{"$f":"$G114*BL114","v":0},null,18,{"$f":"$G114*BO114","v":0},null,9,{"$f":"$G114*BR114","v":0},null,18,{"$f":"$G114*BU114","v":0},null,null,{"$f":"$G114*BX114","v":0},null,null,{"$f":"$G114*CA114","v":0}]
["6.2","H",2,"Poliazbitol (hladni premaz za hidroizolaciju) Upotrebljava se u isporučenom stanju (hladan postupak) bez zagrevanja","POLYASBITOL (cold coating for waterproofing)\nIt is used as delivered (cold process) without heating","kg",{"$f":"CENA!G106","v":0},{"$f":"J115+M115+P115+S115+V115+Y115+AB115+AE115+AH115+AK115+AN115+AQ115+AT115+AW115+AZ115+BC115+BF115+BI115+BL115+BO115+BR115+BU115+BX115+CA115","v":0},{"$f":"G115*H115","v":0},null,{"$f":"$G115*J115","v":0},null,null,0,null,null,{"$f":"$G115*P115","v":0},null,null,{"$f":"$G115*S115","v":0},null,null,{"$f":"$G115*V115","v":0},null,null,{"$f":"$G115*Y115","v":0},null,null,{"$f":"$G115*AB115","v":0},null,null,{"$f":"$G115*AE115","v":0},null,null,{"$f":"$G115*AH115","v":0},null,null,{"$f":"$G115*AK115","v":0},null,null,{"$f":"$G115*AN115","v":0},null,null,{"$f":"$G115*AQ115","v":0},null,null,{"$f":"$G115*AT115","v":0},null,null,{"$f":"$G115*AW115","v":0},null,null,{"$f":"$G115*AZ115","v":0},null,null,{"$f":"$G115*BC115","v":0},null,null,{"$f":"$G115*BF115","v":0},null,null,{"$f":"$G115*BI115","v":0},null,null,{"$f":"$G115*BL115","v":0},null,null,{"$f":"$G115*BO115","v":0},null,null,{"$f":"$G115*BR115","v":0},null,null,{"$f":"$G115*BU115","v":0},null,null,{"$f":"$G115*BX115","v":0},null,null,{"$f":"$G115*CA115","v":0}]
["6.3","H",3,"Ter papir Bitumenska hidroizolaciona traka.","Ter paper Bituminous waterproofing tape.","m2",{"$f":"CENA!G107","v":0},{"$f":"J116+M116+P116+S116+V116+Y116+AB116+AE116+AH116+AK116+AN116+AQ116+AT116+AW116+AZ116+BC116+BF116+BI116+BL116+BO116+BR116+BU116+BX116+CA116","v":0},{"$f":"G116*H116","v":0},null,{"$f":"$G116*J116","v":0},null,null,0,null,null,{"$f":"$G116*P116","v":0},null,null,{"$f":"$G116*S116","v":0},null,null,{"$f":"$G116*V116","v":0},null,null,{"$f":"$G116*Y116","v":0},null,null,{"$f":"$G116*AB116","v":0},null,null,{"$f":"$G116*AE116","v":0},null,null,{"$f":"$G116*AH116","v":0},null,null,{"$f":"$G116*AK116","v":0},null,null,{"$f":"$G116*AN116","v":0},null,null,{"$f":"$G116*AQ116","v":0},null,null,{"$f":"$G116*AT116","v":0},null,null,{"$f":"$G116*AW116","v":0},null,null,{"$f":"$G116*AZ116","v":0},null,null,{"$f":"$G116*BC116","v":0},null,null,{"$f":"$G116*BF116","v":0},null,null,{"$f":"$G116*BI116","v":0},null,null,{"$f":"$G116*BL116","v":0},null,null,{"$f":"$G116*BO116","v":0},null,null,{"$f":"$G116*BR116","v":0},null,null,{"$f":"$G116*BU116","v":0},null,null,{"$f":"$G116*BX116","v":0},null,null,{"$f":"$G116*CA116","v":0}]
["6.4","H",4,"Kondor V-3 (hidroizolaciona traka)\nPlastomer-bitumenska traka, \nuložak stakleni voal, debljina:  ≥ 3 mm","Condor V-3 (waterproof tape)\nPlastomer-bituminous tape,\nglass mat, thickness: ≥ 3 mm","m2",{"$f":"CENA!G108","v":0},{"$f":"J117+M117+P117+S117+V117+Y117+AB117+AE117+AH117+AK117+AN117+AQ117+AT117+AW117+AZ117+BC117+BF117+BI117+BL117+BO117+BR117+BU117+BX117+CA117","v":450},{"$f":"G117*H117","v":0},70,{"$f":"$G117*J117","v":0},null,null,0,null,70,{"$f":"$G117*P117","v":0},null,null,{"$f":"$G117*S117","v":0},null,null,{"$f":"$G117*V117","v":0},null,null,{"$f":"$G117*Y117","v":0},null,null,{"$f":"$G117*AB117","v":0},null,null,{"$f":"$G117*AE117","v":0},null,20,{"$f":"$G117*AH117","v":0},null,null,{"$f":"$G117*AK117","v":0},null,20,{"$f":"$G117*AN117","v":0},null,60,{"$f":"$G117*AQ117","v":0},null,null,{"$f":"$G117*AT117","v":0},null,null,{"$f":"$G117*AW117","v":0},null,null,{"$f":"$G117*AZ117","v":0},null,null,{"$f":"$G117*BC117","v":0},null,null,{"$f":"$G117*BF117","v":0},null,50,{"$f":"$G117*BI117","v":0},null,60,{"$f":"$G117*BL117","v":0},null,30,{"$f":"$G117*BO117","v":0},null,20,{"$f":"$G117*BR117","v":0},null,50,{"$f":"$G117*BU117","v":0},null,null,{"$f":"$G117*BX117","v":0},null,null,{"$f":"$G117*CA117","v":0}]
[]
["7","S",null,"STOLARIJA","DOORS AND WINDOWS"]
["7.1","S",1,"Ulazna vrata od PVC-a (komplet pozicija). \nboja profila: bela RAL 9003\nbroj komora: ≥  5 komora\nširina x visina (zidarske mere)","Entrance door of PVC (set position)\nProfile color: white RAL 9003 \nNumber of chambers: ≥ 5 chambers \nwidth x height (masonry measures)","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["7.1.1",null,"A","JK    90x210 cm - Leva       90 cm ","one wing  90x210 cm - Left      90 cm ","kom/pcs",{"$f":"CENA!G112","v":0},{"$f":"J121+M121+P121+S121+V121+Y121+AB121+AE121+AH121+AK121+AN121+AQ121+AT121+AW121+AZ121+BC121+BF121+BI121+BL121+BO121+BR121+BU121+BX121+CA121","v":5},{"$f":"G121*H121","v":0},null,{"$f":"$G121*J121","v":0},null,null,{"$f":"$G121*M121","v":0},null,1,{"$f":"$G121*P121","v":0},null,null,{"$f":"$G121*S121","v":0},null,null,{"$f":"$G121*V121","v":0},null,null,{"$f":"$G121*Y121","v":0},null,2,{"$f":"$G121*AB121","v":0},null,null,{"$f":"$G121*AE121","v":0},null,null,{"$f":"$G121*AH121","v":0},null,null,{"$f":"$G121*AK121","v":0},null,null,{"$f":"$G121*AN121","v":0},null,1,{"$f":"$G121*AQ121","v":0},null,1,{"$f":"$G121*AT121","v":0},null,null,{"$f":"$G121*AW121","v":0},null,null,{"$f":"$G121*AZ121","v":0},null,null,{"$f":"$G121*BC121","v":0},null,null,{"$f":"$G121*BF121","v":0},null,null,{"$f":"$G121*BI121","v":0},null,null,{"$f":"$G121*BL121","v":0},null,null,{"$f":"$G121*BO121","v":0},null,null,{"$f":"$G121*BR121","v":0},null,null,{"$f":"$G121*BU121","v":0},null,null,{"$f":"$G121*BX121","v":0},null,null,{"$f":"$G121*CA121","v":0}]
["7.1.2",null,"B","JK    90x210 cm - Desna    90 cm","one wing  90x210 cm - Right    90 cm","kom/pcs",{"$f":"CENA!G113","v":0},{"$f":"J122+M122+P122+S122+V122+Y122+AB122+AE122+AH122+AK122+AN122+AQ122+AT122+AW122+AZ122+BC122+BF122+BI122+BL122+BO122+BR122+BU122+BX122+CA122","v":9},{"$f":"G122*H122","v":0},1,{"$f":"$G122*J122","v":0},null,null,0,null,null,{"$f":"$G122*P122","v":0},null,null,0,null,null,{"$f":"$G122*V122","v":0},null,null,{"$f":"$G122*Y122","v":0},null,null,{"$f":"$G122*AB122","v":0},null,null,{"$f":"$G122*AE122","v":0},null,null,{"$f":"$G122*AH122","v":0},null,1,{"$f":"$G122*AK122","v":0},null,1,{"$f":"$G122*AN122","v":0},null,null,{"$f":"$G122*AQ122","v":0},null,null,{"$f":"$G122*AT122","v":0},null,3,{"$f":"$G122*AW122","v":0},null,null,{"$f":"$G122*AZ122","v":0},null,null,{"$f":"$G122*BC122","v":0},null,null,{"$f":"$G122*BF122","v":0},null,null,{"$f":"$G122*BI122","v":0},null,1,{"$f":"$G122*BL122","v":0},null,null,{"$f":"$G122*BO122","v":0},null,1,{"$f":"$G122*BR122","v":0},null,null,{"$f":"$G122*BU122","v":0},null,null,{"$f":"$G122*BX122","v":0},null,1,{"$f":"$G122*CA122","v":0}]
["7.1.3",null,"C","DK 120x210 cm - Leva       90+30 cm","two wings 120x210 cm - Left        90+30 cm","kom/pcs",{"$f":"CENA!G114","v":0},{"$f":"J123+M123+P123+S123+V123+Y123+AB123+AE123+AH123+AK123+AN123+AQ123+AT123+AW123+AZ123+BC123+BF123+BI123+BL123+BO123+BR123+BU123+BX123+CA123","v":5},{"$f":"G123*H123","v":0},null,{"$f":"$G123*J123","v":0},null,1,0,null,null,{"$f":"$G123*P123","v":0},null,null,0,null,1,{"$f":"$G123*V123","v":0},null,1,{"$f":"$G123*Y123","v":0},null,null,{"$f":"$G123*AB123","v":0},null,1,{"$f":"$G123*AE123","v":0},null,null,{"$f":"$G123*AH123","v":0},null,null,{"$f":"$G123*AK123","v":0},null,null,{"$f":"$G123*AN123","v":0},null,null,{"$f":"$G123*AQ123","v":0},null,null,{"$f":"$G123*AT123","v":0},null,null,{"$f":"$G123*AW123","v":0},null,1,{"$f":"$G123*AZ123","v":0},null,null,{"$f":"$G123*BC123","v":0},null,null,{"$f":"$G123*BF123","v":0},null,null,{"$f":"$G123*BI123","v":0},null,null,{"$f":"$G123*BL123","v":0},null,null,{"$f":"$G123*BO123","v":0},null,null,{"$f":"$G123*BR123","v":0},null,null,{"$f":"$G123*BU123","v":0},null,null,{"$f":"$G123*BX123","v":0},null,null,{"$f":"$G123*CA123","v":0}]
["7.1.4",null,"D","DK 120x210 cm - Desna    90+30 cm","two wings 120x210 cm - Right    90+30 cm","kom/pcs",{"$f":"CENA!G115","v":0},{"$f":"J124+M124+P124+S124+V124+Y124+AB124+AE124+AH124+AK124+AN124+AQ124+AT124+AW124+AZ124+BC124+BF124+BI124+BL124+BO124+BR124+BU124+BX124+CA124","v":2},{"$f":"G124*H124","v":0},null,{"$f":"$G124*J124","v":0},null,null,0,null,null,{"$f":"$G124*P124","v":0},null,1,0,null,null,{"$f":"$G124*V124","v":0},null,null,{"$f":"$G124*Y124","v":0},null,null,{"$f":"$G124*AB124","v":0},null,null,{"$f":"$G124*AE124","v":0},null,null,{"$f":"$G124*AH124","v":0},null,null,{"$f":"$G124*AK124","v":0},null,null,{"$f":"$G124*AN124","v":0},null,null,{"$f":"$G124*AQ124","v":0},null,null,{"$f":"$G124*AT124","v":0},null,null,{"$f":"$G124*AW124","v":0},null,null,{"$f":"$G124*AZ124","v":0},null,null,{"$f":"$G124*BC124","v":0},null,1,{"$f":"$G124*BF124","v":0},null,null,{"$f":"$G124*BI124","v":0},null,null,{"$f":"$G124*BL124","v":0},null,null,{"$f":"$G124*BO124","v":0},null,null,{"$f":"$G124*BR124","v":0},null,null,{"$f":"$G124*BU124","v":0},null,null,{"$f":"$G124*BX124","v":0},null,null,{"$f":"$G124*CA124","v":0}]
["7.2","S",2,"Prozori od PVC-a (komplet pozicija).\nVertikalno i horizontalno otvaranje, boja profila: bela RAL 9003, broj komora: ≥  5 komora\nširina x visina (zidarske mere)","Windows made of PVC (set position)\nVertical and horizontal opening, color profile: white RAL 9003, the number of chambers: ≥ 5 chambers \nwidth x height (masonry measures)","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["7.2.1",null,"A","JK     60x60 cm ","one wing 60x60 cm ","kom/pcs",{"$f":"CENA!G117","v":0},{"$f":"J126+M126+P126+S126+V126+Y126+AB126+AE126+AH126+AK126+AN126+AQ126+AT126+AW126+AZ126+BC126+BF126+BI126+BL126+BO126+BR126+BU126+BX126+CA126","v":31},{"$f":"G126*H126","v":0},3,{"$f":"$G126*J126","v":0},null,1,{"$f":"$G126*M126","v":0},null,1,{"$f":"$G126*P126","v":0},null,2,{"$f":"$G126*S126","v":0},null,3,{"$f":"$G126*V126","v":0},null,3,{"$f":"$G126*Y126","v":0},null,1,{"$f":"$G126*AB126","v":0},null,1,{"$f":"$G126*AE126","v":0},null,3,{"$f":"$G126*AH126","v":0},null,null,{"$f":"$G126*AK126","v":0},null,2,{"$f":"$G126*AN126","v":0},null,null,{"$f":"$G126*AQ126","v":0},null,null,{"$f":"$G126*AT126","v":0},null,null,{"$f":"$G126*AW126","v":0},null,2,{"$f":"$G126*AZ126","v":0},null,null,{"$f":"$G126*BC126","v":0},null,2,{"$f":"$G126*BF126","v":0},null,1,{"$f":"$G126*BI126","v":0},null,null,{"$f":"$G126*BL126","v":0},null,2,{"$f":"$G126*BO126","v":0},null,2,{"$f":"$G126*BR126","v":0},null,1,{"$f":"$G126*BU126","v":0},null,1,{"$f":"$G126*BX126","v":0},null,null,{"$f":"$G126*CA126","v":0}]
["7.2.2",null,"B","JK     80x80 cm","one wing 80x80 cm","kom/pcs",{"$f":"CENA!G118","v":0},9,0,null,{"$f":"$G127*J127","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,3,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,2,0,null,1,0,null,1,0,null,null,0,null,null,0,null,2,0]
["7.2.3",null,"C","JK    80x120 cm    ","one wing 80x120 cm    ","kom/pcs",{"$f":"CENA!G119","v":0},30,0,4,{"$f":"$G128*J128","v":0},null,4,0,null,5,0,null,null,0,null,1,0,null,null,0,null,7,0,null,null,0,null,null,0,null,null,0,null,1,0,null,6,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,1,0,null,null,0,null,1,0,null,null,0,null,null,0,null,null,0]
["7.2.4",null,"D","JK    80x140 cm    ","one wing 80x140 cm ","kom/pcs",{"$f":"CENA!G120","v":0},2,0,null,{"$f":"$G129*J129","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,1,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,1,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["7.2.5",null,"E","JK  100x120 cm","one wing 100x120 cm","kom/pcs",{"$f":"CENA!G121","v":0},15,0,2,{"$f":"$G130*J130","v":0},null,null,0,null,null,0,null,3,0,null,null,0,null,null,0,null,1,0,null,null,0,null,null,0,null,null,0,null,1,0,null,null,0,null,null,0,null,1,0,null,4,0,null,2,0,null,1,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["7.2.6",null,"F","JK  100x140 cm","one wing 100x140 cm","kom/pcs",{"$f":"CENA!G122","v":0},3,0,null,{"$f":"$G131*J131","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,3,0,null,null,0]
["7.2.7",null,"G","DK  120x120 cm","two wings 120x120 cm","kom/pcs",{"$f":"CENA!G123","v":0},12,0,null,{"$f":"$G132*J132","v":0},null,null,0,null,1,0,null,1,0,null,null,0,null,null,0,null,null,0,null,4,0,null,2,0,null,null,0,null,null,0,null,null,0,null,null,0,null,2,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,2,0,null,null,0,null,null,0,null,null,0]
["7.2.8",null,"H","DK  120x140 cm","two wings 120x140 cm","kom/pcs",{"$f":"CENA!G124","v":0},6,0,null,{"$f":"$G133*J133","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,2,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,4,0]
["7.2.9",null,"I","DK  140x120 cm ","two wings 140x120 cm ","kom/pcs",{"$f":"CENA!G125","v":0},9,0,null,{"$f":"$G134*J134","v":0},null,null,0,null,null,0,null,null,0,null,2,0,null,null,0,null,null,0,null,null,0,null,null,0,null,2,0,null,null,0,null,null,0,null,null,0,null,null,0,null,2,0,null,1,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,2,0,null,null,0,null,null,0]
["7.2.10",null,"J","DK  140x140 cm ","two wings 140x140 cm ","kom/pcs",{"$f":"CENA!G126","v":0},6,0,null,{"$f":"$G135*J135","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,4,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,2,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["7.2.11",null,"K","DK  160x120 cm","two wings 160x120 cm","kom/pcs",{"$f":"CENA!G127","v":0},6,0,null,{"$f":"$G136*J136","v":0},null,null,0,null,null,0,null,1,0,null,null,0,null,3,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,2,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["7.2.12",null,"L","DK  160x140 cm","two wings 160x140 cm","kom/pcs",{"$f":"CENA!G128","v":0},12,0,null,{"$f":"$G137*J137","v":0},null,null,0,null,null,0,null,null,0,null,2,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,2,0,null,null,0,null,null,0,null,3,0,null,null,0,null,2,0,null,1,0,null,2,0,null,null,0,null,null,0,null,null,0]
["7.3","S",3,"Krovni prozor sa  aluminijumskom opšivkom od laminirane i impregnirane čamove građe","Roof window with aluminum flashings of laminated and impregnated fir timber","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["7.3.1",null,"A","dimenzije 66 x 118   (širinaxvisina)","66 x 118 (width x height)","kom/pcs",{"$f":"CENA!G130","v":0},{"$f":"J139+M139+P139+S139+V139+Y139+AB139+AE139+AH139+AK139+AN139+AQ139+AT139+AW139+AZ139+BC139+BF139+BI139+BL139+BO139+BR139+BU139+BX139+CA139","v":0},{"$f":"G139*H139","v":0},null,{"$f":"$G139*J139","v":0},null,null,{"$f":"$G139*M139","v":0},null,null,{"$f":"$G139*P139","v":0},null,null,{"$f":"$G139*S139","v":0},null,null,{"$f":"$G139*V139","v":0},null,null,{"$f":"$G139*Y139","v":0},null,null,{"$f":"$G139*AB139","v":0},null,null,{"$f":"$G139*AE139","v":0},null,null,{"$f":"$G139*AH139","v":0},null,null,{"$f":"$G139*AK139","v":0},null,null,{"$f":"$G139*AN139","v":0},null,null,{"$f":"$G139*AQ139","v":0},null,null,{"$f":"$G139*AT139","v":0},null,null,{"$f":"$G139*AW139","v":0},null,null,{"$f":"$G139*AZ139","v":0},null,null,{"$f":"$G139*BC139","v":0},null,null,{"$f":"$G139*BF139","v":0},null,null,{"$f":"$G139*BI139","v":0},null,null,{"$f":"$G139*BL139","v":0},null,null,{"$f":"$G139*BO139","v":0},null,null,{"$f":"$G139*BR139","v":0},null,null,{"$f":"$G139*BU139","v":0},null,null,{"$f":"$G139*BX139","v":0},null,null,{"$f":"$G139*CA139","v":0}]
["7.3.2",null,"B","dimenzije 78 x 98     (širinaxvisina)","78 x 98   (width x height)","kom/pcs",{"$f":"CENA!G131","v":0},{"$f":"J140+M140+P140+S140+V140+Y140+AB140+AE140+AH140+AK140+AN140+AQ140+AT140+AW140+AZ140+BC140+BF140+BI140+BL140+BO140+BR140+BU140+BX140+CA140","v":0},{"$f":"G140*H140","v":0},null,{"$f":"$G140*J140","v":0},null,null,0,null,null,{"$f":"$G140*P140","v":0},null,null,0,null,null,{"$f":"$G140*V140","v":0},null,null,{"$f":"$G140*Y140","v":0},null,null,{"$f":"$G140*AB140","v":0},null,null,{"$f":"$G140*AE140","v":0},null,null,{"$f":"$G140*AH140","v":0},null,null,{"$f":"$G140*AK140","v":0},null,null,{"$f":"$G140*AN140","v":0},null,null,{"$f":"$G140*AQ140","v":0},null,null,{"$f":"$G140*AT140","v":0},null,null,{"$f":"$G140*AW140","v":0},null,null,{"$f":"$G140*AZ140","v":0},null,null,{"$f":"$G140*BC140","v":0},null,null,{"$f":"$G140*BF140","v":0},null,null,{"$f":"$G140*BI140","v":0},null,null,{"$f":"$G140*BL140","v":0},null,null,{"$f":"$G140*BO140","v":0},null,null,{"$f":"$G140*BR140","v":0},null,null,{"$f":"$G140*BU140","v":0},null,null,{"$f":"$G140*BX140","v":0},null,null,{"$f":"$G140*CA140","v":0}]
["7.3.3",null,"C","dimenzije 78 x 118   (širinaxvisina)","78 x 118 (width x height)","kom/pcs",{"$f":"CENA!G132","v":0},{"$f":"J141+M141+P141+S141+V141+Y141+AB141+AE141+AH141+AK141+AN141+AQ141+AT141+AW141+AZ141+BC141+BF141+BI141+BL141+BO141+BR141+BU141+BX141+CA141","v":0},{"$f":"G141*H141","v":0},null,{"$f":"$G141*J141","v":0},null,null,0,null,null,{"$f":"$G141*P141","v":0},null,null,0,null,null,{"$f":"$G141*V141","v":0},null,null,{"$f":"$G141*Y141","v":0},null,null,{"$f":"$G141*AB141","v":0},null,null,{"$f":"$G141*AE141","v":0},null,null,{"$f":"$G141*AH141","v":0},null,null,{"$f":"$G141*AK141","v":0},null,null,{"$f":"$G141*AN141","v":0},null,null,{"$f":"$G141*AQ141","v":0},null,null,{"$f":"$G141*AT141","v":0},null,null,{"$f":"$G141*AW141","v":0},null,null,{"$f":"$G141*AZ141","v":0},null,null,{"$f":"$G141*BC141","v":0},null,null,{"$f":"$G141*BF141","v":0},null,null,{"$f":"$G141*BI141","v":0},null,null,{"$f":"$G141*BL141","v":0},null,null,{"$f":"$G141*BO141","v":0},null,null,{"$f":"$G141*BR141","v":0},null,null,{"$f":"$G141*BU141","v":0},null,null,{"$f":"$G141*BX141","v":0},null,null,{"$f":"$G141*CA141","v":0}]
["7.4","S",4,"Balkonska vrata od PVC-a (komplet pozicija). \nboja profila: bela RAL 9003\nbroj komora: ≥  5 komora\nširina x visina (zidarske mere)","Balcony doors from PVC (set position)\nProfile color: white RAL 9003 \nNumber of chambers: ≥ 5 chambers \nwidth x height (masonry measures)","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["7.4.1",null,"A","JK     90x210 cm   - Leva","one wing  90x210 cm - Left     ","kom/pcs",{"$f":"CENA!G134","v":0},{"$f":"J143+M143+P143+S143+V143+Y143+AB143+AE143+AH143+AK143+AN143+AQ143+AT143+AW143+AZ143+BC143+BF143+BI143+BL143+BO143+BR143+BU143+BX143+CA143","v":0},{"$f":"G143*H143","v":0},null,{"$f":"$G143*J143","v":0},null,null,{"$f":"$G143*M143","v":0},null,null,{"$f":"$G143*P143","v":0},null,null,{"$f":"$G143*S143","v":0},null,null,{"$f":"$G143*V143","v":0},null,null,{"$f":"$G143*Y143","v":0},null,null,{"$f":"$G143*AB143","v":0},null,null,{"$f":"$G143*AE143","v":0},null,null,{"$f":"$G143*AH143","v":0},null,null,{"$f":"$G143*AK143","v":0},null,null,{"$f":"$G143*AN143","v":0},null,null,{"$f":"$G143*AQ143","v":0},null,null,{"$f":"$G143*AT143","v":0},null,null,{"$f":"$G143*AW143","v":0},null,null,{"$f":"$G143*AZ143","v":0},null,null,{"$f":"$G143*BC143","v":0},null,null,{"$f":"$G143*BF143","v":0},null,null,{"$f":"$G143*BI143","v":0},null,null,{"$f":"$G143*BL143","v":0},null,null,{"$f":"$G143*BO143","v":0},null,null,{"$f":"$G143*BR143","v":0},null,null,{"$f":"$G143*BU143","v":0},null,null,{"$f":"$G143*BX143","v":0},null,null,{"$f":"$G143*CA143","v":0}]
["7.4.2",null,"B","JK     90x210 cm   - Desna ","one wing  90x210 cm - Right    ","kom/pcs",{"$f":"CENA!G135","v":0},{"$f":"J144+M144+P144+S144+V144+Y144+AB144+AE144+AH144+AK144+AN144+AQ144+AT144+AW144+AZ144+BC144+BF144+BI144+BL144+BO144+BR144+BU144+BX144+CA144","v":0},{"$f":"G144*H144","v":0},null,{"$f":"$G144*J144","v":0},null,null,0,null,null,{"$f":"$G144*P144","v":0},null,null,0,null,null,{"$f":"$G144*V144","v":0},null,null,{"$f":"$G144*Y144","v":0},null,null,{"$f":"$G144*AB144","v":0},null,null,{"$f":"$G144*AE144","v":0},null,null,{"$f":"$G144*AH144","v":0},null,null,{"$f":"$G144*AK144","v":0},null,null,{"$f":"$G144*AN144","v":0},null,null,{"$f":"$G144*AQ144","v":0},null,null,{"$f":"$G144*AT144","v":0},null,null,{"$f":"$G144*AW144","v":0},null,null,{"$f":"$G144*AZ144","v":0},null,null,{"$f":"$G144*BC144","v":0},null,null,{"$f":"$G144*BF144","v":0},null,null,{"$f":"$G144*BI144","v":0},null,null,{"$f":"$G144*BL144","v":0},null,null,{"$f":"$G144*BO144","v":0},null,null,{"$f":"$G144*BR144","v":0},null,null,{"$f":"$G144*BU144","v":0},null,null,{"$f":"$G144*BX144","v":0},null,null,{"$f":"$G144*CA144","v":0}]
["7.4.3",null,"C","DK  140x210 cm","two wings 140x210 cm","kom/pcs",{"$f":"CENA!G136","v":0},{"$f":"J145+M145+P145+S145+V145+Y145+AB145+AE145+AH145+AK145+AN145+AQ145+AT145+AW145+AZ145+BC145+BF145+BI145+BL145+BO145+BR145+BU145+BX145+CA145","v":2},{"$f":"G145*H145","v":0},null,{"$f":"$G145*J145","v":0},null,null,0,null,null,{"$f":"$G145*P145","v":0},null,null,0,null,null,{"$f":"$G145*V145","v":0},null,null,{"$f":"$G145*Y145","v":0},null,1,{"$f":"$G145*AB145","v":0},null,null,{"$f":"$G145*AE145","v":0},null,null,{"$f":"$G145*AH145","v":0},null,null,{"$f":"$G145*AK145","v":0},null,null,{"$f":"$G145*AN145","v":0},null,null,{"$f":"$G145*AQ145","v":0},null,null,{"$f":"$G145*AT145","v":0},null,null,{"$f":"$G145*AW145","v":0},null,null,{"$f":"$G145*AZ145","v":0},null,null,{"$f":"$G145*BC145","v":0},null,null,{"$f":"$G145*BF145","v":0},null,null,{"$f":"$G145*BI145","v":0},null,null,{"$f":"$G145*BL145","v":0},null,1,{"$f":"$G145*BO145","v":0},null,null,{"$f":"$G145*BR145","v":0},null,null,{"$f":"$G145*BU145","v":0},null,null,{"$f":"$G145*BX145","v":0},null,null,{"$f":"$G145*CA145","v":0}]
["7.5","S",5,"Unutrašnja vrata sa ispunom od kartonskog saća (komplet pozicija). \nširina x visina (spoljna mera futera)","Internal doors filled with cardboard honeycomb (set position)\nwidth x height (external measures footer)","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["7.5.1",null,"A","70x205 cm - Leva  (dubina štoka 0-16 cm)","70x205 cm - Left     (depth door 0-16 cm)","kom/pcs",{"$f":"CENA!G138","v":0},{"$f":"J147+M147+P147+S147+V147+Y147+AB147+AE147+AH147+AK147+AN147+AQ147+AT147+AW147+AZ147+BC147+BF147+BI147+BL147+BO147+BR147+BU147+BX147+CA147","v":0},{"$f":"G147*H147","v":0},null,{"$f":"$G147*J147","v":0},null,null,{"$f":"$G147*M147","v":0},null,null,{"$f":"$G147*P147","v":0},null,null,{"$f":"$G147*S147","v":0},null,null,{"$f":"$G147*V147","v":0},null,null,{"$f":"$G147*Y147","v":0},null,null,{"$f":"$G147*AB147","v":0},null,null,{"$f":"$G147*AE147","v":0},null,null,{"$f":"$G147*AH147","v":0},null,null,{"$f":"$G147*AK147","v":0},null,null,{"$f":"$G147*AN147","v":0},null,null,{"$f":"$G147*AQ147","v":0},null,null,{"$f":"$G147*AT147","v":0},null,null,{"$f":"$G147*AW147","v":0},null,null,{"$f":"$G147*AZ147","v":0},null,null,{"$f":"$G147*BC147","v":0},null,null,{"$f":"$G147*BF147","v":0},null,null,{"$f":"$G147*BI147","v":0},null,null,{"$f":"$G147*BL147","v":0},null,null,{"$f":"$G147*BO147","v":0},null,null,{"$f":"$G147*BR147","v":0},null,null,{"$f":"$G147*BU147","v":0},null,null,{"$f":"$G147*BX147","v":0},null,null,{"$f":"$G147*CA147","v":0}]
["7.5.2",null,"B","70x205 cm - Leva  (dubina štoka 16-30 cm)","70x205 cm - Left     (depth door 16-30 cm)","kom/pcs",{"$f":"CENA!G139","v":0},12,0,null,{"$f":"$G148*J148","v":0},null,null,0,null,1,0,null,1,0,null,null,0,null,null,0,null,null,0,null,1,0,null,null,0,null,null,0,null,1,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,1,0,null,1,0,null,1,0,null,1,0,null,1,0,null,2,0,null,1,0]
["7.5.3",null,"C","70x205 cm - Desna (dubina štoka 0-16 cm)","70x205 cm - Right   (depth door  0-16 cm)","kom/pcs",{"$f":"CENA!G140","v":0},0,0,null,{"$f":"$G149*J149","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["7.5.4",null,"D","70x205 cm - Desna (dubina štoka 16-30 cm)","70x205 cm - Right   (depth door  16-30 cm)","kom/pcs",{"$f":"CENA!G141","v":0},6,0,1,{"$f":"$G150*J150","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,1,0,null,1,0,null,1,0,null,1,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,1,0]
["7.5.5",null,"E","80x205 cm - Leva  (dubina štoka 0-16 cm)","80x205 cm - Left     (depth door 0-16 cm)","kom/pcs",{"$f":"CENA!G142","v":0},0,0,null,{"$f":"$G151*J151","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["7.5.6",null,"F","80x205 cm - Leva  (dubina štoka 16-30 cm)","80x205 cm - Left     (depth door 16-30 cm)","kom/pcs",{"$f":"CENA!G143","v":0},3,0,null,{"$f":"$G152*J152","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,2,0,null,null,0,null,null,0,null,1,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["7.5.7",null,"G","80x205 cm - Desna (dubina štoka 0-16 cm)","80x205 cm - Right   (depth door  0-16 cm)","kom/pcs",{"$f":"CENA!G144","v":0},0,0,null,{"$f":"$G153*J153","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["7.5.8",null,"H","80x205 cm - Desna (dubina štoka 16-30 cm)","80x205 cm - Right   (depth door  16-30 cm)","kom/pcs",{"$f":"CENA!G145","v":0},8,0,null,{"$f":"$G154*J154","v":0},null,null,0,null,null,0,null,1,0,null,2,0,null,null,0,null,null,0,null,null,0,null,3,0,null,null,0,null,null,0,null,null,0,null,null,0,null,1,0,null,1,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["7.5.9",null,"I","90x205 cm - Leva  (dubina štoka 0-16 cm)","90x205 cm - Left     (depth door 0-16 cm)","kom/pcs",{"$f":"CENA!G146","v":0},0,0,null,{"$f":"$G155*J155","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["7.5.10",null,"J","90x205 cm - Leva  (dubina štoka 16-30 cm)","90x205 cm - Left     (depth door 16-30 cm)","kom/pcs",{"$f":"CENA!G147","v":0},35,0,1,{"$f":"$G156*J156","v":0},null,2,0,null,2,0,null,2,0,null,3,0,null,1,0,null,null,0,null,2,0,null,1,0,null,null,0,null,1,0,null,2,0,null,null,0,null,1,0,null,null,0,null,2,0,null,3,0,null,2,0,null,1,0,null,null,0,null,1,0,null,4,0,null,2,0,null,2,0]
["7.5.11",null,"K","90x205 cm - Desna (dubina štoka 0-16 cm)","90x205 cm - Right   (depth door  0-16 cm)","kom/pcs",{"$f":"CENA!G148","v":0},0,0,null,{"$f":"$G157*J157","v":0},null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
["7.5.12",null,"L","90x205 cm - Desna (dubina štoka 16-30 cm)","90x205 cm - Right   (depth door  16-30 cm)","kom/pcs",{"$f":"CENA!G149","v":0},43,0,1,{"$f":"$G158*J158","v":0},null,null,0,null,3,0,null,1,0,null,1,0,null,2,0,null,2,0,null,2,0,null,2,0,null,null,0,null,2,0,null,3,0,null,null,0,null,2,0,null,3,0,null,4,0,null,4,0,null,1,0,null,2,0,null,null,0,null,3,0,null,1,0,null,3,0,null,1,0]
[]
["8","D",null,"OSTALA OPREMA I MATERIJAL \n","OTHER EQUIPMENT AND SUPPLIES"]
["8.1","D",1,"Jednostruki dimnjak prečnika Ф 140 mm.\nTroslojni montažni dimnjački sistem namenjen za sva ložišta i sve vrste goriva, bez ventilacije.\nSastavljen je od: dimnjačke cevi od tehničke keramike, izolacije oko cevi dimnjaka od kamene vune minimalne specifične težine 80kg/m3, spoljneg dimnjačkog plašta od lakog betona, vatrostalnog lepka u kartušama, vatrootpornih i gasnonepropusnih atestiranih troslojnih vratanaca , kondenz posude, priključaka za reviziju i ložišta, krovne ploče od staklo betona, nosača tervola i tvrdih tervol ploča za priključke, ventilacione rešetke, dilatacione rozete od nerđajućeg čelika. \nSpoljna dimenzija dimnjačkog plašta za fi14cm=32x32cm.","A single chimney diameter 140 mm.\nThree-layer prefabricated chimney system designed for all furnaces and all types of fuel, with no ventilation. It is composed of: chimney pipe of technical ceramics, pipe insulation around the chimney of stone wool minimum specific weight of 80kg/m3, external chimney mantle of lightweight concrete, refractory adhesive in cartouches, fireproof and gas impermeable certified three-layer side door, condensate pots, connectors for the audit and furnaces, roof tiles of glass concrete girders Tervola and hard tervol plate connections, ventilation grilles, rosettes expansion of stainless steel. The external dimensions of the chimney sleeve fi14cm = 32x32cm.","m1",{"$f":"CENA!G152","v":0},{"$f":"J161+M161+P161+S161+V161+Y161+AB161+AE161+AH161+AK161+AN161+AQ161+AT161+AW161+AZ161+BC161+BF161+BI161+BL161+BO161+BR161+BU161+BX161+CA161","v":24},{"$f":"G161*H161","v":0},null,{"$f":"$G161*J161","v":0},null,null,{"$f":"$G161*M161","v":0},null,null,{"$f":"$G161*P161","v":0},null,null,{"$f":"$G161*S161","v":0},null,null,{"$f":"$G161*V161","v":0},null,null,{"$f":"$G161*Y161","v":0},null,7,{"$f":"$G161*AB161","v":0},null,null,{"$f":"$G161*AE161","v":0},null,null,{"$f":"$G161*AH161","v":0},null,null,{"$f":"$G161*AK161","v":0},null,null,{"$f":"$G161*AN161","v":0},null,null,{"$f":"$G161*AQ161","v":0},null,null,{"$f":"$G161*AT161","v":0},null,null,{"$f":"$G161*AW161","v":0},null,null,{"$f":"$G161*AZ161","v":0},null,null,{"$f":"$G161*BC161","v":0},null,null,{"$f":"$G161*BF161","v":0},null,null,{"$f":"$G161*BI161","v":0},null,null,{"$f":"$G161*BL161","v":0},null,null,{"$f":"$G161*BO161","v":0},null,10,{"$f":"$G161*BR161","v":0},null,null,{"$f":"$G161*BU161","v":0},null,7,{"$f":"$G161*BX161","v":0},null,null,{"$f":"$G161*CA161","v":0}]
[]
["9","V",null,"Vodovod Kanalizacija Oprema","WATER SUPPLY AND SEWAGE"]
[null,null,null,"Vodovod","WATER SUPPLY"]
["9.1","V",1,"Vodovodne polietilenske cevi  PE 100 PN16\nza radni pritisak 16 bara (SDR 11)","Water supply polyethylene pipe PE 100 PN16\nthe working pressure of 16 bar (SDR 11)","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["9.1.1",null,"A","d25  (s min. 2,3)    - 3/4\"","d25  (s min. 2,3)    - 3/4\"","m1",{"$f":"CENA!G157","v":0},{"$f":"J166+M166+P166+S166+V166+Y166+AB166+AE166+AH166+AK166+AN166+AQ166+AT166+AW166+AZ166+BC166+BF166+BI166+BL166+BO166+BR166+BU166+BX166+CA166","v":0},{"$f":"G166*H166","v":0},null,{"$f":"$G166*J166","v":0},null,null,{"$f":"$G166*M166","v":0},null,null,{"$f":"$G166*P166","v":0},null,null,{"$f":"$G166*S166","v":0},null,null,{"$f":"$G166*V166","v":0},null,null,{"$f":"$G166*Y166","v":0},null,null,{"$f":"$G166*AB166","v":0},null,null,{"$f":"$G166*AE166","v":0},null,null,{"$f":"$G166*AH166","v":0},null,null,{"$f":"$G166*AK166","v":0},null,null,{"$f":"$G166*AN166","v":0},null,null,{"$f":"$G166*AQ166","v":0},null,null,{"$f":"$G166*AT166","v":0},null,null,{"$f":"$G166*AW166","v":0},null,null,{"$f":"$G166*AZ166","v":0},null,null,{"$f":"$G166*BC166","v":0},null,null,{"$f":"$G166*BF166","v":0},null,null,{"$f":"$G166*BI166","v":0},null,null,{"$f":"$G166*BL166","v":0},null,null,{"$f":"$G166*BO166","v":0},null,null,{"$f":"$G166*BR166","v":0},null,null,{"$f":"$G166*BU166","v":0},null,null,{"$f":"$G166*BX166","v":0},null,null,{"$f":"$G166*CA166","v":0}]
["9.1.2",null,"B","d32  (s min. 3,0)   -       1\"","d32  (s min. 3,0)   -       1\"","m1",{"$f":"CENA!G158","v":0},{"$f":"J167+M167+P167+S167+V167+Y167+AB167+AE167+AH167+AK167+AN167+AQ167+AT167+AW167+AZ167+BC167+BF167+BI167+BL167+BO167+BR167+BU167+BX167+CA167","v":0},{"$f":"G167*H167","v":0},null,{"$f":"$G167*J167","v":0},null,null,0,null,null,{"$f":"$G167*P167","v":0},null,null,{"$f":"$G167*S167","v":0},null,null,{"$f":"$G167*V167","v":0},null,null,{"$f":"$G167*Y167","v":0},null,null,{"$f":"$G167*AB167","v":0},null,null,{"$f":"$G167*AE167","v":0},null,null,{"$f":"$G167*AH167","v":0},null,null,{"$f":"$G167*AK167","v":0},null,null,{"$f":"$G167*AN167","v":0},null,null,{"$f":"$G167*AQ167","v":0},null,null,{"$f":"$G167*AT167","v":0},null,null,{"$f":"$G167*AW167","v":0},null,null,{"$f":"$G167*AZ167","v":0},null,null,{"$f":"$G167*BC167","v":0},null,null,{"$f":"$G167*BF167","v":0},null,null,{"$f":"$G167*BI167","v":0},null,null,{"$f":"$G167*BL167","v":0},null,null,{"$f":"$G167*BO167","v":0},null,null,{"$f":"$G167*BR167","v":0},null,null,{"$f":"$G167*BU167","v":0},null,null,{"$f":"$G167*BX167","v":0},null,null,{"$f":"$G167*CA167","v":0}]
["9.1.3",null,"C","d40  (s min. 3,7)   -  5/4\"","d40  (s min. 3,7)   -  5/4\"","m1",{"$f":"CENA!G159","v":0},{"$f":"J168+M168+P168+S168+V168+Y168+AB168+AE168+AH168+AK168+AN168+AQ168+AT168+AW168+AZ168+BC168+BF168+BI168+BL168+BO168+BR168+BU168+BX168+CA168","v":0},{"$f":"G168*H168","v":0},null,{"$f":"$G168*J168","v":0},null,null,0,null,null,{"$f":"$G168*P168","v":0},null,null,{"$f":"$G168*S168","v":0},null,null,{"$f":"$G168*V168","v":0},null,null,{"$f":"$G168*Y168","v":0},null,null,{"$f":"$G168*AB168","v":0},null,null,{"$f":"$G168*AE168","v":0},null,null,{"$f":"$G168*AH168","v":0},null,null,{"$f":"$G168*AK168","v":0},null,null,{"$f":"$G168*AN168","v":0},null,null,{"$f":"$G168*AQ168","v":0},null,null,{"$f":"$G168*AT168","v":0},null,null,{"$f":"$G168*AW168","v":0},null,null,{"$f":"$G168*AZ168","v":0},null,null,{"$f":"$G168*BC168","v":0},null,null,{"$f":"$G168*BF168","v":0},null,null,{"$f":"$G168*BI168","v":0},null,null,{"$f":"$G168*BL168","v":0},null,null,{"$f":"$G168*BO168","v":0},null,null,{"$f":"$G168*BR168","v":0},null,null,{"$f":"$G168*BU168","v":0},null,null,{"$f":"$G168*BX168","v":0},null,null,{"$f":"$G168*CA168","v":0}]
["9.2","V",2,"Vodovodne cevi  PP-R 80 PN20 \nza radni pritisak 20 bara, bele ili zelene boje\n(materijal: polipropilen-random kapolimer)","Water pipe PP-R 80 PN20 \nthe working pressure of 20 bar, white or green \n(material: polypropylene random kapolimer)","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["9.2.1",null,"B","d20  (s min.   3,4)    - 1/2\"","d20  (s min.   3,4)    - 1/2\"","m1",{"$f":"CENA!G161","v":0},{"$f":"J170+M170+P170+S170+V170+Y170+AB170+AE170+AH170+AK170+AN170+AQ170+AT170+AW170+AZ170+BC170+BF170+BI170+BL170+BO170+BR170+BU170+BX170+CA170","v":515},{"$f":"G170*H170","v":0},30,{"$f":"$G170*J170","v":0},null,null,{"$f":"$G170*M170","v":0},null,30,{"$f":"$G170*P170","v":0},null,null,{"$f":"$G170*S170","v":0},null,40,{"$f":"$G170*V170","v":0},null,30,{"$f":"$G170*Y170","v":0},null,null,{"$f":"$G170*AB170","v":0},null,40,{"$f":"$G170*AE170","v":0},null,40,{"$f":"$G170*AH170","v":0},null,null,{"$f":"$G170*AK170","v":0},null,40,{"$f":"$G170*AN170","v":0},null,30,{"$f":"$G170*AQ170","v":0},null,30,{"$f":"$G170*AT170","v":0},null,null,{"$f":"$G170*AW170","v":0},null,30,{"$f":"$G170*AZ170","v":0},null,35,{"$f":"$G170*BC170","v":0},null,30,{"$f":"$G170*BF170","v":0},null,30,{"$f":"$G170*BI170","v":0},null,null,{"$f":"$G170*BL170","v":0},null,40,{"$f":"$G170*BO170","v":0},null,40,{"$f":"$G170*BR170","v":0},null,null,{"$f":"$G170*BU170","v":0},null,null,{"$f":"$G170*BX170","v":0},null,null,{"$f":"$G170*CA170","v":0}]
["9.2.2",null,"C","d25  (s min.   4,2)    - 3/4\"","d25  (s min.   4,2)    - 3/4\"","m1",{"$f":"CENA!G162","v":0},{"$f":"J171+M171+P171+S171+V171+Y171+AB171+AE171+AH171+AK171+AN171+AQ171+AT171+AW171+AZ171+BC171+BF171+BI171+BL171+BO171+BR171+BU171+BX171+CA171","v":0},{"$f":"G171*H171","v":0},null,{"$f":"$G171*J171","v":0},null,null,0,null,null,{"$f":"$G171*P171","v":0},null,null,{"$f":"$G171*S171","v":0},null,null,{"$f":"$G171*V171","v":0},null,null,{"$f":"$G171*Y171","v":0},null,null,{"$f":"$G171*AB171","v":0},null,null,{"$f":"$G171*AE171","v":0},null,null,{"$f":"$G171*AH171","v":0},null,null,{"$f":"$G171*AK171","v":0},null,null,{"$f":"$G171*AN171","v":0},null,null,{"$f":"$G171*AQ171","v":0},null,null,{"$f":"$G171*AT171","v":0},null,null,{"$f":"$G171*AW171","v":0},null,null,{"$f":"$G171*AZ171","v":0},null,null,{"$f":"$G171*BC171","v":0},null,null,{"$f":"$G171*BF171","v":0},null,null,{"$f":"$G171*BI171","v":0},null,null,{"$f":"$G171*BL171","v":0},null,null,{"$f":"$G171*BO171","v":0},null,null,{"$f":"$G171*BR171","v":0},null,null,{"$f":"$G171*BU171","v":0},null,null,{"$f":"$G171*BX171","v":0},null,null,{"$f":"$G171*CA171","v":0}]
["9.2.3",null,"D","d32  (s min.   5,4)    -     1\"","d32  (s min.   5,4)    -     1\"","m1",{"$f":"CENA!G163","v":0},{"$f":"J172+M172+P172+S172+V172+Y172+AB172+AE172+AH172+AK172+AN172+AQ172+AT172+AW172+AZ172+BC172+BF172+BI172+BL172+BO172+BR172+BU172+BX172+CA172","v":20},{"$f":"G172*H172","v":0},null,{"$f":"$G172*J172","v":0},null,20,0,null,null,{"$f":"$G172*P172","v":0},null,null,{"$f":"$G172*S172","v":0},null,null,{"$f":"$G172*V172","v":0},null,null,{"$f":"$G172*Y172","v":0},null,null,{"$f":"$G172*AB172","v":0},null,null,{"$f":"$G172*AE172","v":0},null,null,{"$f":"$G172*AH172","v":0},null,null,{"$f":"$G172*AK172","v":0},null,null,{"$f":"$G172*AN172","v":0},null,null,{"$f":"$G172*AQ172","v":0},null,null,{"$f":"$G172*AT172","v":0},null,null,{"$f":"$G172*AW172","v":0},null,null,{"$f":"$G172*AZ172","v":0},null,null,{"$f":"$G172*BC172","v":0},null,null,{"$f":"$G172*BF172","v":0},null,null,{"$f":"$G172*BI172","v":0},null,null,{"$f":"$G172*BL172","v":0},null,null,{"$f":"$G172*BO172","v":0},null,null,{"$f":"$G172*BR172","v":0},null,null,{"$f":"$G172*BU172","v":0},null,null,{"$f":"$G172*BX172","v":0},null,null,{"$f":"$G172*CA172","v":0}]
["9.3","V",3,"Vodomer \nsa prirubnicama, holenderima i pripadajućom opremom za montažu, za pritisak do 16 bara","water gauge\nflanges, unions and associated equipment for assembly, for pressure up to 16 bar","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["9.3.1",null,"A","horizontalni 3/4\"    ","Horizontal 3/4\"    ","kom/pcs",{"$f":"CENA!G165","v":0},{"$f":"J174+M174+P174+S174+V174+Y174+AB174+AE174+AH174+AK174+AN174+AQ174+AT174+AW174+AZ174+BC174+BF174+BI174+BL174+BO174+BR174+BU174+BX174+CA174","v":0},{"$f":"G174*H174","v":0},null,{"$f":"$G174*J174","v":0},null,null,{"$f":"$G174*M174","v":0},null,null,{"$f":"$G174*P174","v":0},null,null,{"$f":"$G174*S174","v":0},null,null,{"$f":"$G174*V174","v":0},null,null,{"$f":"$G174*Y174","v":0},null,null,{"$f":"$G174*AB174","v":0},null,null,{"$f":"$G174*AE174","v":0},null,null,{"$f":"$G174*AH174","v":0},null,null,{"$f":"$G174*AK174","v":0},null,null,{"$f":"$G174*AN174","v":0},null,null,{"$f":"$G174*AQ174","v":0},null,null,{"$f":"$G174*AT174","v":0},null,null,{"$f":"$G174*AW174","v":0},null,null,{"$f":"$G174*AZ174","v":0},null,null,{"$f":"$G174*BC174","v":0},null,null,{"$f":"$G174*BF174","v":0},null,null,{"$f":"$G174*BI174","v":0},null,null,{"$f":"$G174*BL174","v":0},null,null,{"$f":"$G174*BO174","v":0},null,null,{"$f":"$G174*BR174","v":0},null,null,{"$f":"$G174*BU174","v":0},null,null,{"$f":"$G174*BX174","v":0},null,null,{"$f":"$G174*CA174","v":0}]
["9.3.2",null,"B","horizontalni     1\"    ","Horizontal     1\"    ","kom/pcs",{"$f":"CENA!G166","v":0},{"$f":"J175+M175+P175+S175+V175+Y175+AB175+AE175+AH175+AK175+AN175+AQ175+AT175+AW175+AZ175+BC175+BF175+BI175+BL175+BO175+BR175+BU175+BX175+CA175","v":0},{"$f":"G175*H175","v":0},null,{"$f":"$G175*J175","v":0},null,null,0,null,null,{"$f":"$G175*P175","v":0},null,null,{"$f":"$G175*S175","v":0},null,null,{"$f":"$G175*V175","v":0},null,null,{"$f":"$G175*Y175","v":0},null,null,{"$f":"$G175*AB175","v":0},null,null,{"$f":"$G175*AE175","v":0},null,null,{"$f":"$G175*AH175","v":0},null,null,{"$f":"$G175*AK175","v":0},null,null,{"$f":"$G175*AN175","v":0},null,null,{"$f":"$G175*AQ175","v":0},null,null,{"$f":"$G175*AT175","v":0},null,null,{"$f":"$G175*AW175","v":0},null,null,{"$f":"$G175*AZ175","v":0},null,null,{"$f":"$G175*BC175","v":0},null,null,{"$f":"$G175*BF175","v":0},null,null,{"$f":"$G175*BI175","v":0},null,null,{"$f":"$G175*BL175","v":0},null,null,{"$f":"$G175*BO175","v":0},null,null,{"$f":"$G175*BR175","v":0},null,null,{"$f":"$G175*BU175","v":0},null,null,{"$f":"$G175*BX175","v":0},null,null,{"$f":"$G175*CA175","v":0}]
["9.3.3",null,"C","horizontalni 5/4\"","Horizontal 5/4\"","kom/pcs",{"$f":"CENA!G167","v":0},{"$f":"J176+M176+P176+S176+V176+Y176+AB176+AE176+AH176+AK176+AN176+AQ176+AT176+AW176+AZ176+BC176+BF176+BI176+BL176+BO176+BR176+BU176+BX176+CA176","v":0},{"$f":"G176*H176","v":0},null,{"$f":"$G176*J176","v":0},null,null,0,null,null,{"$f":"$G176*P176","v":0},null,null,{"$f":"$G176*S176","v":0},null,null,{"$f":"$G176*V176","v":0},null,null,{"$f":"$G176*Y176","v":0},null,null,{"$f":"$G176*AB176","v":0},null,null,{"$f":"$G176*AE176","v":0},null,null,{"$f":"$G176*AH176","v":0},null,null,{"$f":"$G176*AK176","v":0},null,null,{"$f":"$G176*AN176","v":0},null,null,{"$f":"$G176*AQ176","v":0},null,null,{"$f":"$G176*AT176","v":0},null,null,{"$f":"$G176*AW176","v":0},null,null,{"$f":"$G176*AZ176","v":0},null,null,{"$f":"$G176*BC176","v":0},null,null,{"$f":"$G176*BF176","v":0},null,null,{"$f":"$G176*BI176","v":0},null,null,{"$f":"$G176*BL176","v":0},null,null,{"$f":"$G176*BO176","v":0},null,null,{"$f":"$G176*BR176","v":0},null,null,{"$f":"$G176*BU176","v":0},null,null,{"$f":"$G176*BX176","v":0},null,null,{"$f":"$G176*CA176","v":0}]
["9.4","V",4,"Ravni propusni ventil sa ogrankom za pražnjenje","Skip straight valve with a branch drain","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["9.4.1",null,"A","d25  (s min. 2,3)    - 3/4\"","d25  (s min. 2,3)    - 3/4\"","kom/pcs",{"$f":"CENA!G169","v":0},{"$f":"J178+M178+P178+S178+V178+Y178+AB178+AE178+AH178+AK178+AN178+AQ178+AT178+AW178+AZ178+BC178+BF178+BI178+BL178+BO178+BR178+BU178+BX178+CA178","v":0},{"$f":"G178*H178","v":0},null,{"$f":"$G178*J178","v":0},null,null,{"$f":"$G178*M178","v":0},null,null,{"$f":"$G178*P178","v":0},null,null,{"$f":"$G178*S178","v":0},null,null,{"$f":"$G178*V178","v":0},null,null,{"$f":"$G178*Y178","v":0},null,null,{"$f":"$G178*AB178","v":0},null,null,{"$f":"$G178*AE178","v":0},null,null,{"$f":"$G178*AH178","v":0},null,null,{"$f":"$G178*AK178","v":0},null,null,{"$f":"$G178*AN178","v":0},null,null,{"$f":"$G178*AQ178","v":0},null,null,{"$f":"$G178*AT178","v":0},null,null,{"$f":"$G178*AW178","v":0},null,null,{"$f":"$G178*AZ178","v":0},null,null,{"$f":"$G178*BC178","v":0},null,null,{"$f":"$G178*BF178","v":0},null,null,{"$f":"$G178*BI178","v":0},null,null,{"$f":"$G178*BL178","v":0},null,null,{"$f":"$G178*BO178","v":0},null,null,{"$f":"$G178*BR178","v":0},null,null,{"$f":"$G178*BU178","v":0},null,null,{"$f":"$G178*BX178","v":0},null,null,{"$f":"$G178*CA178","v":0}]
["9.4.2",null,"B","d32  (s min. 3,0)   -       1\"","d32  (s min. 3,0)   -       1\"","kom/pcs",{"$f":"CENA!G170","v":0},{"$f":"J179+M179+P179+S179+V179+Y179+AB179+AE179+AH179+AK179+AN179+AQ179+AT179+AW179+AZ179+BC179+BF179+BI179+BL179+BO179+BR179+BU179+BX179+CA179","v":0},{"$f":"G179*H179","v":0},null,{"$f":"$G179*J179","v":0},null,null,0,null,null,{"$f":"$G179*P179","v":0},null,null,{"$f":"$G179*S179","v":0},null,null,{"$f":"$G179*V179","v":0},null,null,{"$f":"$G179*Y179","v":0},null,null,{"$f":"$G179*AB179","v":0},null,null,{"$f":"$G179*AE179","v":0},null,null,{"$f":"$G179*AH179","v":0},null,null,{"$f":"$G179*AK179","v":0},null,null,{"$f":"$G179*AN179","v":0},null,null,{"$f":"$G179*AQ179","v":0},null,null,{"$f":"$G179*AT179","v":0},null,null,{"$f":"$G179*AW179","v":0},null,null,{"$f":"$G179*AZ179","v":0},null,null,{"$f":"$G179*BC179","v":0},null,null,{"$f":"$G179*BF179","v":0},null,null,{"$f":"$G179*BI179","v":0},null,null,{"$f":"$G179*BL179","v":0},null,null,{"$f":"$G179*BO179","v":0},null,null,{"$f":"$G179*BR179","v":0},null,null,{"$f":"$G179*BU179","v":0},null,null,{"$f":"$G179*BX179","v":0},null,null,{"$f":"$G179*CA179","v":0}]
["9.5","V",5,"Propusni ventil za uzidanje sa kapom ","Gate valve for the wall with cap","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["9.5.1",null,"A","d20  (s min.   3,4)    - 1/2\"","d20  (s min.   3,4)    - 1/2\"","kom/pcs",{"$f":"CENA!G172","v":0},{"$f":"J181+M181+P181+S181+V181+Y181+AB181+AE181+AH181+AK181+AN181+AQ181+AT181+AW181+AZ181+BC181+BF181+BI181+BL181+BO181+BR181+BU181+BX181+CA181","v":74},{"$f":"G181*H181","v":0},5,{"$f":"$G181*J181","v":0},null,null,{"$f":"$G181*M181","v":0},null,5,{"$f":"$G181*P181","v":0},null,null,{"$f":"$G181*S181","v":0},null,5,{"$f":"$G181*V181","v":0},null,5,{"$f":"$G181*Y181","v":0},null,null,{"$f":"$G181*AB181","v":0},null,5,{"$f":"$G181*AE181","v":0},null,5,{"$f":"$G181*AH181","v":0},null,null,{"$f":"$G181*AK181","v":0},null,5,{"$f":"$G181*AN181","v":0},null,5,{"$f":"$G181*AQ181","v":0},null,5,{"$f":"$G181*AT181","v":0},null,null,{"$f":"$G181*AW181","v":0},null,5,{"$f":"$G181*AZ181","v":0},null,4,{"$f":"$G181*BC181","v":0},null,5,{"$f":"$G181*BF181","v":0},null,5,{"$f":"$G181*BI181","v":0},null,null,{"$f":"$G181*BL181","v":0},null,5,{"$f":"$G181*BO181","v":0},null,5,{"$f":"$G181*BR181","v":0},null,null,{"$f":"$G181*BU181","v":0},null,null,{"$f":"$G181*BX181","v":0},null,null,{"$f":"$G181*CA181","v":0}]
["9.5.2",null,"B","d25  (s min.   4,2)    - 3/4\"","d25  (s min.   4,2)    - 3/4\"","kom/pcs",{"$f":"CENA!G173","v":0},{"$f":"J182+M182+P182+S182+V182+Y182+AB182+AE182+AH182+AK182+AN182+AQ182+AT182+AW182+AZ182+BC182+BF182+BI182+BL182+BO182+BR182+BU182+BX182+CA182","v":0},{"$f":"G182*H182","v":0},null,{"$f":"$G182*J182","v":0},null,null,0,null,null,{"$f":"$G182*P182","v":0},null,null,{"$f":"$G182*S182","v":0},null,null,{"$f":"$G182*V182","v":0},null,null,{"$f":"$G182*Y182","v":0},null,null,{"$f":"$G182*AB182","v":0},null,null,{"$f":"$G182*AE182","v":0},null,null,{"$f":"$G182*AH182","v":0},null,null,{"$f":"$G182*AK182","v":0},null,null,{"$f":"$G182*AN182","v":0},null,null,{"$f":"$G182*AQ182","v":0},null,null,{"$f":"$G182*AT182","v":0},null,null,{"$f":"$G182*AW182","v":0},null,null,{"$f":"$G182*AZ182","v":0},null,null,{"$f":"$G182*BC182","v":0},null,null,{"$f":"$G182*BF182","v":0},null,null,{"$f":"$G182*BI182","v":0},null,null,{"$f":"$G182*BL182","v":0},null,null,{"$f":"$G182*BO182","v":0},null,null,{"$f":"$G182*BR182","v":0},null,null,{"$f":"$G182*BU182","v":0},null,null,{"$f":"$G182*BX182","v":0},null,null,{"$f":"$G182*CA182","v":0}]
["9.5.3",null,"C","d32  (s min. 3,0)   -       1\"","d32  (s min. 3,0)   -       1\"","kom/pcs",{"$f":"CENA!G174","v":0},{"$f":"J183+M183+P183+S183+V183+Y183+AB183+AE183+AH183+AK183+AN183+AQ183+AT183+AW183+AZ183+BC183+BF183+BI183+BL183+BO183+BR183+BU183+BX183+CA183","v":0},{"$f":"G183*H183","v":0},null,{"$f":"$G183*J183","v":0},null,null,0,null,null,{"$f":"$G183*P183","v":0},null,null,{"$f":"$G183*S183","v":0},null,null,{"$f":"$G183*V183","v":0},null,null,{"$f":"$G183*Y183","v":0},null,null,{"$f":"$G183*AB183","v":0},null,null,{"$f":"$G183*AE183","v":0},null,null,{"$f":"$G183*AH183","v":0},null,null,{"$f":"$G183*AK183","v":0},null,null,{"$f":"$G183*AN183","v":0},null,null,{"$f":"$G183*AQ183","v":0},null,null,{"$f":"$G183*AT183","v":0},null,null,{"$f":"$G183*AW183","v":0},null,null,{"$f":"$G183*AZ183","v":0},null,null,{"$f":"$G183*BC183","v":0},null,null,{"$f":"$G183*BF183","v":0},null,null,{"$f":"$G183*BI183","v":0},null,null,{"$f":"$G183*BL183","v":0},null,null,{"$f":"$G183*BO183","v":0},null,null,{"$f":"$G183*BR183","v":0},null,null,{"$f":"$G183*BU183","v":0},null,null,{"$f":"$G183*BX183","v":0},null,null,{"$f":"$G183*CA183","v":0}]
["9.6","V",6,"Ugaoni \"EK\" sa kapom","Angle valve \"EK\" with cap","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["9.6.1",null,"A","d20  (s min.   3,4)    - 1/2\"","d20  (s min.   3,4)    - 1/2\"","kom/pcs",{"$f":"CENA!G176","v":0},{"$f":"J185+M185+P185+S185+V185+Y185+AB185+AE185+AH185+AK185+AN185+AQ185+AT185+AW185+AZ185+BC185+BF185+BI185+BL185+BO185+BR185+BU185+BX185+CA185","v":74},{"$f":"G185*H185","v":0},5,{"$f":"$G185*J185","v":0},null,null,{"$f":"$G185*M185","v":0},null,5,{"$f":"$G185*P185","v":0},null,null,{"$f":"$G185*S185","v":0},null,5,{"$f":"$G185*V185","v":0},null,5,{"$f":"$G185*Y185","v":0},null,null,{"$f":"$G185*AB185","v":0},null,5,{"$f":"$G185*AE185","v":0},null,5,{"$f":"$G185*AH185","v":0},null,null,{"$f":"$G185*AK185","v":0},null,5,{"$f":"$G185*AN185","v":0},null,5,{"$f":"$G185*AQ185","v":0},null,5,{"$f":"$G185*AT185","v":0},null,null,{"$f":"$G185*AW185","v":0},null,5,{"$f":"$G185*AZ185","v":0},null,4,{"$f":"$G185*BC185","v":0},null,5,{"$f":"$G185*BF185","v":0},null,5,{"$f":"$G185*BI185","v":0},null,null,{"$f":"$G185*BL185","v":0},null,5,{"$f":"$G185*BO185","v":0},null,5,{"$f":"$G185*BR185","v":0},null,null,{"$f":"$G185*BU185","v":0},null,null,{"$f":"$G185*BX185","v":0},null,null,{"$f":"$G185*CA185","v":0}]
["9.7","V",7,"Termička izolacija vodovodnih cevi  -tipa plamaflex ISO ili sl.","Thermal insulation of water pipes-type PLAMAFLEX ISO etc..","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["9.7.1",null,"B","d20   (22/9)   - 1/2\"","d20   (22/9)   - 1/2\"","m1",{"$f":"CENA!G178","v":0},{"$f":"J187+M187+P187+S187+V187+Y187+AB187+AE187+AH187+AK187+AN187+AQ187+AT187+AW187+AZ187+BC187+BF187+BI187+BL187+BO187+BR187+BU187+BX187+CA187","v":0},{"$f":"G187*H187","v":0},null,{"$f":"$G187*J187","v":0},null,null,{"$f":"$G187*M187","v":0},null,null,{"$f":"$G187*P187","v":0},null,null,{"$f":"$G187*S187","v":0},null,null,{"$f":"$G187*V187","v":0},null,null,{"$f":"$G187*Y187","v":0},null,null,{"$f":"$G187*AB187","v":0},null,null,{"$f":"$G187*AE187","v":0},null,null,{"$f":"$G187*AH187","v":0},null,null,{"$f":"$G187*AK187","v":0},null,null,{"$f":"$G187*AN187","v":0},null,null,{"$f":"$G187*AQ187","v":0},null,null,{"$f":"$G187*AT187","v":0},null,null,{"$f":"$G187*AW187","v":0},null,null,{"$f":"$G187*AZ187","v":0},null,null,{"$f":"$G187*BC187","v":0},null,null,{"$f":"$G187*BF187","v":0},null,null,{"$f":"$G187*BI187","v":0},null,null,{"$f":"$G187*BL187","v":0},null,null,{"$f":"$G187*BO187","v":0},null,null,{"$f":"$G187*BR187","v":0},null,null,{"$f":"$G187*BU187","v":0},null,null,{"$f":"$G187*BX187","v":0},null,null,{"$f":"$G187*CA187","v":0}]
["9.7.2",null,"C","d25   (25/9) - 3/4\"","d25   (25/9) - 3/4\"","m1",{"$f":"CENA!G179","v":0},{"$f":"J188+M188+P188+S188+V188+Y188+AB188+AE188+AH188+AK188+AN188+AQ188+AT188+AW188+AZ188+BC188+BF188+BI188+BL188+BO188+BR188+BU188+BX188+CA188","v":0},{"$f":"G188*H188","v":0},null,{"$f":"$G188*J188","v":0},null,null,0,null,null,{"$f":"$G188*P188","v":0},null,null,{"$f":"$G188*S188","v":0},null,null,{"$f":"$G188*V188","v":0},null,null,{"$f":"$G188*Y188","v":0},null,null,{"$f":"$G188*AB188","v":0},null,null,{"$f":"$G188*AE188","v":0},null,null,{"$f":"$G188*AH188","v":0},null,null,{"$f":"$G188*AK188","v":0},null,null,{"$f":"$G188*AN188","v":0},null,null,{"$f":"$G188*AQ188","v":0},null,null,{"$f":"$G188*AT188","v":0},null,null,{"$f":"$G188*AW188","v":0},null,null,{"$f":"$G188*AZ188","v":0},null,null,{"$f":"$G188*BC188","v":0},null,null,{"$f":"$G188*BF188","v":0},null,null,{"$f":"$G188*BI188","v":0},null,null,{"$f":"$G188*BL188","v":0},null,null,{"$f":"$G188*BO188","v":0},null,null,{"$f":"$G188*BR188","v":0},null,null,{"$f":"$G188*BU188","v":0},null,null,{"$f":"$G188*BX188","v":0},null,null,{"$f":"$G188*CA188","v":0}]
["9.7.3",null,"D","d32   (35/9)-     1\"","d32   (35/9)-     1\"","m1",{"$f":"CENA!G180","v":0},{"$f":"J189+M189+P189+S189+V189+Y189+AB189+AE189+AH189+AK189+AN189+AQ189+AT189+AW189+AZ189+BC189+BF189+BI189+BL189+BO189+BR189+BU189+BX189+CA189","v":0},{"$f":"G189*H189","v":0},null,{"$f":"$G189*J189","v":0},null,null,0,null,null,{"$f":"$G189*P189","v":0},null,null,{"$f":"$G189*S189","v":0},null,null,{"$f":"$G189*V189","v":0},null,null,{"$f":"$G189*Y189","v":0},null,null,{"$f":"$G189*AB189","v":0},null,null,{"$f":"$G189*AE189","v":0},null,null,{"$f":"$G189*AH189","v":0},null,null,{"$f":"$G189*AK189","v":0},null,null,{"$f":"$G189*AN189","v":0},null,null,{"$f":"$G189*AQ189","v":0},null,null,{"$f":"$G189*AT189","v":0},null,null,{"$f":"$G189*AW189","v":0},null,null,{"$f":"$G189*AZ189","v":0},null,null,{"$f":"$G189*BC189","v":0},null,null,{"$f":"$G189*BF189","v":0},null,null,{"$f":"$G189*BI189","v":0},null,null,{"$f":"$G189*BL189","v":0},null,null,{"$f":"$G189*BO189","v":0},null,null,{"$f":"$G189*BR189","v":0},null,null,{"$f":"$G189*BU189","v":0},null,null,{"$f":"$G189*BX189","v":0},null,null,{"$f":"$G189*CA189","v":0}]
[null,null,null,"Kanalizacija","SEWAGE"]
["9.8","V",8,"PVC kanalizacione cevi SDR 41 / SN4 / PN5\nza spoljni razvod, kućna i ulična kanalizacija","PVC sewer pipe SDR 41 / CH4 / PN5\nfor external distribution, household and street sewage","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["9.8.1",null,"A","d110 (s min.   3,2)    dužina 6,0m","d110 (s min.   3,2)    length 6,0m","kom/pcs",{"$f":"CENA!G183","v":0},{"$f":"J192+M192+P192+S192+V192+Y192+AB192+AE192+AH192+AK192+AN192+AQ192+AT192+AW192+AZ192+BC192+BF192+BI192+BL192+BO192+BR192+BU192+BX192+CA192","v":0},{"$f":"G192*H192","v":0},null,{"$f":"$G192*J192","v":0},null,null,{"$f":"$G192*M192","v":0},null,null,{"$f":"$G192*P192","v":0},null,null,{"$f":"$G192*S192","v":0},null,null,{"$f":"$G192*V192","v":0},null,null,{"$f":"$G192*Y192","v":0},null,null,{"$f":"$G192*AB192","v":0},null,null,{"$f":"$G192*AE192","v":0},null,null,{"$f":"$G192*AH192","v":0},null,null,{"$f":"$G192*AK192","v":0},null,null,{"$f":"$G192*AN192","v":0},null,null,{"$f":"$G192*AQ192","v":0},null,null,{"$f":"$G192*AT192","v":0},null,null,{"$f":"$G192*AW192","v":0},null,null,{"$f":"$G192*AZ192","v":0},null,null,{"$f":"$G192*BC192","v":0},null,null,{"$f":"$G192*BF192","v":0},null,null,{"$f":"$G192*BI192","v":0},null,null,{"$f":"$G192*BL192","v":0},null,null,{"$f":"$G192*BO192","v":0},null,null,{"$f":"$G192*BR192","v":0},null,null,{"$f":"$G192*BU192","v":0},null,null,{"$f":"$G192*BX192","v":0},null,null,{"$f":"$G192*CA192","v":0}]
["9.8.2",null,"B","d160 (s min.   4,0)    dužina 6,0m","d160 (s min.   4,0)    length 6,0m","kom/pcs",{"$f":"CENA!G184","v":0},{"$f":"J193+M193+P193+S193+V193+Y193+AB193+AE193+AH193+AK193+AN193+AQ193+AT193+AW193+AZ193+BC193+BF193+BI193+BL193+BO193+BR193+BU193+BX193+CA193","v":0},{"$f":"G193*H193","v":0},null,{"$f":"$G193*J193","v":0},null,null,0,null,null,{"$f":"$G193*P193","v":0},null,null,{"$f":"$G193*S193","v":0},null,null,{"$f":"$G193*V193","v":0},null,null,{"$f":"$G193*Y193","v":0},null,null,{"$f":"$G193*AB193","v":0},null,null,{"$f":"$G193*AE193","v":0},null,null,{"$f":"$G193*AH193","v":0},null,null,{"$f":"$G193*AK193","v":0},null,null,{"$f":"$G193*AN193","v":0},null,null,{"$f":"$G193*AQ193","v":0},null,null,{"$f":"$G193*AT193","v":0},null,null,{"$f":"$G193*AW193","v":0},null,null,{"$f":"$G193*AZ193","v":0},null,null,{"$f":"$G193*BC193","v":0},null,null,{"$f":"$G193*BF193","v":0},null,null,{"$f":"$G193*BI193","v":0},null,null,{"$f":"$G193*BL193","v":0},null,null,{"$f":"$G193*BO193","v":0},null,null,{"$f":"$G193*BR193","v":0},null,null,{"$f":"$G193*BU193","v":0},null,null,{"$f":"$G193*BX193","v":0},null,null,{"$f":"$G193*CA193","v":0}]
["9.9","V",9,"Plastične PP cevi SDR 51 / SN2 / PN4\nza unutrašnji (kućni) razvod, kućna kanalizacija","Plastic PP pipes SDR 51 / SN2 / PN4\nfor internal (home) distribution, household sewage","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["9.9.1",null,"A","d50     (s min.   1,8)    dužina 3,0m","d50     (s min.   1,8)    length 3,0m","kom/pcs",{"$f":"CENA!G186","v":0},{"$f":"J195+M195+P195+S195+V195+Y195+AB195+AE195+AH195+AK195+AN195+AQ195+AT195+AW195+AZ195+BC195+BF195+BI195+BL195+BO195+BR195+BU195+BX195+CA195","v":78},{"$f":"G195*H195","v":0},5,{"$f":"$G195*J195","v":0},null,null,{"$f":"$G195*M195","v":0},null,5,{"$f":"$G195*P195","v":0},null,null,{"$f":"$G195*S195","v":0},null,5,{"$f":"$G195*V195","v":0},null,5,{"$f":"$G195*Y195","v":0},null,null,{"$f":"$G195*AB195","v":0},null,5,{"$f":"$G195*AE195","v":0},null,5,{"$f":"$G195*AH195","v":0},null,null,{"$f":"$G195*AK195","v":0},null,8,{"$f":"$G195*AN195","v":0},null,5,{"$f":"$G195*AQ195","v":0},null,5,{"$f":"$G195*AT195","v":0},null,null,{"$f":"$G195*AW195","v":0},null,5,{"$f":"$G195*AZ195","v":0},null,5,{"$f":"$G195*BC195","v":0},null,5,{"$f":"$G195*BF195","v":0},null,5,{"$f":"$G195*BI195","v":0},null,null,{"$f":"$G195*BL195","v":0},null,5,{"$f":"$G195*BO195","v":0},null,5,{"$f":"$G195*BR195","v":0},null,null,{"$f":"$G195*BU195","v":0},null,null,{"$f":"$G195*BX195","v":0},null,null,{"$f":"$G195*CA195","v":0}]
["9.9.2",null,"B","d75     (s min.   1,9)    dužina 3,0m","d75     (s min.   1,9)    length 3,0m","kom/pcs",{"$f":"CENA!G187","v":0},{"$f":"J196+M196+P196+S196+V196+Y196+AB196+AE196+AH196+AK196+AN196+AQ196+AT196+AW196+AZ196+BC196+BF196+BI196+BL196+BO196+BR196+BU196+BX196+CA196","v":0},{"$f":"G196*H196","v":0},null,{"$f":"$G196*J196","v":0},null,null,0,null,null,{"$f":"$G196*P196","v":0},null,null,{"$f":"$G196*S196","v":0},null,null,{"$f":"$G196*V196","v":0},null,null,{"$f":"$G196*Y196","v":0},null,null,{"$f":"$G196*AB196","v":0},null,null,{"$f":"$G196*AE196","v":0},null,null,{"$f":"$G196*AH196","v":0},null,null,{"$f":"$G196*AK196","v":0},null,null,{"$f":"$G196*AN196","v":0},null,null,{"$f":"$G196*AQ196","v":0},null,null,{"$f":"$G196*AT196","v":0},null,null,{"$f":"$G196*AW196","v":0},null,null,{"$f":"$G196*AZ196","v":0},null,null,{"$f":"$G196*BC196","v":0},null,null,{"$f":"$G196*BF196","v":0},null,null,{"$f":"$G196*BI196","v":0},null,null,{"$f":"$G196*BL196","v":0},null,null,{"$f":"$G196*BO196","v":0},null,null,{"$f":"$G196*BR196","v":0},null,null,{"$f":"$G196*BU196","v":0},null,null,{"$f":"$G196*BX196","v":0},null,null,{"$f":"$G196*CA196","v":0}]
["9.9.3",null,"C","d110  (s min.   2,7)    dužina 3,0m","d110  (s min.   2,7)    length 3,0m","kom/pcs",{"$f":"CENA!G188","v":0},{"$f":"J197+M197+P197+S197+V197+Y197+AB197+AE197+AH197+AK197+AN197+AQ197+AT197+AW197+AZ197+BC197+BF197+BI197+BL197+BO197+BR197+BU197+BX197+CA197","v":32},{"$f":"G197*H197","v":0},5,{"$f":"$G197*J197","v":0},null,null,0,null,null,{"$f":"$G197*P197","v":0},null,null,{"$f":"$G197*S197","v":0},null,null,{"$f":"$G197*V197","v":0},null,null,{"$f":"$G197*Y197","v":0},null,null,{"$f":"$G197*AB197","v":0},null,null,{"$f":"$G197*AE197","v":0},null,null,{"$f":"$G197*AH197","v":0},null,null,{"$f":"$G197*AK197","v":0},null,8,{"$f":"$G197*AN197","v":0},null,5,{"$f":"$G197*AQ197","v":0},null,null,{"$f":"$G197*AT197","v":0},null,null,{"$f":"$G197*AW197","v":0},null,5,{"$f":"$G197*AZ197","v":0},null,2,{"$f":"$G197*BC197","v":0},null,null,{"$f":"$G197*BF197","v":0},null,null,{"$f":"$G197*BI197","v":0},null,null,{"$f":"$G197*BL197","v":0},null,5,{"$f":"$G197*BO197","v":0},null,2,{"$f":"$G197*BR197","v":0},null,null,{"$f":"$G197*BU197","v":0},null,null,{"$f":"$G197*BX197","v":0},null,null,{"$f":"$G197*CA197","v":0}]
["9.10","V",10,"Plitki PE podni slivnik d50 sa horizontalnim odvodom dimenzija 150x150mm","Shallow PE floor drain with horizontal outlet d50 size 150x150mm","kom/pcs",{"$f":"CENA!G189","v":0},{"$f":"J198+M198+P198+S198+V198+Y198+AB198+AE198+AH198+AK198+AN198+AQ198+AT198+AW198+AZ198+BC198+BF198+BI198+BL198+BO198+BR198+BU198+BX198+CA198","v":16},{"$f":"G198*H198","v":0},1,{"$f":"$G198*J198","v":0},null,null,0,null,1,{"$f":"$G198*P198","v":0},null,1,{"$f":"$G198*S198","v":0},null,1,{"$f":"$G198*V198","v":0},null,1,{"$f":"$G198*Y198","v":0},null,null,{"$f":"$G198*AB198","v":0},null,1,{"$f":"$G198*AE198","v":0},null,1,{"$f":"$G198*AH198","v":0},null,null,{"$f":"$G198*AK198","v":0},null,1,{"$f":"$G198*AN198","v":0},null,1,{"$f":"$G198*AQ198","v":0},null,1,{"$f":"$G198*AT198","v":0},null,null,{"$f":"$G198*AW198","v":0},null,1,{"$f":"$G198*AZ198","v":0},null,1,{"$f":"$G198*BC198","v":0},null,1,{"$f":"$G198*BF198","v":0},null,1,{"$f":"$G198*BI198","v":0},null,null,{"$f":"$G198*BL198","v":0},null,1,{"$f":"$G198*BO198","v":0},null,1,{"$f":"$G198*BR198","v":0},null,null,{"$f":"$G198*BU198","v":0},null,null,{"$f":"$G198*BX198","v":0},null,null,{"$f":"$G198*CA198","v":0}]
["9.11","V",11,"Zidni sifoni sa odvodnom mesinganom cevi d32 (mašina za pranje veša i sudova)","Wall siphon with drainage brass tubes d32 (washing machines, dishwashers)","kom/pcs",{"$f":"CENA!G190","v":0},{"$f":"J199+M199+P199+S199+V199+Y199+AB199+AE199+AH199+AK199+AN199+AQ199+AT199+AW199+AZ199+BC199+BF199+BI199+BL199+BO199+BR199+BU199+BX199+CA199","v":16},{"$f":"G199*H199","v":0},1,{"$f":"$G199*J199","v":0},null,null,0,null,1,{"$f":"$G199*P199","v":0},null,1,{"$f":"$G199*S199","v":0},null,1,{"$f":"$G199*V199","v":0},null,1,{"$f":"$G199*Y199","v":0},null,null,{"$f":"$G199*AB199","v":0},null,1,{"$f":"$G199*AE199","v":0},null,1,{"$f":"$G199*AH199","v":0},null,null,{"$f":"$G199*AK199","v":0},null,1,{"$f":"$G199*AN199","v":0},null,1,{"$f":"$G199*AQ199","v":0},null,1,{"$f":"$G199*AT199","v":0},null,null,{"$f":"$G199*AW199","v":0},null,1,{"$f":"$G199*AZ199","v":0},null,1,{"$f":"$G199*BC199","v":0},null,1,{"$f":"$G199*BF199","v":0},null,1,{"$f":"$G199*BI199","v":0},null,null,{"$f":"$G199*BL199","v":0},null,1,{"$f":"$G199*BO199","v":0},null,1,{"$f":"$G199*BR199","v":0},null,null,{"$f":"$G199*BU199","v":0},null,null,{"$f":"$G199*BX199","v":0},null,null,{"$f":"$G199*CA199","v":0}]
[null,null,null,"Oprema u kupatilu","BATHROOM EQUPIMENT"]
["9.12","V",12,"WC šolja od keramike  I klase","Ceramic toilet bowl class 1","kom/pcs",{"$f":"CENA!G192","v":0},{"$f":"J201+M201+P201+S201+V201+Y201+AB201+AE201+AH201+AK201+AN201+AQ201+AT201+AW201+AZ201+BC201+BF201+BI201+BL201+BO201+BR201+BU201+BX201+CA201","v":17},{"$f":"G201*H201","v":0},1,{"$f":"$G201*J201","v":0},null,null,{"$f":"$G201*M201","v":0},null,1,{"$f":"$G201*P201","v":0},null,1,{"$f":"$G201*S201","v":0},null,1,{"$f":"$G201*V201","v":0},null,1,{"$f":"$G201*Y201","v":0},null,null,{"$f":"$G201*AB201","v":0},null,1,{"$f":"$G201*AE201","v":0},null,1,{"$f":"$G201*AH201","v":0},null,null,{"$f":"$G201*AK201","v":0},null,1,{"$f":"$G201*AN201","v":0},null,1,{"$f":"$G201*AQ201","v":0},null,1,{"$f":"$G201*AT201","v":0},null,null,{"$f":"$G201*AW201","v":0},null,1,{"$f":"$G201*AZ201","v":0},null,1,{"$f":"$G201*BC201","v":0},null,1,{"$f":"$G201*BF201","v":0},null,1,{"$f":"$G201*BI201","v":0},null,null,{"$f":"$G201*BL201","v":0},null,1,{"$f":"$G201*BO201","v":0},null,1,{"$f":"$G201*BR201","v":0},null,null,{"$f":"$G201*BU201","v":0},null,1,{"$f":"$G201*BX201","v":0},null,null,{"$f":"$G201*CA201","v":0}]
["9.13","V",13,"Niskomontažni plastični predzidni vodokotlić \nza nisku montažu iznad wc šolje sa plovkom i svim potrebnim delovima za funkcionisanje vodokotlića","Low mounting plastic-wall toilet tank\nfor low installation above the toilet bowl float and all the parts required for the operation of flushing","kom/pcs",{"$f":"CENA!G193","v":0},17,0,1,{"$f":"$G202*J202","v":0},null,null,0,null,1,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,null,0,null,1,0,null,null,0]
["9.14","V",14,"Umivaonikom sa stubom od keramike  I klase","Washbasin with ceramic pillar class 1","kom/pcs",{"$f":"CENA!G194","v":0},17,0,1,{"$f":"$G203*J203","v":0},null,null,0,null,1,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,null,0,null,1,0,null,null,0]
["9.15","V",15,"Pravougaona akrilna tuš kada\ndimenzija 90x90cm sa odlivnim ventilom","Rectangular acrylic shower \nsize 90x90cm with discharge valve","kom/pcs",{"$f":"CENA!G195","v":0},18,0,1,{"$f":"$G204*J204","v":0},null,1,0,null,1,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,null,0,null,1,0,null,null,0]
["9.16","V",16,"Električni akumulacioni bojler 50l vertikalni \ngrejač 2 kW, napon 230V, kazan izrađen od emajliranog lima, sa  pratećim materijalom za ugradnju","Electric storage water heater 50l vertical \nheater 2 kW, 230V, caldron made ​​of enameled steel, with supporting material for installation","kom/pcs",{"$f":"CENA!G196","v":0},17,0,1,{"$f":"$G205*J205","v":0},null,null,0,null,1,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,null,0,null,1,0,null,null,0]
["9.17","V",17,"Ogledalo sa etažerom (iznad umivaonika)\nčetvrtasto, min. dimenzija 80x60cm","Mirror with shelf above wash basin \nsquare, min. 80x60cm","kom/pcs",{"$f":"CENA!G197","v":0},17,0,1,{"$f":"$G206*J206","v":0},null,null,0,null,1,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,1,0,null,1,0,null,null,0,null,1,0,null,1,0,null,null,0,null,1,0,null,null,0]
["9.18","V",18,"Baterije (slavine) \nhromirane baterije za hladnu i toplu vodu","Lever\nchrome lever for cold and hot water","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["9.18.1",null,"A","za umivaonik jednoručna stojeća ","For washbasin single lever basin standing","kom/pcs",{"$f":"CENA!G199","v":0},{"$f":"J208+M208+P208+S208+V208+Y208+AB208+AE208+AH208+AK208+AN208+AQ208+AT208+AW208+AZ208+BC208+BF208+BI208+BL208+BO208+BR208+BU208+BX208+CA208","v":17},{"$f":"G208*H208","v":0},1,{"$f":"$G208*J208","v":0},null,null,{"$f":"$G208*M208","v":0},null,1,{"$f":"$G208*P208","v":0},null,1,{"$f":"$G208*S208","v":0},null,1,{"$f":"$G208*V208","v":0},null,1,{"$f":"$G208*Y208","v":0},null,null,{"$f":"$G208*AB208","v":0},null,1,{"$f":"$G208*AE208","v":0},null,1,{"$f":"$G208*AH208","v":0},null,null,{"$f":"$G208*AK208","v":0},null,1,{"$f":"$G208*AN208","v":0},null,1,{"$f":"$G208*AQ208","v":0},null,1,{"$f":"$G208*AT208","v":0},null,null,{"$f":"$G208*AW208","v":0},null,1,{"$f":"$G208*AZ208","v":0},null,1,{"$f":"$G208*BC208","v":0},null,1,{"$f":"$G208*BF208","v":0},null,1,{"$f":"$G208*BI208","v":0},null,null,{"$f":"$G208*BL208","v":0},null,1,{"$f":"$G208*BO208","v":0},null,1,{"$f":"$G208*BR208","v":0},null,null,{"$f":"$G208*BU208","v":0},null,1,{"$f":"$G208*BX208","v":0},null,null,{"$f":"$G208*CA208","v":0}]
["9.18.2",null,"B","za tuš kadu (sa tuš ručicom i tuš crevom)\njednoručna sa poniklovanim savitljivim crevom","For shower bath (with shower head and shower hose) Single lever with nickel hoses","kom/pcs",{"$f":"CENA!G200","v":0},{"$f":"J209+M209+P209+S209+V209+Y209+AB209+AE209+AH209+AK209+AN209+AQ209+AT209+AW209+AZ209+BC209+BF209+BI209+BL209+BO209+BR209+BU209+BX209+CA209","v":17},{"$f":"G209*H209","v":0},1,{"$f":"$G209*J209","v":0},null,null,0,null,1,{"$f":"$G209*P209","v":0},null,1,{"$f":"$G209*S209","v":0},null,1,{"$f":"$G209*V209","v":0},null,1,{"$f":"$G209*Y209","v":0},null,null,{"$f":"$G209*AB209","v":0},null,1,{"$f":"$G209*AE209","v":0},null,1,{"$f":"$G209*AH209","v":0},null,null,{"$f":"$G209*AK209","v":0},null,1,{"$f":"$G209*AN209","v":0},null,1,{"$f":"$G209*AQ209","v":0},null,1,{"$f":"$G209*AT209","v":0},null,null,{"$f":"$G209*AW209","v":0},null,1,{"$f":"$G209*AZ209","v":0},null,1,{"$f":"$G209*BC209","v":0},null,1,{"$f":"$G209*BF209","v":0},null,1,{"$f":"$G209*BI209","v":0},null,null,{"$f":"$G209*BL209","v":0},null,1,{"$f":"$G209*BO209","v":0},null,1,{"$f":"$G209*BR209","v":0},null,null,{"$f":"$G209*BU209","v":0},null,1,{"$f":"$G209*BX209","v":0},null,null,{"$f":"$G209*CA209","v":0}]
["9.18.3",null,"C","za mašinu za veš i sudove, holender slavina DN20/15, s pripadajućom opremom za ugradnju ","for washing machine and dishwasher, union DN20/15 taps, and all the equipment for installation","kom/pcs",{"$f":"CENA!G201","v":0},{"$f":"J210+M210+P210+S210+V210+Y210+AB210+AE210+AH210+AK210+AN210+AQ210+AT210+AW210+AZ210+BC210+BF210+BI210+BL210+BO210+BR210+BU210+BX210+CA210","v":17},{"$f":"G210*H210","v":0},1,{"$f":"$G210*J210","v":0},null,null,0,null,1,{"$f":"$G210*P210","v":0},null,1,{"$f":"$G210*S210","v":0},null,1,{"$f":"$G210*V210","v":0},null,1,{"$f":"$G210*Y210","v":0},null,null,{"$f":"$G210*AB210","v":0},null,1,{"$f":"$G210*AE210","v":0},null,1,{"$f":"$G210*AH210","v":0},null,null,{"$f":"$G210*AK210","v":0},null,1,{"$f":"$G210*AN210","v":0},null,1,{"$f":"$G210*AQ210","v":0},null,1,{"$f":"$G210*AT210","v":0},null,null,{"$f":"$G210*AW210","v":0},null,1,{"$f":"$G210*AZ210","v":0},null,1,{"$f":"$G210*BC210","v":0},null,1,{"$f":"$G210*BF210","v":0},null,1,{"$f":"$G210*BI210","v":0},null,null,{"$f":"$G210*BL210","v":0},null,1,{"$f":"$G210*BO210","v":0},null,1,{"$f":"$G210*BR210","v":0},null,null,{"$f":"$G210*BU210","v":0},null,1,{"$f":"$G210*BX210","v":0},null,null,{"$f":"$G210*CA210","v":0}]
[null,null,null,"Oprema u kuhinji","KITCHEN EQUIPMENT"]
["9.19","V",19,"Korito sudopere od \"Inox \"-a (dvodelno)\n(izrađeno od plemenitog nerđajućeg čelika)\norjenacione dimenzije:  780 x 435 x 150 mm","kitchen sink \"Inox\" two-part\n(made of stainless steel)\napprox. dim:  780 x 435 x 150 mm","kom/pcs",{"$f":"CENA!G203","v":0},{"$f":"J212+M212+P212+S212+V212+Y212+AB212+AE212+AH212+AK212+AN212+AQ212+AT212+AW212+AZ212+BC212+BF212+BI212+BL212+BO212+BR212+BU212+BX212+CA212","v":9},{"$f":"G212*H212","v":0},null,{"$f":"$G212*J212","v":0},null,null,{"$f":"$G212*M212","v":0},null,1,{"$f":"$G212*P212","v":0},null,null,{"$f":"$G212*S212","v":0},null,1,{"$f":"$G212*V212","v":0},null,null,{"$f":"$G212*Y212","v":0},null,null,{"$f":"$G212*AB212","v":0},null,1,{"$f":"$G212*AE212","v":0},null,1,{"$f":"$G212*AH212","v":0},null,null,{"$f":"$G212*AK212","v":0},null,1,{"$f":"$G212*AN212","v":0},null,1,{"$f":"$G212*AQ212","v":0},null,null,{"$f":"$G212*AT212","v":0},null,null,{"$f":"$G212*AW212","v":0},null,null,{"$f":"$G212*AZ212","v":0},null,1,{"$f":"$G212*BC212","v":0},null,1,{"$f":"$G212*BF212","v":0},null,null,{"$f":"$G212*BI212","v":0},null,null,{"$f":"$G212*BL212","v":0},null,1,{"$f":"$G212*BO212","v":0},null,null,{"$f":"$G212*BR212","v":0},null,null,{"$f":"$G212*BU212","v":0},null,null,{"$f":"$G212*BX212","v":0},null,null,{"$f":"$G212*CA212","v":0}]
["9.20","V",20,"Električni akumulacioni bojler 5l\nza ugradnju iznad sudopere, vertikalni grejač 2 kW, napon 230V, kazan izrađen od plastike\nsa  pratećim materijalom za ugradnju","Electric storage water heater 5l\nFitting over the sink, vertical heater 2 kW, 230V, caldron made ​​of plastic with the materials for installation","kom/pcs",{"$f":"CENA!G204","v":0},{"$f":"J213+M213+P213+S213+V213+Y213+AB213+AE213+AH213+AK213+AN213+AQ213+AT213+AW213+AZ213+BC213+BF213+BI213+BL213+BO213+BR213+BU213+BX213+CA213","v":8},{"$f":"G213*H213","v":0},null,{"$f":"$G213*J213","v":0},null,null,0,null,null,{"$f":"$G213*P213","v":0},null,null,{"$f":"$G213*S213","v":0},null,1,{"$f":"$G213*V213","v":0},null,null,{"$f":"$G213*Y213","v":0},null,null,{"$f":"$G213*AB213","v":0},null,1,{"$f":"$G213*AE213","v":0},null,1,{"$f":"$G213*AH213","v":0},null,null,{"$f":"$G213*AK213","v":0},null,1,{"$f":"$G213*AN213","v":0},null,1,{"$f":"$G213*AQ213","v":0},null,null,{"$f":"$G213*AT213","v":0},null,null,{"$f":"$G213*AW213","v":0},null,null,{"$f":"$G213*AZ213","v":0},null,1,{"$f":"$G213*BC213","v":0},null,null,{"$f":"$G213*BF213","v":0},null,null,{"$f":"$G213*BI213","v":0},null,null,{"$f":"$G213*BL213","v":0},null,1,{"$f":"$G213*BO213","v":0},null,1,{"$f":"$G213*BR213","v":0},null,null,{"$f":"$G213*BU213","v":0},null,null,{"$f":"$G213*BX213","v":0},null,null,{"$f":"$G213*CA213","v":0}]
["9.21","V",21,"Baterija za sudoperu jednoručna stojeća hromirana baterija za hladnu i toplu vodu ","Sink-standing single lever chrome mixer for hot and cold water","kom/pcs",{"$f":"CENA!G205","v":0},{"$f":"J214+M214+P214+S214+V214+Y214+AB214+AE214+AH214+AK214+AN214+AQ214+AT214+AW214+AZ214+BC214+BF214+BI214+BL214+BO214+BR214+BU214+BX214+CA214","v":13},{"$f":"G214*H214","v":0},null,{"$f":"$G214*J214","v":0},null,null,0,null,1,{"$f":"$G214*P214","v":0},null,1,{"$f":"$G214*S214","v":0},null,1,{"$f":"$G214*V214","v":0},null,1,{"$f":"$G214*Y214","v":0},null,null,{"$f":"$G214*AB214","v":0},null,1,{"$f":"$G214*AE214","v":0},null,1,{"$f":"$G214*AH214","v":0},null,null,{"$f":"$G214*AK214","v":0},null,1,{"$f":"$G214*AN214","v":0},null,1,{"$f":"$G214*AQ214","v":0},null,1,{"$f":"$G214*AT214","v":0},null,null,{"$f":"$G214*AW214","v":0},null,null,{"$f":"$G214*AZ214","v":0},null,1,{"$f":"$G214*BC214","v":0},null,1,{"$f":"$G214*BF214","v":0},null,null,{"$f":"$G214*BI214","v":0},null,null,{"$f":"$G214*BL214","v":0},null,1,{"$f":"$G214*BO214","v":0},null,1,{"$f":"$G214*BR214","v":0},null,null,{"$f":"$G214*BU214","v":0},null,null,{"$f":"$G214*BX214","v":0},null,null,{"$f":"$G214*CA214","v":0}]
[]
["10","E",null,"ELEKTRO MATERIJAL I OPREMA\n","Electrical materials and equipment"]
[null,null,null,"Kablovi i kablovski pribor","Electrical cables and cable accessories"]
["10.1","E",1,"Napojni kablovi","Power cables","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["10.1.1",null,"A","X00-A      4x16 mm2","X00-A      4x16 mm2","m",{"$f":"CENA!G210","v":0},{"$f":"J219+M219+P219+S219+V219+Y219+AB219+AE219+AH219+AK219+AN219+AQ219+AT219+AW219+AZ219+BC219+BF219+BI219+BL219+BO219+BR219+BU219+BX219+CA219","v":0},{"$f":"G219*H219","v":0},null,{"$f":"$G219*J219","v":0},null,null,{"$f":"$G219*M219","v":0},null,null,{"$f":"$G219*P219","v":0},null,null,{"$f":"$G219*S219","v":0},null,null,{"$f":"$G219*V219","v":0},null,null,{"$f":"$G219*Y219","v":0},null,null,{"$f":"$G219*AB219","v":0},null,null,{"$f":"$G219*AE219","v":0},null,null,{"$f":"$G219*AH219","v":0},null,null,{"$f":"$G219*AK219","v":0},null,null,{"$f":"$G219*AN219","v":0},null,null,{"$f":"$G219*AQ219","v":0},null,null,{"$f":"$G219*AT219","v":0},null,null,{"$f":"$G219*AW219","v":0},null,null,{"$f":"$G219*AZ219","v":0},null,null,{"$f":"$G219*BC219","v":0},null,null,{"$f":"$G219*BF219","v":0},null,null,{"$f":"$G219*BI219","v":0},null,null,{"$f":"$G219*BL219","v":0},null,null,{"$f":"$G219*BO219","v":0},null,null,{"$f":"$G219*BR219","v":0},null,null,{"$f":"$G219*BU219","v":0},null,null,{"$f":"$G219*BX219","v":0},null,null,{"$f":"$G219*CA219","v":0}]
["10.1.2",null,"B","PP00-Y   5x6    mm2","PP00-Y   5x6    mm2","m",{"$f":"CENA!G211","v":0},{"$f":"J220+M220+P220+S220+V220+Y220+AB220+AE220+AH220+AK220+AN220+AQ220+AT220+AW220+AZ220+BC220+BF220+BI220+BL220+BO220+BR220+BU220+BX220+CA220","v":0},{"$f":"G220*H220","v":0},null,{"$f":"$G220*J220","v":0},null,null,0,null,null,{"$f":"$G220*P220","v":0},null,null,0,null,null,{"$f":"$G220*V220","v":0},null,null,{"$f":"$G220*Y220","v":0},null,null,{"$f":"$G220*AB220","v":0},null,null,{"$f":"$G220*AE220","v":0},null,null,{"$f":"$G220*AH220","v":0},null,null,{"$f":"$G220*AK220","v":0},null,null,{"$f":"$G220*AN220","v":0},null,null,{"$f":"$G220*AQ220","v":0},null,null,{"$f":"$G220*AT220","v":0},null,null,{"$f":"$G220*AW220","v":0},null,null,{"$f":"$G220*AZ220","v":0},null,null,{"$f":"$G220*BC220","v":0},null,null,{"$f":"$G220*BF220","v":0},null,null,{"$f":"$G220*BI220","v":0},null,null,{"$f":"$G220*BL220","v":0},null,null,{"$f":"$G220*BO220","v":0},null,null,{"$f":"$G220*BR220","v":0},null,null,{"$f":"$G220*BU220","v":0},null,null,{"$f":"$G220*BX220","v":0},null,null,{"$f":"$G220*CA220","v":0}]
["10.1.3",null,"C","PP00-Y   5x10  mm2","PP00-Y   5x10  mm2","m",{"$f":"CENA!G212","v":0},{"$f":"J221+M221+P221+S221+V221+Y221+AB221+AE221+AH221+AK221+AN221+AQ221+AT221+AW221+AZ221+BC221+BF221+BI221+BL221+BO221+BR221+BU221+BX221+CA221","v":0},{"$f":"G221*H221","v":0},null,{"$f":"$G221*J221","v":0},null,null,0,null,null,{"$f":"$G221*P221","v":0},null,null,0,null,null,{"$f":"$G221*V221","v":0},null,null,{"$f":"$G221*Y221","v":0},null,null,{"$f":"$G221*AB221","v":0},null,null,{"$f":"$G221*AE221","v":0},null,null,{"$f":"$G221*AH221","v":0},null,null,{"$f":"$G221*AK221","v":0},null,null,{"$f":"$G221*AN221","v":0},null,null,{"$f":"$G221*AQ221","v":0},null,null,{"$f":"$G221*AT221","v":0},null,null,{"$f":"$G221*AW221","v":0},null,null,{"$f":"$G221*AZ221","v":0},null,null,{"$f":"$G221*BC221","v":0},null,null,{"$f":"$G221*BF221","v":0},null,null,{"$f":"$G221*BI221","v":0},null,null,{"$f":"$G221*BL221","v":0},null,null,{"$f":"$G221*BO221","v":0},null,null,{"$f":"$G221*BR221","v":0},null,null,{"$f":"$G221*BU221","v":0},null,null,{"$f":"$G221*BX221","v":0},null,null,{"$f":"$G221*CA221","v":0}]
["10.2","E",2,"Instalacioni kablovi","Installation cables","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["10.2.1",null,"A","PP-Y       3x1,5  mm2","PP-Y       3x1,5  mm2","m",{"$f":"CENA!G214","v":0},{"$f":"J223+M223+P223+S223+V223+Y223+AB223+AE223+AH223+AK223+AN223+AQ223+AT223+AW223+AZ223+BC223+BF223+BI223+BL223+BO223+BR223+BU223+BX223+CA223","v":790},{"$f":"G223*H223","v":0},150,{"$f":"$G223*J223","v":0},null,50,{"$f":"$G223*M223","v":0},null,50,{"$f":"$G223*P223","v":0},null,null,{"$f":"$G223*S223","v":0},null,100,{"$f":"$G223*V223","v":0},null,null,{"$f":"$G223*Y223","v":0},null,40,{"$f":"$G223*AB223","v":0},null,100,{"$f":"$G223*AE223","v":0},null,null,{"$f":"$G223*AH223","v":0},null,null,{"$f":"$G223*AK223","v":0},null,50,{"$f":"$G223*AN223","v":0},null,50,{"$f":"$G223*AQ223","v":0},null,null,{"$f":"$G223*AT223","v":0},null,null,{"$f":"$G223*AW223","v":0},null,null,{"$f":"$G223*AZ223","v":0},null,100,{"$f":"$G223*BC223","v":0},null,null,{"$f":"$G223*BF223","v":0},null,null,{"$f":"$G223*BI223","v":0},null,null,{"$f":"$G223*BL223","v":0},null,50,{"$f":"$G223*BO223","v":0},null,50,{"$f":"$G223*BR223","v":0},null,null,{"$f":"$G223*BU223","v":0},null,null,{"$f":"$G223*BX223","v":0},null,null,{"$f":"$G223*CA223","v":0}]
["10.2.2",null,"B","PP-Y       4x1,5  mm2","PP-Y       4x1,5  mm2","m",{"$f":"CENA!G215","v":0},{"$f":"J224+M224+P224+S224+V224+Y224+AB224+AE224+AH224+AK224+AN224+AQ224+AT224+AW224+AZ224+BC224+BF224+BI224+BL224+BO224+BR224+BU224+BX224+CA224","v":0},{"$f":"G224*H224","v":0},null,{"$f":"$G224*J224","v":0},null,null,0,null,null,{"$f":"$G224*P224","v":0},null,null,0,null,null,{"$f":"$G224*V224","v":0},null,null,{"$f":"$G224*Y224","v":0},null,null,{"$f":"$G224*AB224","v":0},null,null,{"$f":"$G224*AE224","v":0},null,null,{"$f":"$G224*AH224","v":0},null,null,{"$f":"$G224*AK224","v":0},null,null,{"$f":"$G224*AN224","v":0},null,null,{"$f":"$G224*AQ224","v":0},null,null,{"$f":"$G224*AT224","v":0},null,null,{"$f":"$G224*AW224","v":0},null,null,{"$f":"$G224*AZ224","v":0},null,null,{"$f":"$G224*BC224","v":0},null,null,{"$f":"$G224*BF224","v":0},null,null,{"$f":"$G224*BI224","v":0},null,null,{"$f":"$G224*BL224","v":0},null,null,{"$f":"$G224*BO224","v":0},null,null,{"$f":"$G224*BR224","v":0},null,null,{"$f":"$G224*BU224","v":0},null,null,{"$f":"$G224*BX224","v":0},null,null,{"$f":"$G224*CA224","v":0}]
["10.2.3",null,"C","PP-Y       3x2,5  mm2","PP-Y       3x2,5  mm2","m",{"$f":"CENA!G216","v":0},{"$f":"J225+M225+P225+S225+V225+Y225+AB225+AE225+AH225+AK225+AN225+AQ225+AT225+AW225+AZ225+BC225+BF225+BI225+BL225+BO225+BR225+BU225+BX225+CA225","v":1080},{"$f":"G225*H225","v":0},150,{"$f":"$G225*J225","v":0},null,50,0,null,100,{"$f":"$G225*P225","v":0},null,70,0,null,150,{"$f":"$G225*V225","v":0},null,null,{"$f":"$G225*Y225","v":0},null,40,{"$f":"$G225*AB225","v":0},null,150,{"$f":"$G225*AE225","v":0},null,null,{"$f":"$G225*AH225","v":0},null,null,{"$f":"$G225*AK225","v":0},null,50,{"$f":"$G225*AN225","v":0},null,50,{"$f":"$G225*AQ225","v":0},null,null,{"$f":"$G225*AT225","v":0},null,null,{"$f":"$G225*AW225","v":0},null,null,{"$f":"$G225*AZ225","v":0},null,150,{"$f":"$G225*BC225","v":0},null,null,{"$f":"$G225*BF225","v":0},null,null,{"$f":"$G225*BI225","v":0},null,null,{"$f":"$G225*BL225","v":0},null,70,{"$f":"$G225*BO225","v":0},null,50,{"$f":"$G225*BR225","v":0},null,null,{"$f":"$G225*BU225","v":0},null,null,{"$f":"$G225*BX225","v":0},null,null,{"$f":"$G225*CA225","v":0}]
["10.2.4",null,"D","PP-Y       5x2,5  mm2","PP-Y       5x2,5  mm2","m",{"$f":"CENA!G217","v":0},{"$f":"J226+M226+P226+S226+V226+Y226+AB226+AE226+AH226+AK226+AN226+AQ226+AT226+AW226+AZ226+BC226+BF226+BI226+BL226+BO226+BR226+BU226+BX226+CA226","v":620},{"$f":"G226*H226","v":0},100,{"$f":"$G226*J226","v":0},null,50,0,null,50,{"$f":"$G226*P226","v":0},null,null,0,null,100,{"$f":"$G226*V226","v":0},null,null,{"$f":"$G226*Y226","v":0},null,null,{"$f":"$G226*AB226","v":0},null,100,{"$f":"$G226*AE226","v":0},null,null,{"$f":"$G226*AH226","v":0},null,null,{"$f":"$G226*AK226","v":0},null,20,{"$f":"$G226*AN226","v":0},null,50,{"$f":"$G226*AQ226","v":0},null,null,{"$f":"$G226*AT226","v":0},null,null,{"$f":"$G226*AW226","v":0},null,null,{"$f":"$G226*AZ226","v":0},null,100,{"$f":"$G226*BC226","v":0},null,null,{"$f":"$G226*BF226","v":0},null,null,{"$f":"$G226*BI226","v":0},null,null,{"$f":"$G226*BL226","v":0},null,50,{"$f":"$G226*BO226","v":0},null,null,{"$f":"$G226*BR226","v":0},null,null,{"$f":"$G226*BU226","v":0},null,null,{"$f":"$G226*BX226","v":0},null,null,{"$f":"$G226*CA226","v":0}]
["10.3","E",3,"Instalacione PVC cevi","PVC pipe for installations of cables","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["10.3.1",null,"A","fi 16mm2","fi 16mm2","m",{"$f":"CENA!G219","v":0},{"$f":"J228+M228+P228+S228+V228+Y228+AB228+AE228+AH228+AK228+AN228+AQ228+AT228+AW228+AZ228+BC228+BF228+BI228+BL228+BO228+BR228+BU228+BX228+CA228","v":0},{"$f":"G228*H228","v":0},null,{"$f":"$G228*J228","v":0},null,null,{"$f":"$G228*M228","v":0},null,null,{"$f":"$G228*P228","v":0},null,null,{"$f":"$G228*S228","v":0},null,null,{"$f":"$G228*V228","v":0},null,null,{"$f":"$G228*Y228","v":0},null,null,{"$f":"$G228*AB228","v":0},null,null,{"$f":"$G228*AE228","v":0},null,null,{"$f":"$G228*AH228","v":0},null,null,{"$f":"$G228*AK228","v":0},null,null,{"$f":"$G228*AN228","v":0},null,null,{"$f":"$G228*AQ228","v":0},null,null,{"$f":"$G228*AT228","v":0},null,null,{"$f":"$G228*AW228","v":0},null,null,{"$f":"$G228*AZ228","v":0},null,null,{"$f":"$G228*BC228","v":0},null,null,{"$f":"$G228*BF228","v":0},null,null,{"$f":"$G228*BI228","v":0},null,null,{"$f":"$G228*BL228","v":0},null,null,{"$f":"$G228*BO228","v":0},null,null,{"$f":"$G228*BR228","v":0},null,null,{"$f":"$G228*BU228","v":0},null,null,{"$f":"$G228*BX228","v":0},null,null,{"$f":"$G228*CA228","v":0}]
["10.3.2",null,"B","fi 50mm2","fi 50mm2","m",{"$f":"CENA!G220","v":0},{"$f":"J229+M229+P229+S229+V229+Y229+AB229+AE229+AH229+AK229+AN229+AQ229+AT229+AW229+AZ229+BC229+BF229+BI229+BL229+BO229+BR229+BU229+BX229+CA229","v":0},{"$f":"G229*H229","v":0},null,{"$f":"$G229*J229","v":0},null,null,0,null,null,{"$f":"$G229*P229","v":0},null,null,0,null,null,{"$f":"$G229*V229","v":0},null,null,{"$f":"$G229*Y229","v":0},null,null,{"$f":"$G229*AB229","v":0},null,null,{"$f":"$G229*AE229","v":0},null,null,{"$f":"$G229*AH229","v":0},null,null,{"$f":"$G229*AK229","v":0},null,null,{"$f":"$G229*AN229","v":0},null,null,{"$f":"$G229*AQ229","v":0},null,null,{"$f":"$G229*AT229","v":0},null,null,{"$f":"$G229*AW229","v":0},null,null,{"$f":"$G229*AZ229","v":0},null,null,{"$f":"$G229*BC229","v":0},null,null,{"$f":"$G229*BF229","v":0},null,null,{"$f":"$G229*BI229","v":0},null,null,{"$f":"$G229*BL229","v":0},null,null,{"$f":"$G229*BO229","v":0},null,null,{"$f":"$G229*BR229","v":0},null,null,{"$f":"$G229*BU229","v":0},null,null,{"$f":"$G229*BX229","v":0},null,null,{"$f":"$G229*CA229","v":0}]
[null,null,null,"Razvodne table i oprema","The junction boards and equipment"]
["10.4","E",4,"Razvodna tabla Stanska, za ugradnju na zid sa transparentim vratima, sa mestom za 18 modula, DIN šinom, IP40\nRazvodna tabla sadrži :","Junction board (for flat) for wall mounting with transparent door, with space for 18 modules, DIN rail, IP40\nJunction board contains:","kom/pcs",{"$f":"CENA!G222","v":0},{"$f":"J231+M231+P231+S231+V231+Y231+AB231+AE231+AH231+AK231+AN231+AQ231+AT231+AW231+AZ231+BC231+BF231+BI231+BL231+BO231+BR231+BU231+BX231+CA231","v":8},{"$f":"G231*H231","v":0},1,{"$f":"$G231*J231","v":0},null,1,{"$f":"$G231*M231","v":0},null,1,{"$f":"$G231*P231","v":0},null,null,0,null,1,{"$f":"$G231*V231","v":0},null,null,{"$f":"$G231*Y231","v":0},null,null,{"$f":"$G231*AB231","v":0},null,1,{"$f":"$G231*AE231","v":0},null,null,{"$f":"$G231*AH231","v":0},null,null,{"$f":"$G231*AK231","v":0},null,null,{"$f":"$G231*AN231","v":0},null,1,{"$f":"$G231*AQ231","v":0},null,null,{"$f":"$G231*AT231","v":0},null,null,{"$f":"$G231*AW231","v":0},null,null,{"$f":"$G231*AZ231","v":0},null,1,{"$f":"$G231*BC231","v":0},null,null,{"$f":"$G231*BF231","v":0},null,null,{"$f":"$G231*BI231","v":0},null,null,{"$f":"$G231*BL231","v":0},null,null,{"$f":"$G231*BO231","v":0},null,1,{"$f":"$G231*BR231","v":0},null,null,{"$f":"$G231*BU231","v":0},null,null,{"$f":"$G231*BX231","v":0},null,null,{"$f":"$G231*CA231","v":0}]
[null,null,null,"Jednopolni instalacioni prekidač\n(automatski osigurač) za montažu na DIN šinu nom. napona 230V/400V, 50Hz; karakteristike B; prekidne moći 6kA:","Single-pole fuse\n(Automatic fuse) for mounting on DIN rail nom. voltage 230V/400V, 50Hz, features B; breaking capacity 6kA:","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
[null,null,null,"nazivne struje 6A, komada 1","rated current of 6A","kom/pcs","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
[null,null,null,"nazivne struje 10A, komada 2","rated current of 10A","kom/pcs","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
[null,null,null,"nazivne struje 16A, komada 9","rated current of 16A","kom/pcs","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
[null,null,null,"Signalna sijalica\nza signalizaciju tarife 230V za ugradnju u stansku razvodnu tablu, montažu na DIN šinu, komada 1","The indicator lamp\nfor signaling rates 230V for use in flat junction board, mounting on DIN rail","kom/pcs","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
[null,null,null,"FID sklopka za ugradnju u stansku razvodnu tablu, montažu na DIN šinu, ","FID switch for installation in junction board, mounting on DIN rail","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
[null,null,null,"16A/30mA,  2-polna,   230V, 50Hz; komada 2","16A/30mA, 2-pole, 230V, 50Hz;","kom/pcs","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
[null,null,null,"25A/0,5A,    4-polna,    230V/400V, 50Hz; komada 1","25A / 0,5 A, 4-pole, 230V/400V, 50Hz;","kom/pcs","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
[null,null,null,"Instalaciono zvono 230V, 50Hz; za ugradnju u stansku razvodnu tablu, montažu na DIN šinu, komada 1","Bell 230V, 50Hz, for use in junction board, mounting on DIN rail","kom/pcs","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
[null,null,null,"Instalacioni materijal","Installation material"]
["10.5","E",5,"Instalaciona kutija\nza ugradnju u završnu obradu zida","Installation box\nfor installation in the wall","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["10.5.1",null,"A","fi 60 mm","fi 60 mm","kom/pcs",{"$f":"CENA!G234","v":0},{"$f":"J243+M243+P243+S243+V243+Y243+AB243+AE243+AH243+AK243+AN243+AQ243+AT243+AW243+AZ243+BC243+BF243+BI243+BL243+BO243+BR243+BU243+BX243+CA243","v":140},{"$f":"G243*H243","v":0},20,{"$f":"$G243*J243","v":0},null,null,{"$f":"$G243*M243","v":0},null,20,{"$f":"$G243*P243","v":0},null,null,{"$f":"$G243*S243","v":0},null,20,{"$f":"$G243*V243","v":0},null,null,{"$f":"$G243*Y243","v":0},null,null,{"$f":"$G243*AB243","v":0},null,20,{"$f":"$G243*AE243","v":0},null,null,{"$f":"$G243*AH243","v":0},null,null,{"$f":"$G243*AK243","v":0},null,10,{"$f":"$G243*AN243","v":0},null,15,{"$f":"$G243*AQ243","v":0},null,null,{"$f":"$G243*AT243","v":0},null,null,{"$f":"$G243*AW243","v":0},null,null,{"$f":"$G243*AZ243","v":0},null,20,{"$f":"$G243*BC243","v":0},null,null,{"$f":"$G243*BF243","v":0},null,null,{"$f":"$G243*BI243","v":0},null,null,{"$f":"$G243*BL243","v":0},null,10,{"$f":"$G243*BO243","v":0},null,5,{"$f":"$G243*BR243","v":0},null,null,{"$f":"$G243*BU243","v":0},null,null,{"$f":"$G243*BX243","v":0},null,null,{"$f":"$G243*CA243","v":0}]
["10.5.2",null,"B","fi 78 mm","fi 78 mm","kom/pcs",{"$f":"CENA!G235","v":0},{"$f":"J244+M244+P244+S244+V244+Y244+AB244+AE244+AH244+AK244+AN244+AQ244+AT244+AW244+AZ244+BC244+BF244+BI244+BL244+BO244+BR244+BU244+BX244+CA244","v":89},{"$f":"G244*H244","v":0},15,{"$f":"$G244*J244","v":0},null,null,0,null,10,{"$f":"$G244*P244","v":0},null,null,0,null,15,{"$f":"$G244*V244","v":0},null,null,{"$f":"$G244*Y244","v":0},null,null,{"$f":"$G244*AB244","v":0},null,15,{"$f":"$G244*AE244","v":0},null,null,{"$f":"$G244*AH244","v":0},null,null,{"$f":"$G244*AK244","v":0},null,5,{"$f":"$G244*AN244","v":0},null,10,{"$f":"$G244*AQ244","v":0},null,null,{"$f":"$G244*AT244","v":0},null,null,{"$f":"$G244*AW244","v":0},null,null,{"$f":"$G244*AZ244","v":0},null,10,{"$f":"$G244*BC244","v":0},null,null,{"$f":"$G244*BF244","v":0},null,null,{"$f":"$G244*BI244","v":0},null,null,{"$f":"$G244*BL244","v":0},null,5,{"$f":"$G244*BO244","v":0},null,4,{"$f":"$G244*BR244","v":0},null,null,{"$f":"$G244*BU244","v":0},null,null,{"$f":"$G244*BX244","v":0},null,null,{"$f":"$G244*CA244","v":0}]
["10.5.3",null,"C","100x100mm","100x100mm","kom/pcs",{"$f":"CENA!G236","v":0},{"$f":"J245+M245+P245+S245+V245+Y245+AB245+AE245+AH245+AK245+AN245+AQ245+AT245+AW245+AZ245+BC245+BF245+BI245+BL245+BO245+BR245+BU245+BX245+CA245","v":63},{"$f":"G245*H245","v":0},10,{"$f":"$G245*J245","v":0},null,null,0,null,15,{"$f":"$G245*P245","v":0},null,null,0,null,10,{"$f":"$G245*V245","v":0},null,null,{"$f":"$G245*Y245","v":0},null,null,{"$f":"$G245*AB245","v":0},null,10,{"$f":"$G245*AE245","v":0},null,null,{"$f":"$G245*AH245","v":0},null,null,{"$f":"$G245*AK245","v":0},null,1,{"$f":"$G245*AN245","v":0},null,5,{"$f":"$G245*AQ245","v":0},null,null,{"$f":"$G245*AT245","v":0},null,null,{"$f":"$G245*AW245","v":0},null,null,{"$f":"$G245*AZ245","v":0},null,5,{"$f":"$G245*BC245","v":0},null,null,{"$f":"$G245*BF245","v":0},null,null,{"$f":"$G245*BI245","v":0},null,null,{"$f":"$G245*BL245","v":0},null,2,{"$f":"$G245*BO245","v":0},null,5,{"$f":"$G245*BR245","v":0},null,null,{"$f":"$G245*BU245","v":0},null,null,{"$f":"$G245*BX245","v":0},null,null,{"$f":"$G245*CA245","v":0}]
["10.6","E",6,"Instalaciona priključnica IP20 za ugradnju u završnu obradu zida sa zaštitnim kontaktom","Installation socket IP20 for installation in the wall with a protection contact","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["10.6.1",null,"A","16A, monofazna, 250 V","16A, single-phase, 250 V","kom/pcs",{"$f":"CENA!G238","v":0},{"$f":"J247+M247+P247+S247+V247+Y247+AB247+AE247+AH247+AK247+AN247+AQ247+AT247+AW247+AZ247+BC247+BF247+BI247+BL247+BO247+BR247+BU247+BX247+CA247","v":91},{"$f":"G247*H247","v":0},15,{"$f":"$G247*J247","v":0},null,null,{"$f":"$G247*M247","v":0},null,15,{"$f":"$G247*P247","v":0},null,5,{"$f":"$G247*S247","v":0},null,15,{"$f":"$G247*V247","v":0},null,null,{"$f":"$G247*Y247","v":0},null,null,{"$f":"$G247*AB247","v":0},null,10,{"$f":"$G247*AE247","v":0},null,null,{"$f":"$G247*AH247","v":0},null,null,{"$f":"$G247*AK247","v":0},null,1,{"$f":"$G247*AN247","v":0},null,10,{"$f":"$G247*AQ247","v":0},null,null,{"$f":"$G247*AT247","v":0},null,null,{"$f":"$G247*AW247","v":0},null,null,{"$f":"$G247*AZ247","v":0},null,10,{"$f":"$G247*BC247","v":0},null,null,{"$f":"$G247*BF247","v":0},null,null,{"$f":"$G247*BI247","v":0},null,null,{"$f":"$G247*BL247","v":0},null,5,{"$f":"$G247*BO247","v":0},null,5,{"$f":"$G247*BR247","v":0},null,null,{"$f":"$G247*BU247","v":0},null,null,{"$f":"$G247*BX247","v":0},null,null,{"$f":"$G247*CA247","v":0}]
["10.6.2",null,"B","16A, monofazna, dupla, 250 V","16A, single-phase, double, 250 V","kom/pcs",{"$f":"CENA!G239","v":0},{"$f":"J248+M248+P248+S248+V248+Y248+AB248+AE248+AH248+AK248+AN248+AQ248+AT248+AW248+AZ248+BC248+BF248+BI248+BL248+BO248+BR248+BU248+BX248+CA248","v":64},{"$f":"G248*H248","v":0},10,{"$f":"$G248*J248","v":0},null,null,0,null,10,{"$f":"$G248*P248","v":0},null,2,0,null,10,{"$f":"$G248*V248","v":0},null,null,{"$f":"$G248*Y248","v":0},null,null,{"$f":"$G248*AB248","v":0},null,10,{"$f":"$G248*AE248","v":0},null,null,{"$f":"$G248*AH248","v":0},null,null,{"$f":"$G248*AK248","v":0},null,5,{"$f":"$G248*AN248","v":0},null,5,{"$f":"$G248*AQ248","v":0},null,null,{"$f":"$G248*AT248","v":0},null,null,{"$f":"$G248*AW248","v":0},null,null,{"$f":"$G248*AZ248","v":0},null,5,{"$f":"$G248*BC248","v":0},null,null,{"$f":"$G248*BF248","v":0},null,null,{"$f":"$G248*BI248","v":0},null,null,{"$f":"$G248*BL248","v":0},null,2,{"$f":"$G248*BO248","v":0},null,5,{"$f":"$G248*BR248","v":0},null,null,{"$f":"$G248*BU248","v":0},null,null,{"$f":"$G248*BX248","v":0},null,null,{"$f":"$G248*CA248","v":0}]
["10.6.3",null,"C","16A, trofazna, 400V","16A, three-phase, 400V","kom/pcs",{"$f":"CENA!G240","v":0},{"$f":"J249+M249+P249+S249+V249+Y249+AB249+AE249+AH249+AK249+AN249+AQ249+AT249+AW249+AZ249+BC249+BF249+BI249+BL249+BO249+BR249+BU249+BX249+CA249","v":13},{"$f":"G249*H249","v":0},2,{"$f":"$G249*J249","v":0},null,null,0,null,2,{"$f":"$G249*P249","v":0},null,null,0,null,2,{"$f":"$G249*V249","v":0},null,null,{"$f":"$G249*Y249","v":0},null,null,{"$f":"$G249*AB249","v":0},null,2,{"$f":"$G249*AE249","v":0},null,null,{"$f":"$G249*AH249","v":0},null,null,{"$f":"$G249*AK249","v":0},null,1,{"$f":"$G249*AN249","v":0},null,1,{"$f":"$G249*AQ249","v":0},null,null,{"$f":"$G249*AT249","v":0},null,null,{"$f":"$G249*AW249","v":0},null,null,{"$f":"$G249*AZ249","v":0},null,1,{"$f":"$G249*BC249","v":0},null,null,{"$f":"$G249*BF249","v":0},null,null,{"$f":"$G249*BI249","v":0},null,null,{"$f":"$G249*BL249","v":0},null,1,{"$f":"$G249*BO249","v":0},null,1,{"$f":"$G249*BR249","v":0},null,null,{"$f":"$G249*BU249","v":0},null,null,{"$f":"$G249*BX249","v":0},null,null,{"$f":"$G249*CA249","v":0}]
["10.7","E",7,"Instalaciona priključnica IP43 sa poklopcem za ugradnju u završnu obradu zida, sa zaštit. kontaktom, 16A, monofazna, 250 V","Installation socket IP43 with cover for use in wall with protection. contact, 16A, single-phase, 250 V","kom/pcs",{"$f":"CENA!G241","v":0},{"$f":"J250+M250+P250+S250+V250+Y250+AB250+AE250+AH250+AK250+AN250+AQ250+AT250+AW250+AZ250+BC250+BF250+BI250+BL250+BO250+BR250+BU250+BX250+CA250","v":9},{"$f":"G250*H250","v":0},1,{"$f":"$G250*J250","v":0},null,null,0,null,1,{"$f":"$G250*P250","v":0},null,null,null,null,1,{"$f":"$G250*V250","v":0},null,null,{"$f":"$G250*Y250","v":0},null,null,{"$f":"$G250*AB250","v":0},null,1,{"$f":"$G250*AE250","v":0},null,null,{"$f":"$G250*AH250","v":0},null,null,{"$f":"$G250*AK250","v":0},null,1,{"$f":"$G250*AN250","v":0},null,1,{"$f":"$G250*AQ250","v":0},null,null,{"$f":"$G250*AT250","v":0},null,null,{"$f":"$G250*AW250","v":0},null,null,{"$f":"$G250*AZ250","v":0},null,1,{"$f":"$G250*BC250","v":0},null,null,{"$f":"$G250*BF250","v":0},null,null,{"$f":"$G250*BI250","v":0},null,null,{"$f":"$G250*BL250","v":0},null,1,{"$f":"$G250*BO250","v":0},null,1,{"$f":"$G250*BR250","v":0},null,null,{"$f":"$G250*BU250","v":0},null,null,{"$f":"$G250*BX250","v":0},null,null,{"$f":"$G250*CA250","v":0}]
["10.8","E",8,"Prekidači\n IP20 za ugradnju u završnu obradu zida","Switches \n IP20 for installation in wall","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["10.8.1",null,"A","običan, 10A","regular, 10A","kom/pcs",{"$f":"CENA!G243","v":0},{"$f":"J252+M252+P252+S252+V252+Y252+AB252+AE252+AH252+AK252+AN252+AQ252+AT252+AW252+AZ252+BC252+BF252+BI252+BL252+BO252+BR252+BU252+BX252+CA252","v":74},{"$f":"G252*H252","v":0},10,{"$f":"$G252*J252","v":0},null,null,{"$f":"$G252*M252","v":0},null,10,{"$f":"$G252*P252","v":0},null,2,{"$f":"$G252*S252","v":0},null,10,{"$f":"$G252*V252","v":0},null,null,{"$f":"$G252*Y252","v":0},null,null,{"$f":"$G252*AB252","v":0},null,10,{"$f":"$G252*AE252","v":0},null,null,{"$f":"$G252*AH252","v":0},null,null,{"$f":"$G252*AK252","v":0},null,5,{"$f":"$G252*AN252","v":0},null,10,{"$f":"$G252*AQ252","v":0},null,null,{"$f":"$G252*AT252","v":0},null,null,{"$f":"$G252*AW252","v":0},null,null,{"$f":"$G252*AZ252","v":0},null,10,{"$f":"$G252*BC252","v":0},null,null,{"$f":"$G252*BF252","v":0},null,null,{"$f":"$G252*BI252","v":0},null,null,{"$f":"$G252*BL252","v":0},null,2,{"$f":"$G252*BO252","v":0},null,5,{"$f":"$G252*BR252","v":0},null,null,{"$f":"$G252*BU252","v":0},null,null,{"$f":"$G252*BX252","v":0},null,null,{"$f":"$G252*CA252","v":0}]
["10.8.2",null,"B","serijski, 10A","serial, 10A","kom/pcs",{"$f":"CENA!G244","v":0},{"$f":"J253+M253+P253+S253+V253+Y253+AB253+AE253+AH253+AK253+AN253+AQ253+AT253+AW253+AZ253+BC253+BF253+BI253+BL253+BO253+BR253+BU253+BX253+CA253","v":36},{"$f":"G253*H253","v":0},5,{"$f":"$G253*J253","v":0},null,null,0,null,5,{"$f":"$G253*P253","v":0},null,1,0,null,5,{"$f":"$G253*V253","v":0},null,null,{"$f":"$G253*Y253","v":0},null,null,{"$f":"$G253*AB253","v":0},null,5,{"$f":"$G253*AE253","v":0},null,null,{"$f":"$G253*AH253","v":0},null,null,{"$f":"$G253*AK253","v":0},null,2,{"$f":"$G253*AN253","v":0},null,5,{"$f":"$G253*AQ253","v":0},null,null,{"$f":"$G253*AT253","v":0},null,null,{"$f":"$G253*AW253","v":0},null,null,{"$f":"$G253*AZ253","v":0},null,2,{"$f":"$G253*BC253","v":0},null,null,{"$f":"$G253*BF253","v":0},null,null,{"$f":"$G253*BI253","v":0},null,null,{"$f":"$G253*BL253","v":0},null,1,{"$f":"$G253*BO253","v":0},null,5,{"$f":"$G253*BR253","v":0},null,null,{"$f":"$G253*BU253","v":0},null,null,{"$f":"$G253*BX253","v":0},null,null,{"$f":"$G253*CA253","v":0}]
["10.8.3",null,"C","za zvono ","for bell","kom/pcs",{"$f":"CENA!G245","v":0},{"$f":"J254+M254+P254+S254+V254+Y254+AB254+AE254+AH254+AK254+AN254+AQ254+AT254+AW254+AZ254+BC254+BF254+BI254+BL254+BO254+BR254+BU254+BX254+CA254","v":9},{"$f":"G254*H254","v":0},1,{"$f":"$G254*J254","v":0},null,null,0,null,1,{"$f":"$G254*P254","v":0},null,null,0,null,1,{"$f":"$G254*V254","v":0},null,null,{"$f":"$G254*Y254","v":0},null,null,{"$f":"$G254*AB254","v":0},null,1,{"$f":"$G254*AE254","v":0},null,null,{"$f":"$G254*AH254","v":0},null,null,{"$f":"$G254*AK254","v":0},null,1,{"$f":"$G254*AN254","v":0},null,1,{"$f":"$G254*AQ254","v":0},null,null,{"$f":"$G254*AT254","v":0},null,null,{"$f":"$G254*AW254","v":0},null,null,{"$f":"$G254*AZ254","v":0},null,1,{"$f":"$G254*BC254","v":0},null,null,{"$f":"$G254*BF254","v":0},null,null,{"$f":"$G254*BI254","v":0},null,null,{"$f":"$G254*BL254","v":0},null,1,{"$f":"$G254*BO254","v":0},null,1,{"$f":"$G254*BR254","v":0},null,null,{"$f":"$G254*BU254","v":0},null,null,{"$f":"$G254*BX254","v":0},null,null,{"$f":"$G254*CA254","v":0}]
["10.8.4",null,"D","Instalacioni  prekidač \"KIP\" 16A","Installation switch \"KIP\" 16A","kom/pcs",{"$f":"CENA!G246","v":0},{"$f":"J255+M255+P255+S255+V255+Y255+AB255+AE255+AH255+AK255+AN255+AQ255+AT255+AW255+AZ255+BC255+BF255+BI255+BL255+BO255+BR255+BU255+BX255+CA255","v":9},{"$f":"G255*H255","v":0},1,{"$f":"$G255*J255","v":0},null,null,0,null,1,{"$f":"$G255*P255","v":0},null,null,0,null,1,{"$f":"$G255*V255","v":0},null,null,{"$f":"$G255*Y255","v":0},null,null,{"$f":"$G255*AB255","v":0},null,1,{"$f":"$G255*AE255","v":0},null,null,{"$f":"$G255*AH255","v":0},null,null,{"$f":"$G255*AK255","v":0},null,1,{"$f":"$G255*AN255","v":0},null,1,{"$f":"$G255*AQ255","v":0},null,null,{"$f":"$G255*AT255","v":0},null,null,{"$f":"$G255*AW255","v":0},null,null,{"$f":"$G255*AZ255","v":0},null,1,{"$f":"$G255*BC255","v":0},null,null,{"$f":"$G255*BF255","v":0},null,null,{"$f":"$G255*BI255","v":0},null,null,{"$f":"$G255*BL255","v":0},null,1,{"$f":"$G255*BO255","v":0},null,1,{"$f":"$G255*BR255","v":0},null,null,{"$f":"$G255*BU255","v":0},null,null,{"$f":"$G255*BX255","v":0},null,null,{"$f":"$G255*CA255","v":0}]
["10.9","E",9,"Indikator za kupatilo\n sa tri sklopke 16A i signalnim sijalicama","The indicator for the bathroom \nThree switches 16A and signal lights","kom/pcs",{"$f":"CENA!G247","v":0},{"$f":"J256+M256+P256+S256+V256+Y256+AB256+AE256+AH256+AK256+AN256+AQ256+AT256+AW256+AZ256+BC256+BF256+BI256+BL256+BO256+BR256+BU256+BX256+CA256","v":13},{"$f":"G256*H256","v":0},1,{"$f":"$G256*J256","v":0},null,null,0,null,1,{"$f":"$G256*P256","v":0},null,1,0,null,1,{"$f":"$G256*V256","v":0},null,1,{"$f":"$G256*Y256","v":0},null,null,{"$f":"$G256*AB256","v":0},null,1,{"$f":"$G256*AE256","v":0},null,null,{"$f":"$G256*AH256","v":0},null,null,{"$f":"$G256*AK256","v":0},null,1,{"$f":"$G256*AN256","v":0},null,1,{"$f":"$G256*AQ256","v":0},null,null,{"$f":"$G256*AT256","v":0},null,null,{"$f":"$G256*AW256","v":0},null,1,{"$f":"$G256*AZ256","v":0},null,1,{"$f":"$G256*BC256","v":0},null,null,{"$f":"$G256*BF256","v":0},null,1,{"$f":"$G256*BI256","v":0},null,null,{"$f":"$G256*BL256","v":0},null,1,{"$f":"$G256*BO256","v":0},null,1,{"$f":"$G256*BR256","v":0},null,null,{"$f":"$G256*BU256","v":0},null,null,{"$f":"$G256*BX256","v":0},null,null,{"$f":"$G256*CA256","v":0}]
[null,null,null,"Svetiljke","Lighting"]
["10.10","E",10,"Svetiljka za montažu na plafon  sa inkadescentnom sijalicom 60W, E-27, ","Luminaire to be mounted on the ceiling with a 60W incandescent bulb, E-27","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["10.10.1",null,"A"," IP 43 za sanitarni čvor","IP 43 for toilet",null,{"$f":"CENA!G250","v":0},{"$f":"J259+M259+P259+S259+V259+Y259+AB259+AE259+AH259+AK259+AN259+AQ259+AT259+AW259+AZ259+BC259+BF259+BI259+BL259+BO259+BR259+BU259+BX259+CA259","v":13},{"$f":"G259*H259","v":0},1,{"$f":"$G259*J259","v":0},null,null,{"$f":"$G259*M259","v":0},null,1,{"$f":"$G259*P259","v":0},null,1,0,null,1,{"$f":"$G259*V259","v":0},null,1,{"$f":"$G259*Y259","v":0},null,null,{"$f":"$G259*AB259","v":0},null,1,{"$f":"$G259*AE259","v":0},null,null,{"$f":"$G259*AH259","v":0},null,null,{"$f":"$G259*AK259","v":0},null,1,{"$f":"$G259*AN259","v":0},null,1,{"$f":"$G259*AQ259","v":0},null,null,{"$f":"$G259*AT259","v":0},null,null,{"$f":"$G259*AW259","v":0},null,1,{"$f":"$G259*AZ259","v":0},null,1,{"$f":"$G259*BC259","v":0},null,null,{"$f":"$G259*BF259","v":0},null,1,{"$f":"$G259*BI259","v":0},null,null,{"$f":"$G259*BL259","v":0},null,1,{"$f":"$G259*BO259","v":0},null,1,{"$f":"$G259*BR259","v":0},null,null,{"$f":"$G259*BU259","v":0},null,null,{"$f":"$G259*BX259","v":0},null,null,{"$f":"$G259*CA259","v":0}]
["10.10.2",null,"B","IP 20 za unutrašnje prostorije","IP 20 for indoor rooms",null,{"$f":"CENA!G251","v":0},{"$f":"J260+M260+P260+S260+V260+Y260+AB260+AE260+AH260+AK260+AN260+AQ260+AT260+AW260+AZ260+BC260+BF260+BI260+BL260+BO260+BR260+BU260+BX260+CA260","v":61},{"$f":"G260*H260","v":0},5,{"$f":"$G260*J260","v":0},null,null,0,null,5,{"$f":"$G260*P260","v":0},null,5,0,null,5,{"$f":"$G260*V260","v":0},null,5,{"$f":"$G260*Y260","v":0},null,null,{"$f":"$G260*AB260","v":0},null,5,{"$f":"$G260*AE260","v":0},null,null,{"$f":"$G260*AH260","v":0},null,null,{"$f":"$G260*AK260","v":0},null,5,{"$f":"$G260*AN260","v":0},null,5,{"$f":"$G260*AQ260","v":0},null,null,{"$f":"$G260*AT260","v":0},null,null,{"$f":"$G260*AW260","v":0},null,5,{"$f":"$G260*AZ260","v":0},null,5,{"$f":"$G260*BC260","v":0},null,null,{"$f":"$G260*BF260","v":0},null,5,{"$f":"$G260*BI260","v":0},null,null,{"$f":"$G260*BL260","v":0},null,5,{"$f":"$G260*BO260","v":0},null,1,{"$f":"$G260*BR260","v":0},null,null,{"$f":"$G260*BU260","v":0},null,null,{"$f":"$G260*BX260","v":0},null,null,{"$f":"$G260*CA260","v":0}]
[null,null,null,"Instalacija uzemljenja i gromobrana","Earthing and lightning protection"]
["10.11","E",11,"Pocinkovana traka","Galvanized strip",null,"/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["10.11.1",null,"A","FeZn 25x4mm","FeZn 25x4mm","m",{"$f":"CENA!G254","v":0},{"$f":"J263+M263+P263+S263+V263+Y263+AB263+AE263+AH263+AK263+AN263+AQ263+AT263+AW263+AZ263+BC263+BF263+BI263+BL263+BO263+BR263+BU263+BX263+CA263","v":0},{"$f":"G263*H263","v":0},null,{"$f":"$G263*J263","v":0},null,null,{"$f":"$G263*M263","v":0},null,null,{"$f":"$G263*P263","v":0},null,null,{"$f":"$G263*S263","v":0},null,null,{"$f":"$G263*V263","v":0},null,null,{"$f":"$G263*Y263","v":0},null,null,{"$f":"$G263*AB263","v":0},null,null,{"$f":"$G263*AE263","v":0},null,null,{"$f":"$G263*AH263","v":0},null,null,{"$f":"$G263*AK263","v":0},null,null,{"$f":"$G263*AN263","v":0},null,null,{"$f":"$G263*AQ263","v":0},null,null,{"$f":"$G263*AT263","v":0},null,null,{"$f":"$G263*AW263","v":0},null,null,{"$f":"$G263*AZ263","v":0},null,null,{"$f":"$G263*BC263","v":0},null,null,{"$f":"$G263*BF263","v":0},null,null,{"$f":"$G263*BI263","v":0},null,null,{"$f":"$G263*BL263","v":0},null,null,{"$f":"$G263*BO263","v":0},null,null,{"$f":"$G263*BR263","v":0},null,null,{"$f":"$G263*BU263","v":0},null,null,{"$f":"$G263*BX263","v":0},null,null,{"$f":"$G263*CA263","v":0}]
["10.11.2",null,"B","FeZn 20x3mm","FeZn 20x3mm","m",{"$f":"CENA!G255","v":0},{"$f":"J264+M264+P264+S264+V264+Y264+AB264+AE264+AH264+AK264+AN264+AQ264+AT264+AW264+AZ264+BC264+BF264+BI264+BL264+BO264+BR264+BU264+BX264+CA264","v":0},{"$f":"G264*H264","v":0},null,{"$f":"$G264*J264","v":0},null,null,0,null,null,{"$f":"$G264*P264","v":0},null,null,0,null,null,{"$f":"$G264*V264","v":0},null,null,{"$f":"$G264*Y264","v":0},null,null,{"$f":"$G264*AB264","v":0},null,null,{"$f":"$G264*AE264","v":0},null,null,{"$f":"$G264*AH264","v":0},null,null,{"$f":"$G264*AK264","v":0},null,null,{"$f":"$G264*AN264","v":0},null,null,{"$f":"$G264*AQ264","v":0},null,null,{"$f":"$G264*AT264","v":0},null,null,{"$f":"$G264*AW264","v":0},null,null,{"$f":"$G264*AZ264","v":0},null,null,{"$f":"$G264*BC264","v":0},null,null,{"$f":"$G264*BF264","v":0},null,null,{"$f":"$G264*BI264","v":0},null,null,{"$f":"$G264*BL264","v":0},null,null,{"$f":"$G264*BO264","v":0},null,null,{"$f":"$G264*BR264","v":0},null,null,{"$f":"$G264*BU264","v":0},null,null,{"$f":"$G264*BX264","v":0},null,null,{"$f":"$G264*CA264","v":0}]
["10.12","E",12,"SIP ormarić (PS49) sa sabirnicom za izjednačenje potencijala","SIP boxes (PS 49) with bonding","kom/pcs",{"$f":"CENA!G256","v":0},{"$f":"J265+M265+P265+S265+V265+Y265+AB265+AE265+AH265+AK265+AN265+AQ265+AT265+AW265+AZ265+BC265+BF265+BI265+BL265+BO265+BR265+BU265+BX265+CA265","v":0},{"$f":"G265*H265","v":0},null,{"$f":"$G265*J265","v":0},null,null,0,null,null,{"$f":"$G265*P265","v":0},null,null,0,null,null,{"$f":"$G265*V265","v":0},null,null,{"$f":"$G265*Y265","v":0},null,null,{"$f":"$G265*AB265","v":0},null,null,{"$f":"$G265*AE265","v":0},null,null,{"$f":"$G265*AH265","v":0},null,null,{"$f":"$G265*AK265","v":0},null,null,{"$f":"$G265*AN265","v":0},null,null,{"$f":"$G265*AQ265","v":0},null,null,{"$f":"$G265*AT265","v":0},null,null,{"$f":"$G265*AW265","v":0},null,null,{"$f":"$G265*AZ265","v":0},null,null,{"$f":"$G265*BC265","v":0},null,null,{"$f":"$G265*BF265","v":0},null,null,{"$f":"$G265*BI265","v":0},null,null,{"$f":"$G265*BL265","v":0},null,null,{"$f":"$G265*BO265","v":0},null,null,{"$f":"$G265*BR265","v":0},null,null,{"$f":"$G265*BU265","v":0},null,null,{"$f":"$G265*BX265","v":0},null,null,{"$f":"$G265*CA265","v":0}]
["10.13","E",13,"Provodnici za uzemljenje","Grounding conductors","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["10.13.1",null,"A","PP00-Y  1x16mm2","PP00-Y  1x16mm2","m",{"$f":"CENA!G258","v":0},{"$f":"J267+M267+P267+S267+V267+Y267+AB267+AE267+AH267+AK267+AN267+AQ267+AT267+AW267+AZ267+BC267+BF267+BI267+BL267+BO267+BR267+BU267+BX267+CA267","v":0},{"$f":"G267*H267","v":0},null,{"$f":"$G267*J267","v":0},null,null,{"$f":"$G267*M267","v":0},null,null,{"$f":"$G267*P267","v":0},null,null,{"$f":"$G267*S267","v":0},null,null,{"$f":"$G267*V267","v":0},null,null,{"$f":"$G267*Y267","v":0},null,null,{"$f":"$G267*AB267","v":0},null,null,{"$f":"$G267*AE267","v":0},null,null,{"$f":"$G267*AH267","v":0},null,null,{"$f":"$G267*AK267","v":0},null,null,{"$f":"$G267*AN267","v":0},null,null,{"$f":"$G267*AQ267","v":0},null,null,{"$f":"$G267*AT267","v":0},null,null,{"$f":"$G267*AW267","v":0},null,null,{"$f":"$G267*AZ267","v":0},null,null,{"$f":"$G267*BC267","v":0},null,null,{"$f":"$G267*BF267","v":0},null,null,{"$f":"$G267*BI267","v":0},null,null,{"$f":"$G267*BL267","v":0},null,null,{"$f":"$G267*BO267","v":0},null,null,{"$f":"$G267*BR267","v":0},null,null,{"$f":"$G267*BU267","v":0},null,null,{"$f":"$G267*BX267","v":0},null,null,{"$f":"$G267*CA267","v":0}]
["10.13.2",null,"B","P/F-Y      1x6mm2","P/F-Y      1x6mm2","m",{"$f":"CENA!G259","v":0},{"$f":"J268+M268+P268+S268+V268+Y268+AB268+AE268+AH268+AK268+AN268+AQ268+AT268+AW268+AZ268+BC268+BF268+BI268+BL268+BO268+BR268+BU268+BX268+CA268","v":0},{"$f":"G268*H268","v":0},null,{"$f":"$G268*J268","v":0},null,null,0,null,null,{"$f":"$G268*P268","v":0},null,null,0,null,null,{"$f":"$G268*V268","v":0},null,null,{"$f":"$G268*Y268","v":0},null,null,{"$f":"$G268*AB268","v":0},null,null,{"$f":"$G268*AE268","v":0},null,null,{"$f":"$G268*AH268","v":0},null,null,{"$f":"$G268*AK268","v":0},null,null,{"$f":"$G268*AN268","v":0},null,null,{"$f":"$G268*AQ268","v":0},null,null,{"$f":"$G268*AT268","v":0},null,null,{"$f":"$G268*AW268","v":0},null,null,{"$f":"$G268*AZ268","v":0},null,null,{"$f":"$G268*BC268","v":0},null,null,{"$f":"$G268*BF268","v":0},null,null,{"$f":"$G268*BI268","v":0},null,null,{"$f":"$G268*BL268","v":0},null,null,{"$f":"$G268*BO268","v":0},null,null,{"$f":"$G268*BR268","v":0},null,null,{"$f":"$G268*BU268","v":0},null,null,{"$f":"$G268*BX268","v":0},null,null,{"$f":"$G268*CA268","v":0}]
["10.13.3",null,"C","P/F-Y      1x4mm2","P/F-Y      1x4mm2","m",{"$f":"CENA!G260","v":0},{"$f":"J269+M269+P269+S269+V269+Y269+AB269+AE269+AH269+AK269+AN269+AQ269+AT269+AW269+AZ269+BC269+BF269+BI269+BL269+BO269+BR269+BU269+BX269+CA269","v":0},{"$f":"G269*H269","v":0},null,{"$f":"$G269*J269","v":0},null,null,0,null,null,{"$f":"$G269*P269","v":0},null,null,0,null,null,{"$f":"$G269*V269","v":0},null,null,{"$f":"$G269*Y269","v":0},null,null,{"$f":"$G269*AB269","v":0},null,null,{"$f":"$G269*AE269","v":0},null,null,{"$f":"$G269*AH269","v":0},null,null,{"$f":"$G269*AK269","v":0},null,null,{"$f":"$G269*AN269","v":0},null,null,{"$f":"$G269*AQ269","v":0},null,null,{"$f":"$G269*AT269","v":0},null,null,{"$f":"$G269*AW269","v":0},null,null,{"$f":"$G269*AZ269","v":0},null,null,{"$f":"$G269*BC269","v":0},null,null,{"$f":"$G269*BF269","v":0},null,null,{"$f":"$G269*BI269","v":0},null,null,{"$f":"$G269*BL269","v":0},null,null,{"$f":"$G269*BO269","v":0},null,null,{"$f":"$G269*BR269","v":0},null,null,{"$f":"$G269*BU269","v":0},null,null,{"$f":"$G269*BX269","v":0},null,null,{"$f":"$G269*CA269","v":0}]
[null,null,null,"Instalacija slabe struje","Installation of low voltage"]
["10.14","E",14,"Antenski koaksijalni kabl RG 6","Antenna Coaxial Cable RG 6","m",{"$f":"CENA!G262","v":0},{"$f":"J271+M271+P271+S271+V271+Y271+AB271+AE271+AH271+AK271+AN271+AQ271+AT271+AW271+AZ271+BC271+BF271+BI271+BL271+BO271+BR271+BU271+BX271+CA271","v":0},{"$f":"G271*H271","v":0},null,{"$f":"$G271*J271","v":0},null,null,{"$f":"$G271*M271","v":0},null,null,{"$f":"$G271*P271","v":0},null,null,{"$f":"$G271*S271","v":0},null,null,{"$f":"$G271*V271","v":0},null,null,{"$f":"$G271*Y271","v":0},null,null,{"$f":"$G271*AB271","v":0},null,null,{"$f":"$G271*AE271","v":0},null,null,{"$f":"$G271*AH271","v":0},null,null,{"$f":"$G271*AK271","v":0},null,null,{"$f":"$G271*AN271","v":0},null,null,{"$f":"$G271*AQ271","v":0},null,null,{"$f":"$G271*AT271","v":0},null,null,{"$f":"$G271*AW271","v":0},null,null,{"$f":"$G271*AZ271","v":0},null,null,{"$f":"$G271*BC271","v":0},null,null,{"$f":"$G271*BF271","v":0},null,null,{"$f":"$G271*BI271","v":0},null,null,{"$f":"$G271*BL271","v":0},null,null,{"$f":"$G271*BO271","v":0},null,null,{"$f":"$G271*BR271","v":0},null,null,{"$f":"$G271*BU271","v":0},null,null,{"$f":"$G271*BX271","v":0},null,null,{"$f":"$G271*CA271","v":0}]
["10.15","E",15,"Telefonski kabl sa bakarnim provodnicima \nIY(St)Y 2x2x0.8mm","Telephone cable with copper conductors \nIY (St) Y 2x2x0.8mm","m",{"$f":"CENA!G263","v":0},{"$f":"J272+M272+P272+S272+V272+Y272+AB272+AE272+AH272+AK272+AN272+AQ272+AT272+AW272+AZ272+BC272+BF272+BI272+BL272+BO272+BR272+BU272+BX272+CA272","v":0},{"$f":"G272*H272","v":0},null,{"$f":"$G272*J272","v":0},null,null,0,null,null,{"$f":"$G272*P272","v":0},null,null,0,null,null,{"$f":"$G272*V272","v":0},null,null,{"$f":"$G272*Y272","v":0},null,null,{"$f":"$G272*AB272","v":0},null,null,{"$f":"$G272*AE272","v":0},null,null,{"$f":"$G272*AH272","v":0},null,null,{"$f":"$G272*AK272","v":0},null,null,{"$f":"$G272*AN272","v":0},null,null,{"$f":"$G272*AQ272","v":0},null,null,{"$f":"$G272*AT272","v":0},null,null,{"$f":"$G272*AW272","v":0},null,null,{"$f":"$G272*AZ272","v":0},null,null,{"$f":"$G272*BC272","v":0},null,null,{"$f":"$G272*BF272","v":0},null,null,{"$f":"$G272*BI272","v":0},null,null,{"$f":"$G272*BL272","v":0},null,null,{"$f":"$G272*BO272","v":0},null,null,{"$f":"$G272*BR272","v":0},null,null,{"$f":"$G272*BU272","v":0},null,null,{"$f":"$G272*BX272","v":0},null,null,{"$f":"$G272*CA272","v":0}]
["10.16","E",16,"Priključnice","Connectors","/","/","/","/","/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/",null,"/","/"]
["10.16.1",null,"A","Telefonska - RJ11 za montažu u dozni fi 60mm","Phone - RJ11 for mounting in enclosure fi 60mm","m",{"$f":"CENA!G265","v":0},{"$f":"J274+M274+P274+S274+V274+Y274+AB274+AE274+AH274+AK274+AN274+AQ274+AT274+AW274+AZ274+BC274+BF274+BI274+BL274+BO274+BR274+BU274+BX274+CA274","v":0},{"$f":"G274*H274","v":0},null,{"$f":"$G274*J274","v":0},null,null,{"$f":"$G274*M274","v":0},null,null,{"$f":"$G274*P274","v":0},null,null,{"$f":"$G274*S274","v":0},null,null,{"$f":"$G274*V274","v":0},null,null,{"$f":"$G274*Y274","v":0},null,null,{"$f":"$G274*AB274","v":0},null,null,{"$f":"$G274*AE274","v":0},null,null,{"$f":"$G274*AH274","v":0},null,null,{"$f":"$G274*AK274","v":0},null,null,{"$f":"$G274*AN274","v":0},null,null,{"$f":"$G274*AQ274","v":0},null,null,{"$f":"$G274*AT274","v":0},null,null,{"$f":"$G274*AW274","v":0},null,null,{"$f":"$G274*AZ274","v":0},null,null,{"$f":"$G274*BC274","v":0},null,null,{"$f":"$G274*BF274","v":0},null,null,{"$f":"$G274*BI274","v":0},null,null,{"$f":"$G274*BL274","v":0},null,null,{"$f":"$G274*BO274","v":0},null,null,{"$f":"$G274*BR274","v":0},null,null,{"$f":"$G274*BU274","v":0},null,null,{"$f":"$G274*BX274","v":0},null,null,{"$f":"$G274*CA274","v":0}]
["10.16.2",null,"B","RTV priključnica za montažu u dozni fi 60mm","RTV connector for mounting in enclosure fi 60 mm","kom/pcs",{"$f":"CENA!G266","v":0},{"$f":"J275+M275+P275+S275+V275+Y275+AB275+AE275+AH275+AK275+AN275+AQ275+AT275+AW275+AZ275+BC275+BF275+BI275+BL275+BO275+BR275+BU275+BX275+CA275","v":0},{"$f":"G275*H275","v":0},null,{"$f":"$G275*J275","v":0},null,null,0,null,null,{"$f":"$G275*P275","v":0},null,null,0,null,null,{"$f":"$G275*V275","v":0},null,null,{"$f":"$G275*Y275","v":0},null,null,{"$f":"$G275*AB275","v":0},null,null,{"$f":"$G275*AE275","v":0},null,null,{"$f":"$G275*AH275","v":0},null,null,{"$f":"$G275*AK275","v":0},null,null,{"$f":"$G275*AN275","v":0},null,null,{"$f":"$G275*AQ275","v":0},null,null,{"$f":"$G275*AT275","v":0},null,null,{"$f":"$G275*AW275","v":0},null,null,{"$f":"$G275*AZ275","v":0},null,null,{"$f":"$G275*BC275","v":0},null,null,{"$f":"$G275*BF275","v":0},null,null,{"$f":"$G275*BI275","v":0},null,null,{"$f":"$G275*BL275","v":0},null,null,{"$f":"$G275*BO275","v":0},null,null,{"$f":"$G275*BR275","v":0},null,null,{"$f":"$G275*BU275","v":0},null,null,{"$f":"$G275*BX275","v":0},null,null,{"$f":"$G275*CA275","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"SUM(I14:I275)","v":0},null,{"$f":"SUM(K14:K275)","v":0},null,null,{"$f":"SUM(N14:N275)","v":0},null,null,{"$f":"SUM(Q14:Q275)","v":0},null,null,{"$f":"SUM(T14:T275)","v":0},null,null,{"$f":"SUM(W14:W275)","v":0},null,null,{"$f":"SUM(Z14:Z275)","v":0},null,null,{"$f":"SUM(AC14:AC275)","v":0},null,null,{"$f":"SUM(AF14:AF275)","v":0},null,null,{"$f":"SUM(AI14:AI275)","v":0},null,null,{"$f":"SUM(AL14:AL275)","v":0},null,null,{"$f":"SUM(AO14:AO275)","v":0},null,null,{"$f":"SUM(AR14:AR275)","v":0},null,null,{"$f":"SUM(AU14:AU275)","v":0},null,null,{"$f":"SUM(AX14:AX275)","v":0},null,null,{"$f":"SUM(BA14:BA275)","v":0},null,null,{"$f":"SUM(BD14:BD275)","v":0},null,null,{"$f":"SUM(BG14:BG275)","v":0},null,null,{"$f":"SUM(BJ14:BJ275)","v":0},null,null,{"$f":"SUM(BM14:BM275)","v":0},null,null,{"$f":"SUM(BP14:BP275)","v":0},null,null,{"$f":"SUM(BS14:BS275)","v":0},null,null,{"$f":"SUM(BV14:BV275)","v":0},null,null,{"$f":"SUM(BY14:BY275)","v":0},null,null,{"$f":"SUM(CB14:CB275)","v":0}]

{"sheet":"vendors list","index":3,"n_rows":266,"n_cols":9,"rows_kept":266,"cut":false,"hidden":false,"merged":[]}
[]
["KOD/\nCODE",null,null,"Opis građevinskog materijala ","Description of building materials","Jed.\nprod./\nUNIT","Proizvođač/ Manufacturer","Oznaka proizvoda/ Product label","Napomena/ Remark"]
[]
[1,"A",null,"OSNOVNI GRAĐEVINSKI MATERIJAL","BASIC BUILDING MATERIALS"]
["1.1","O",1,"Cement  za betone do MB 30","Cement for concrete up to 30 MB","kg"]
["1.2","O",2,"Hidratisani gašeni kreč pripremljen u prahu","Hydrated slaked lime powdered","kg"]
["1.3","O",3,"Rebrasto betonsko gvožđe (RA) ","Ribbed reinforcement steel","/",{"$f":"KORISNICI!G16","v":"/"},{"$f":"KORISNICI!H16","v":"/"},{"$f":"KORISNICI!I16","v":"/"}]
["1.3.1",null,"A","10 mm   - dužine 12m","10 mm   - length 12m ","kg"]
["1.3.2",null,"B","12 mm   - dužine 12m","12 mm   - length 12m","kg"]
["1.3.3",null,"C","14 mm   - dužine 12m","14 mm   - length 12m","kg"]
["1.3.4",null,"D","16 mm   - dužine 12m","16 mm   - length 12m","kg"]
["1.4","O",4,"Glatko betonsko gvožđe (GA) ","Glibly reinforcement steel","/",{"$f":"KORISNICI!G21","v":"/"},{"$f":"KORISNICI!H21","v":"/"},{"$f":"KORISNICI!I21","v":"/"}]
["1.4.1",null,"B","  8 mm   - dužine 12m","  8 mm   - length 12m","kg"]
["1.4.2",null,"C","10 mm  - dužine 12m","10 mm  - length 12m","kg"]
["1.5","O",5,"Armaturna betonska mreža \ndim. (dxš) 6000 x 2150 = 12,9 m2/kom","Reinforcement mesh\ndim. (lxw) 6000 x 2150 = 12,9 m2/pcs","/",{"$f":"KORISNICI!G24","v":"/"},{"$f":"KORISNICI!H24","v":"/"},{"$f":"KORISNICI!I24","v":"/"}]
["1.5.1",null,"A","Q84    /4x4/150x150/ ","Q84    /4x4/150x150/ ","kg"]
["1.5.2",null,"B","Q131  /5x5/150x150/ ","Q131  /5x5/150x150/ ","kg"]
["1.5.3",null,"C","Q188  /6x6/150x150/ ","Q188  /6x6/150x150/ ","kg"]
["1.5.4",null,"D","Q283  /6x6/100x100/","Q283  /6x6/100x100/","kg"]
["1.5.5",null,"E","Q335  /8x8/150x150/","Q335  /8x8/150x150/","kg"]
[]
[2,"Z",null,"MATERIJAL ZA ZIDANJE, MALTERISANJE, GLETOVANJE I FARBANJE","MASONRY, PLASTERING FAIRING AND PAINTING MATERIAL"]
["2.1","Z",1,"Giter blok (d/š/v) 250x190x190 mm","Gitter block (l/w/h) 250x190x190 mm","kom/pcs"]
["2.2","Z",2,"Giter polublok (12cm) (d/š/v) 250x120x190mm","Gitter half block (12cm) (l/w/h) 250x120x190mm","kom/pcs"]
["2.3","Z",3,"Opeka puna (d/š/v) 250x120x65 mm","Brick (full-without holes) (l/w/h) 250x120x65 mm","kom/pcs"]
["2.4","Z",4,"Blok od porobetona za pregradni zid\n(d/š/v) 625x200x200 mm","Aerated concrete block for partition wall\n(l/w/h) 625x200x200 mm","kom/pcs"]
["2.5","Z",5,"Fert nosači (gredice)\nDužina nosača je jednaka dužini binora = \nširina otvora između zidova + 30 cm.\nBroj gredica = dužina prostorije x 0,40","Fert beams\nBoom length is equal to the length of Binor =\nwidth of the openings between the walls + 30 cm.\nNumber of beams = length of room x 0.40","/",{"$f":"KORISNICI!G36","v":"/"},{"$f":"KORISNICI!H36","v":"/"},{"$f":"KORISNICI!I36","v":"/"}]
["2.5.1",null,"A","0,00-3,90 m ","0,00-3,90 m ","m1"]
["2.5.2",null,"B","3,91-4,50 m ","3,91-4,50 m ","m1"]
["2.5.3",null,"C","4,51-4,90 m ","4,51-4,90 m ","m1"]
["2.5.4",null,"D","4,91-5,30 m ","4,91-5,30 m ","m1"]
["2.5.5",null,"E","5,31-5,90 m ","5,31-5,90 m ","m1"]
["2.5.6",null,"F","5,91-6,30 m ","5,91-6,30 m ","m1"]
["2.6","Z",6,"Fert ispuna (d/š/v) 245x285/275x160 mm ","Fert fillings (l/w/h) 245x285/275x160 mm ","kom/pcs"]
["2.7","Z",7,"Malter za zidanje \nPripremljeno krečno - cementno vezivo","Mortar for masonry\nPrepared lime - cement binder","kg"]
["2.8","Z",8,"Malter za malterisanje \nPripremljeno krečno - cementno vezivo","Mortar for plastering\nPrepared lime - cement binder","kg"]
["2.9","Z",9,"Krečna glet masa\nBezcementna krečna masa za gletovanje","Lime smoothing mass\nNo cement lime compound for smoothing","kg"]
["2.10","Z",10,"Poludisperzivna boja \nPoludisperziona boja  razrediva vodom","Semi dispersion paint","kg"]
[]
["3","K",null,"MATERIJAL ZA KROVNU KONSTRUKCIJU, KROVNI POKRIVAČ, OSB I GIPS KARONSKE TABLE","ROOF CONSTRUCTION AND ROOFING MATERIAL, OSB AND PLASTERBOARD TABLE"]
["3.1","K",1,"Presovani glineni crep I klase\ndimenzija: 400-450x245-275 mm","Pressed clay tiles class 1\ndim: 400-450x245-275 mm","kom/pcs"]
["3.2","K",3,"Biber crep I klase dimenzija: 180x380 mm","Biber clay tiles class 1 dim: 180x380 mm","kom/pcs"]
["3.3","K",2,"Slemeni crep I klase (žljebnjak)","Ridge clay tiles class 1","kom/pcs"]
["3.4","K",4,"Paropropusna i vodonepropusna krovna  folija kontrola vodene pare iznad termoizolacije","Vapour permeable and waterproof roof sheeting control of water vapor above the insulation","m2"]
["3.5","K",5,"Staklena mineralna vuna \ntermoizolacija potkrovlja između rogova","Glass Mineral Wool \nloft insulation between the rafters","/",{"$f":"KORISNICI!G54","v":"/"},{"$f":"KORISNICI!H54","v":"/"},{"$f":"KORISNICI!I54","v":"/"}]
["3.5.1",null,"A","debljina d=10 cm  ","thickness d=10 cm  ","m2"]
["3.5.2",null,"B","debljina d=12 cm  ","thickness d=12 cm  ","m2"]
["3.5.3",null,"C","debljina d=14 cm  ","thickness d=14 cm  ","m2"]
["3.6","K",6,"Parna brana\nkontrola vodene pare ispod termoizolacije","Vapor barrier \ncontrol of water vapor below the insulation","m2"]
["3.7","K",7,"Čamova rezana građa različitog preseka\ndužine 400 cm","Fir lumber of different cross-section\nlength 400 cm","/",{"$f":"KORISNICI!G59","v":"/"},{"$f":"KORISNICI!H59","v":"/"},{"$f":"KORISNICI!I59","v":"/"}]
["3.7.1",null,"A","Rog/Venčanica/Raspinjača           10/12 cm","rafters / wall plate / ridge collar 10/12 cm","m3"]
["3.7.2",null,"B","Rog/Stub/Grebenjača/Slemenja.   12/14 cm","column / pile / hip rafter / ridge 12/14 cm","m3"]
["3.7.3",null,"C","Stub/Grebenjača                         14/14 cm","column / hip rafter 14/14 cm","m3"]
["3.7.4",null,"H","Tavanjače                                   18/26 cm","attic beams 18/26 cm","m3"]
["3.8","K",8,"Čamova rezana građa različitog preseka\ndužine 600 cm","Fir lumber of different cross-section\nlength 600 cm","/",{"$f":"KORISNICI!G64","v":"/"},{"$f":"KORISNICI!H64","v":"/"},{"$f":"KORISNICI!I64","v":"/"}]
["3.8.1",null,"A","Rog/Venčanica/Raspinjača          10/12 cm","rafters / wall plate / ridge collar 10/12 cm","m3"]
["3.8.2",null,"B","Rog/Stub/Grebenjača/Slemenja.   12/14 cm","column / pile / hip rafter / ridge 12/14 cm","m3"]
["3.8.3",null,"C","Stub/Grebenjača                         14/14 cm","column / hip rafter 14/14 cm","m3"]
["3.8.4",null,"D","Rožnjača                                    14/16 cm","Purlin 14/16 cm","m3"]
["3.8.5",null,"E","Kosnik/Pajanta                           10/10 cm","Strut 10/10 cm","m3"]
["3.8.6",null,"F","Klešta                                         6/12 cm","Collar tie 6/12 cm","m3"]
["3.8.7",null,"G","Krovna štafla                                5/8  cm","Roof battens 5/8  cm","m3"]
["3.8.8",null,"H","Tavanjače                                   18/26 cm","attic beams 18/26 cm","m3"]
["3.9","K",9,"Građevinska daska - fosna\n4,8/25/400 cm","Fir board\n4,8/25/400 cm","m3"]
["3.10","K",10,"Krovna daska od čamove rezane građe \n2,4-2,5/15 cm, isporučuje se dužine l=3,0 metra","Roof fir board\n2,4-2,5/15 cm, lenght l=3,0 m","m3"]
["3.11","K",11,"Krovna letva od čamove rezane građe \n 3 / 5 cm , isporučuje se dužine l=3,0 metra","Fir batten\n 3 / 5 cm , lenght l=3,0 m","m1"]
["3.12","K",12,"OSB3  vlagootporne konstruktivne ploče\nd=18 mm / dim. 2440 x 1220","OSB3  moisture resistant structural panels\nd=18 mm / dim. 2440 x 1220","kom/pcs"]
["3.13","K",13,"Standardne gips kartonske ploče - Tip A\ndimenzije: 1200-1250 x 2000 mm","Standard plasterboard table - Type A\ndim: 1200-1250 x 2000 mm","kom/pcs"]
["3.14","K",14,"Vlagootporne gips kartonske ploče - Tip H2\ndimenzije: 1200-1250 x 2000 mm","Moisture resistant Plasterboard - Type H2\ndim: 1200-1250 x 2000 mm","kom/pcs"]
["3.15","K",15,"Čelični pocinkovani i farbani olučni elementi prečnika: Ø 100 mm dužine 600 cm","Galvanized steel and painted gutter elements diameter: Ø 100 mm length 600 cm","/",{"$f":"KORISNICI!G79","v":"/"},{"$f":"KORISNICI!H79","v":"/"},{"$f":"KORISNICI!I79","v":"/"}]
["3.15.1",null,"A","Horizontalni polukružni","horizontal semicircular gutter","kom/pcs"]
["3.15.2",null,"B","Vertikalni kružni oluk","Vertical circular gutter","kom/pcs"]
[]
["4","P",null,"MATERIJAL ZA PODOVE, LAMINAT, PLOČICE I XPS","FLOORING, LAMINATE, TILES AND XPS"]
["4.1","P",1,"Unutrašnje podne keramičke pločice\nMin. dimenzije pločica: 200x300 mm","Floor tiles for inside\nMin. tile size: 200x300 mm","m2"]
["4.2","P",2,"Unutrašnje zidne keramičke pločice \nMin. dimenzije pločica: 200x300 mm","Wall tiles for inside\nMin. tile size: 200x300 mm","m2"]
["4.3","P",3,"Lepak za keramičke pločice\nFleksibilni, polimer-cementni lepak","Glue for ceramic tiles\nFlexible, polymer-cement glue","kg"]
["4.4","P",4,"Fleksibilna masa za fugovanje\nVodoodbojna fug masa na bazi cementa","Flexible mass for grouting\nWaterproof grout cement based","kg"]
["4.5","P",5,"Laminat - jakopresovani (HLP)\nsa klik sistemom, dezen: hrast natur (prirodni)","Laminate (HLP)\nwith click system, design: oak natural (natural)","m2"]
["4.6","P",6,"Lajsne za laminat od medijapana \nmaterijal: medijapan / MDF","Moldings for laminate MDF\nMaterial: MDF / MDF","m1"]
["4.7","P",7,"Podloga za laminat od polietilenske pene\nSunđerasta podloga za laminat","The base for laminate of polyethylene foam\nFoam base for laminate","m2"]
["4.8","P",8,"Cementni suvi estrih (cementna košuljica).\nPripremljeno cementno praškasto vezivo","Cement dry screed (cement screed)\nPrepared cement powder binder","kg"]
["4.9","P",9,"Građevinska PVC folija Za razdvajanje cementne košuljice od termo izolacije.","PVC foil for construction. To separate the cement screed of thermal insulation.","m2"]
["4.10","P",10,"Stirodur (XPS za izolaciju na podovima)\nploča od ekstrudirane polistirenske pene","Stirodur (XPS insulation for floors)\npanel of extruded polystyrene foam","/",{"$f":"KORISNICI!G93","v":"/"},{"$f":"KORISNICI!H93","v":"/"},{"$f":"KORISNICI!I93","v":"/"}]
["4.10.1",null,"A","debljine d=2 cm","d=2 cm","m2"]
["4.10.2",null,"B","debljine d=5 cm","d=5 cm","m2"]
[]
["5","F",null,"MATERIJAL ZA IZRADU FASADE","FACADE MATERIAL"]
["5.1","F",1,"EPS za termoizolaciju fasadnih zidova\nploča od ekspandiranog polistirena ","Thermal insulation for facade walls (EPS)\nplates made of expanded polystyrene","/",{"$f":"KORISNICI!G98","v":"/"},{"$f":"KORISNICI!H98","v":"/"},{"$f":"KORISNICI!I98","v":"/"}]
["5.1.1",null,"A","debljina d=8 cm","d=8 cm","m2"]
["5.1.2",null,"B","debljina d=10 cm","d=10 cm","m2"]
["5.1.3",null,"C","debljina d=12 cm","d=12 cm","m2"]
["5.1.4",null,"D","debljina d=14 cm","d=14 cm","m2"]
["5.2","F",2,"GrađevinskI lepak za EPS ploče \ncementni lepak namenjen za lepljenje ploča od ekspandiranog polistirena (EPS) i armiranje armaturne (rabic) mrežice ","Construction glue for EPS plates\ncement adhesive for gluing plates made of expanded polystyrene (EPS) and reinforcing wire (rabic) net","kg"]
["5.3","F",3,"Armaturna (rabic) staklena mrežica.\nVisokokvalitetna alkalno postojana staklena mrežica","Reinforcing (rabic) fiberglass mesh\nHigh quality alkali resistant fiberglass mesh","m2"]
["5.4","F",4,"Aktivni predpremaz pre nanošenja tankoslojnog fasadnog maltera.\npredpremaz za izjednačavanje upijanja - podloga","Active primer before applying the thin-layer plaster primer for the equalization of absorption surface","kg"]
["5.5","F",5,"Fasadni tankoslojni akrilni malter\nZavršni malter u pastoznom stanju, namenjen za zaštitu fasadnih zidnih površina","Facade thin-layer acrylic plaster\nFinishing plaster in paste-like state, intended for the protection of facade wall surfaces","/",{"$f":"KORISNICI!G106","v":"/"},{"$f":"KORISNICI!H106","v":"/"},{"$f":"KORISNICI!I106","v":"/"}]
["5.5.1",null,"A","boja približna RAL 1034 -kajsija ","color similar to RAL 1034-apricot","kg"]
["5.5.2",null,"B","boja približna RAL 6005 -pastelno zelena","color similar to RAL 6005 pastel-green","kg"]
["5.5.3",null,"C","boja približna RAL 5023 -pastelno plava","color similar to RAL 5023 pastel-blue","kg"]
["5.5.4",null,"D","boja približna RAL 3011 -pastelno crvena","color similar to RAL 3011 pastel-red","kg"]
["5.5.5",null,"E","boja približna RAL 8002 -braon","color similar to RAL 8002 brown","kg"]
[]
["6","H",null,"MATERIJAL ZA HIDRO IZOLACIJE","WATERPROOFING MATERIAL"]
["6.1","H",1,"Bitulit (prethodni premaz za hidroizolaciju)\nUpotrebljava se u isporučenom stanju (hladan  postupak ) bez zagrevanja","Bitulit (previous coating for waterproofing)\nIt is used as delivered (cold process) without heating","kg"]
["6.2","H",2,"Poliazbitol (hladni premaz za hidroizolaciju) Upotrebljava se u isporučenom stanju (hladan postupak) bez zagrevanja","POLYASBITOL (cold coating for waterproofing)\nIt is used as delivered (cold process) without heating","kg"]
["6.3","H",3,"Ter papir Bitumenska hidroizolaciona traka.","Ter paper Bituminous waterproofing tape.","m2"]
["6.4","H",4,"Kondor V-3 (hidroizolaciona traka)\nPlastomer-bitumenska traka, \nuložak stakleni voal, debljina:  ≥ 3 mm","Condor V-3 (waterproof tape)\nPlastomer-bituminous tape,\nglass mat, thickness: ≥ 3 mm","m2"]
[]
["7","S",null,"STOLARIJA","DOORS AND WINDOWS"]
["7.1","S",1,"Ulazna vrata od PVC-a (komplet pozicija). \nboja profila: bela RAL 9003\nbroj komora: ≥  5 komora\nširina x visina (zidarske mere)","Entrance door of PVC (set position)\nProfile color: white RAL 9003 \nNumber of chambers: ≥ 5 chambers \nwidth x height (masonry measures)","/",{"$f":"KORISNICI!G120","v":"/"},{"$f":"KORISNICI!H120","v":"/"},{"$f":"KORISNICI!I120","v":"/"}]
["7.1.1",null,"A","JK    90x210 cm - Leva       90 cm ","one wing  90x210 cm - Left      90 cm ","kom/pcs"]
["7.1.2",null,"B","JK    90x210 cm - Desna    90 cm","one wing  90x210 cm - Right    90 cm","kom/pcs"]
["7.1.3",null,"C","DK 120x210 cm - Leva       90+30 cm","two wings 120x210 cm - Left        90+30 cm","kom/pcs"]
["7.1.4",null,"D","DK 120x210 cm - Desna    90+30 cm","two wings 120x210 cm - Right    90+30 cm","kom/pcs"]
["7.2","S",2,"Prozori od PVC-a (komplet pozicija).\nVertikalno i horizontalno otvaranje, boja profila: bela RAL 9003, broj komora: ≥  5 komora\nširina x visina (zidarske mere)","Windows made of PVC (set position)\nVertical and horizontal opening, color profile: white RAL 9003, the number of chambers: ≥ 5 chambers \nwidth x height (masonry measures)","/",{"$f":"KORISNICI!G125","v":"/"},{"$f":"KORISNICI!H125","v":"/"},{"$f":"KORISNICI!I125","v":"/"}]
["7.2.1",null,"A","JK     60x60 cm ","one wing 60x60 cm ","kom/pcs"]
["7.2.2",null,"B","JK     80x80 cm","one wing 80x80 cm","kom/pcs"]
["7.2.3",null,"C","JK    80x120 cm    ","one wing 80x120 cm    ","kom/pcs"]
["7.2.4",null,"D","JK    80x140 cm    ","one wing 80x140 cm ","kom/pcs"]
["7.2.5",null,"E","JK  100x120 cm","one wing 100x120 cm","kom/pcs"]
["7.2.6",null,"F","JK  100x140 cm","one wing 100x140 cm","kom/pcs"]
["7.2.7",null,"G","DK  120x120 cm","two wings 120x120 cm","kom/pcs"]
["7.2.8",null,"H","DK  120x140 cm","two wings 120x140 cm","kom/pcs"]
["7.2.9",null,"I","DK  140x120 cm ","two wings 140x120 cm ","kom/pcs"]
["7.2.10",null,"J","DK  140x140 cm ","two wings 140x140 cm ","kom/pcs"]
["7.2.11",null,"K","DK  160x120 cm","two wings 160x120 cm","kom/pcs"]
["7.2.12",null,"L","DK  160x140 cm","two wings 160x140 cm","kom/pcs"]
["7.3","S",3,"Krovni prozor sa  aluminijumskom opšivkom od laminirane i impregnirane čamove građe","Roof window with aluminum flashings of laminated and impregnated fir timber","/",{"$f":"KORISNICI!G138","v":"/"},{"$f":"KORISNICI!H138","v":"/"},{"$f":"KORISNICI!I138","v":"/"}]
["7.3.1",null,"A","dimenzije 66 x 118   (širinaxvisina)","66 x 118 (width x height)","kom/pcs"]
["7.3.2",null,"B","dimenzije 78 x 98     (širinaxvisina)","78 x 98   (width x height)","kom/pcs"]
["7.3.3",null,"C","dimenzije 78 x 118   (širinaxvisina)","78 x 118 (width x height)","kom/pcs"]
["7.4","S",4,"Balkonska vrata od PVC-a (komplet pozicija). \nboja profila: bela RAL 9003\nbroj komora: ≥  5 komora\nširina x visina (zidarske mere)","Balcony doors from PVC (set position)\nProfile color: white RAL 9003 \nNumber of chambers: ≥ 5 chambers \nwidth x height (masonry measures)","/",{"$f":"KORISNICI!G142","v":"/"},{"$f":"KORISNICI!H142","v":"/"},{"$f":"KORISNICI!I142","v":"/"}]
["7.4.1",null,"A","JK     90x210 cm   - Leva","one wing  90x210 cm - Left     ","kom/pcs"]
["7.4.2",null,"B","JK     90x210 cm   - Desna ","one wing  90x210 cm - Right    ","kom/pcs"]
["7.4.3",null,"C","DK  140x210 cm","two wings 140x210 cm","kom/pcs"]
["7.5","S",5,"Unutrašnja vrata sa ispunom od kartonskog saća (komplet pozicija). \nširina x visina (spoljna mera futera)","Internal doors filled with cardboard honeycomb (set position)\nwidth x height (external measures footer)","/",{"$f":"KORISNICI!G146","v":"/"},{"$f":"KORISNICI!H146","v":"/"},{"$f":"KORISNICI!I146","v":"/"}]
["7.5.1",null,"A","70x205 cm - Leva  (dubina štoka 0-16 cm)","70x205 cm - Left     (depth door 0-16 cm)","kom/pcs"]
["7.5.2",null,"B","70x205 cm - Leva  (dubina štoka 16-30 cm)","70x205 cm - Left     (depth door 16-30 cm)","kom/pcs"]
["7.5.3",null,"C","70x205 cm - Desna (dubina štoka 0-16 cm)","70x205 cm - Right   (depth door  0-16 cm)","kom/pcs"]
["7.5.4",null,"D","70x205 cm - Desna (dubina štoka 16-30 cm)","70x205 cm - Right   (depth door  16-30 cm)","kom/pcs"]
["7.5.5",null,"E","80x205 cm - Leva  (dubina štoka 0-16 cm)","80x205 cm - Left     (depth door 0-16 cm)","kom/pcs"]
["7.5.6",null,"F","80x205 cm - Leva  (dubina štoka 16-30 cm)","80x205 cm - Left     (depth door 16-30 cm)","kom/pcs"]
["7.5.7",null,"G","80x205 cm - Desna (dubina štoka 0-16 cm)","80x205 cm - Right   (depth door  0-16 cm)","kom/pcs"]
["7.5.8",null,"H","80x205 cm - Desna (dubina štoka 16-30 cm)","80x205 cm - Right   (depth door  16-30 cm)","kom/pcs"]
["7.5.9",null,"I","90x205 cm - Leva  (dubina štoka 0-16 cm)","90x205 cm - Left     (depth door 0-16 cm)","kom/pcs"]
["7.5.10",null,"J","90x205 cm - Leva  (dubina štoka 16-30 cm)","90x205 cm - Left     (depth door 16-30 cm)","kom/pcs"]
["7.5.11",null,"K","90x205 cm - Desna (dubina štoka 0-16 cm)","90x205 cm - Right   (depth door  0-16 cm)","kom/pcs"]
["7.5.12",null,"L","90x205 cm - Desna (dubina štoka 16-30 cm)","90x205 cm - Right   (depth door  16-30 cm)","kom/pcs"]
[]
["8","D",null,"OSTALA OPREMA I MATERIJAL \n","OTHER EQUIPMENT AND SUPPLIES"]
["8.1","D",1,"Jednostruki dimnjak prečnika Ф 140 mm.\nTroslojni montažni dimnjački sistem namenjen za sva ložišta i sve vrste goriva, bez ventilacije.\nSastavljen je od: dimnjačke cevi od tehničke keramike, izolacije oko cevi dimnjaka od kamene vune minimalne specifične težine 80kg/m3, spoljneg dimnjačkog plašta od lakog betona, vatrostalnog lepka u kartušama, vatrootpornih i gasnonepropusnih atestiranih troslojnih vratanaca , kondenz posude, priključaka za reviziju i ložišta, krovne ploče od staklo betona, nosača tervola i tvrdih tervol ploča za priključke, ventilacione rešetke, dilatacione rozete od nerđajućeg čelika. \nSpoljna dimenzija dimnjačkog plašta za fi14cm=32x32cm.","A single chimney diameter 140 mm.\nThree-layer prefabricated chimney system designed for all furnaces and all types of fuel, with no ventilation. It is composed of: chimney pipe of technical ceramics, pipe insulation around the chimney of stone wool minimum specific weight of 80kg/m3, external chimney mantle of lightweight concrete, refractory adhesive in cartouches, fireproof and gas impermeable certified three-layer side door, condensate pots, connectors for the audit and furnaces, roof tiles of glass concrete girders Tervola and hard tervol plate connections, ventilation grilles, rosettes expansion of stainless steel. The external dimensions of the chimney sleeve fi14cm = 32x32cm.","m1"]
[]
["9","V",null,"Vodovod Kanalizacija Oprema","WATER SUPPLY AND SEWAGE"]
[null,null,null,"Vodovod","WATER SUPPLY"]
["9.1","V",1,"Vodovodne polietilenske cevi  PE 100 PN16\nza radni pritisak 16 bara (SDR 11)","Water supply polyethylene pipe PE 100 PN16\nthe working pressure of 16 bar (SDR 11)","/",{"$f":"KORISNICI!G165","v":"/"},{"$f":"KORISNICI!H165","v":"/"},{"$f":"KORISNICI!I165","v":"/"}]
["9.1.1",null,"A","d25  (s min. 2,3)    - 3/4\"","d25  (s min. 2,3)    - 3/4\"","m1"]
["9.1.2",null,"B","d32  (s min. 3,0)   -       1\"","d32  (s min. 3,0)   -       1\"","m1"]
["9.1.3",null,"C","d40  (s min. 3,7)   -  5/4\"","d40  (s min. 3,7)   -  5/4\"","m1"]
["9.2","V",2,"Vodovodne cevi  PP-R 80 PN20 \nza radni pritisak 20 bara, bele ili zelene boje\n(materijal: polipropilen-random kapolimer)","Water pipe PP-R 80 PN20 \nthe working pressure of 20 bar, white or green \n(material: polypropylene random kapolimer)","/",{"$f":"KORISNICI!G169","v":"/"},{"$f":"KORISNICI!H169","v":"/"},{"$f":"KORISNICI!I169","v":"/"}]
["9.2.1",null,"B","d20  (s min.   3,4)    - 1/2\"","d20  (s min.   3,4)    - 1/2\"","m1"]
["9.2.2",null,"C","d25  (s min.   4,2)    - 3/4\"","d25  (s min.   4,2)    - 3/4\"","m1"]
["9.2.3",null,"D","d32  (s min.   5,4)    -     1\"","d32  (s min.   5,4)    -     1\"","m1"]
["9.3","V",3,"Vodomer \nsa prirubnicama, holenderima i pripadajućom opremom za montažu, za pritisak do 16 bara","water gauge\nflanges, unions and associated equipment for assembly, for pressure up to 16 bar","/",{"$f":"KORISNICI!G173","v":"/"},{"$f":"KORISNICI!H173","v":"/"},{"$f":"KORISNICI!I173","v":"/"}]
["9.3.1",null,"A","horizontalni 3/4\"    ","Horizontal 3/4\"    ","kom/pcs"]
["9.3.2",null,"B","horizontalni     1\"    ","Horizontal     1\"    ","kom/pcs"]
["9.3.3",null,"C","horizontalni 5/4\"","Horizontal 5/4\"","kom/pcs"]
["9.4","V",4,"Ravni propusni ventil sa ogrankom za pražnjenje","Skip straight valve with a branch drain","/",{"$f":"KORISNICI!G177","v":"/"},{"$f":"KORISNICI!H177","v":"/"},{"$f":"KORISNICI!I177","v":"/"}]
["9.4.1",null,"A","d25  (s min. 2,3)    - 3/4\"","d25  (s min. 2,3)    - 3/4\"","kom/pcs"]
["9.4.2",null,"B","d32  (s min. 3,0)   -       1\"","d32  (s min. 3,0)   -       1\"","kom/pcs"]
["9.5","V",5,"Propusni ventil za uzidanje sa kapom ","Gate valve for the wall with cap","/",{"$f":"KORISNICI!G180","v":"/"},{"$f":"KORISNICI!H180","v":"/"},{"$f":"KORISNICI!I180","v":"/"}]
["9.5.1",null,"A","d20  (s min.   3,4)    - 1/2\"","d20  (s min.   3,4)    - 1/2\"","kom/pcs"]
["9.5.2",null,"B","d25  (s min.   4,2)    - 3/4\"","d25  (s min.   4,2)    - 3/4\"","kom/pcs"]
["9.5.3",null,"C","d32  (s min. 3,0)   -       1\"","d32  (s min. 3,0)   -       1\"","kom/pcs"]
["9.6","V",6,"Ugaoni \"EK\" sa kapom","Angle valve \"EK\" with cap","/",{"$f":"KORISNICI!G184","v":"/"},{"$f":"KORISNICI!H184","v":"/"},{"$f":"KORISNICI!I184","v":"/"}]
["9.6.1",null,"A","d20  (s min.   3,4)    - 1/2\"","d20  (s min.   3,4)    - 1/2\"","kom/pcs"]
["9.7","V",7,"Termička izolacija vodovodnih cevi  -tipa plamaflex ISO ili sl.","Thermal insulation of water pipes-type PLAMAFLEX ISO etc..","/",{"$f":"KORISNICI!G186","v":"/"},{"$f":"KORISNICI!H186","v":"/"},{"$f":"KORISNICI!I186","v":"/"}]
["9.7.1",null,"B","d20   (22/9)   - 1/2\"","d20   (22/9)   - 1/2\"","m1"]
["9.7.2",null,"C","d25   (25/9) - 3/4\"","d25   (25/9) - 3/4\"","m1"]
["9.7.3",null,"D","d32   (35/9)-     1\"","d32   (35/9)-     1\"","m1"]
[null,null,null,"Kanalizacija","SEWAGE"]
["9.8","V",8,"PVC kanalizacione cevi SDR 41 / SN4 / PN5\nza spoljni razvod, kućna i ulična kanalizacija","PVC sewer pipe SDR 41 / CH4 / PN5\nfor external distribution, household and street sewage","/",{"$f":"KORISNICI!G191","v":"/"},{"$f":"KORISNICI!H191","v":"/"},{"$f":"KORISNICI!I191","v":"/"}]
["9.8.1",null,"A","d110 (s min.   3,2)    dužina 6,0m","d110 (s min.   3,2)    length 6,0m","kom/pcs"]
["9.8.2",null,"B","d160 (s min.   4,0)    dužina 6,0m","d160 (s min.   4,0)    length 6,0m","kom/pcs"]
["9.9","V",9,"Plastične PP cevi SDR 51 / SN2 / PN4\nza unutrašnji (kućni) razvod, kućna kanalizacija","Plastic PP pipes SDR 51 / SN2 / PN4\nfor internal (home) distribution, household sewage","/",{"$f":"KORISNICI!G194","v":"/"},{"$f":"KORISNICI!H194","v":"/"},{"$f":"KORISNICI!I194","v":"/"}]
["9.9.1",null,"A","d50     (s min.   1,8)    dužina 3,0m","d50     (s min.   1,8)    length 3,0m","kom/pcs"]
["9.9.2",null,"B","d75     (s min.   1,9)    dužina 3,0m","d75     (s min.   1,9)    length 3,0m","kom/pcs"]
["9.9.3",null,"C","d110  (s min.   2,7)    dužina 3,0m","d110  (s min.   2,7)    length 3,0m","kom/pcs"]
["9.10","V",10,"Plitki PE podni slivnik d50 sa horizontalnim odvodom dimenzija 150x150mm","Shallow PE floor drain with horizontal outlet d50 size 150x150mm","kom/pcs"]
["9.11","V",11,"Zidni sifoni sa odvodnom mesinganom cevi d32 (mašina za pranje veša i sudova)","Wall siphon with drainage brass tubes d32 (washing machines, dishwashers)","kom/pcs"]
[null,null,null,"Oprema u kupatilu","BATHROOM EQUPIMENT"]
["9.12","V",12,"WC šolja od keramike  I klase","Ceramic toilet bowl class 1","kom/pcs"]
["9.13","V",13,"Niskomontažni plastični predzidni vodokotlić \nza nisku montažu iznad wc šolje sa plovkom i svim potrebnim delovima za funkcionisanje vodokotlića","Low mounting plastic-wall toilet tank\nfor low installation above the toilet bowl float and all the parts required for the operation of flushing","kom/pcs"]
["9.14","V",14,"Umivaonikom sa stubom od keramike  I klase","Washbasin with ceramic pillar class 1","kom/pcs"]
["9.15","V",15,"Pravougaona akrilna tuš kada\ndimenzija 90x90cm sa odlivnim ventilom","Rectangular acrylic shower \nsize 90x90cm with discharge valve","kom/pcs"]
["9.16","V",16,"Električni akumulacioni bojler 50l vertikalni \ngrejač 2 kW, napon 230V, kazan izrađen od emajliranog lima, sa  pratećim materijalom za ugradnju","Electric storage water heater 50l vertical \nheater 2 kW, 230V, caldron made ​​of enameled steel, with supporting material for installation","kom/pcs"]
["9.17","V",17,"Ogledalo sa etažerom (iznad umivaonika)\nčetvrtasto, min. dimenzija 80x60cm","Mirror with shelf above wash basin \nsquare, min. 80x60cm","kom/pcs"]
["9.18","V",18,"Baterije (slavine) \nhromirane baterije za hladnu i toplu vodu","Lever\nchrome lever for cold and hot water","/",{"$f":"KORISNICI!G207","v":"/"},{"$f":"KORISNICI!H207","v":"/"},{"$f":"KORISNICI!I207","v":"/"}]
["9.18.1",null,"A","za umivaonik jednoručna stojeća ","For washbasin single lever basin standing","kom/pcs"]
["9.18.2",null,"B","za tuš kadu (sa tuš ručicom i tuš crevom)\njednoručna sa poniklovanim savitljivim crevom","For shower bath (with shower head and shower hose) Single lever with nickel hoses","kom/pcs"]
["9.18.3",null,"C","za mašinu za veš i sudove, holender slavina DN20/15, s pripadajućom opremom za ugradnju ","for washing machine and dishwasher, union DN20/15 taps, and all the equipment for installation","kom/pcs"]
[null,null,null,"Oprema u kuhinji","KITCHEN EQUIPMENT"]
["9.19","V",19,"Korito sudopere od \"Inox \"-a (dvodelno)\n(izrađeno od plemenitog nerđajućeg čelika)\norjenacione dimenzije:  780 x 435 x 150 mm","kitchen sink \"Inox\" two-part\n(made of stainless steel)\napprox. dim:  780 x 435 x 150 mm","kom/pcs"]
["9.20","V",20,"Električni akumulacioni bojler 5l\nza ugradnju iznad sudopere, vertikalni grejač 2 kW, napon 230V, kazan izrađen od plastike\nsa  pratećim materijalom za ugradnju","Electric storage water heater 5l\nFitting over the sink, vertical heater 2 kW, 230V, caldron made ​​of plastic with the materials for installation","kom/pcs"]
["9.21","V",21,"Baterija za sudoperu jednoručna stojeća hromirana baterija za hladnu i toplu vodu ","Sink-standing single lever chrome mixer for hot and cold water","kom/pcs"]
[]
["10","E",null,"ELEKTRO MATERIJAL I OPREMA\n","Electrical materials and equipment"]
[null,null,null,"Kablovi i kablovski pribor","Electrical cables and cable accessories"]
["10.1","E",1,"Napojni kablovi","Power cables","/",{"$f":"KORISNICI!G218","v":"/"},{"$f":"KORISNICI!H218","v":"/"},{"$f":"KORISNICI!I218","v":"/"}]
["10.1.1",null,"A","X00-A      4x16 mm2","X00-A      4x16 mm2","m"]
["10.1.2",null,"B","PP00-Y   5x6    mm2","PP00-Y   5x6    mm2","m"]
["10.1.3",null,"C","PP00-Y   5x10  mm2","PP00-Y   5x10  mm2","m"]
["10.2","E",2,"Instalacioni kablovi","Installation cables","/",{"$f":"KORISNICI!G222","v":"/"},{"$f":"KORISNICI!H222","v":"/"},{"$f":"KORISNICI!I222","v":"/"}]
["10.2.1",null,"A","PP-Y       3x1,5  mm2","PP-Y       3x1,5  mm2","m"]
["10.2.2",null,"B","PP-Y       4x1,5  mm2","PP-Y       4x1,5  mm2","m"]
["10.2.3",null,"C","PP-Y       3x2,5  mm2","PP-Y       3x2,5  mm2","m"]
["10.2.4",null,"D","PP-Y       5x2,5  mm2","PP-Y       5x2,5  mm2","m"]
["10.3","E",3,"Instalacione PVC cevi","PVC pipe for installations of cables","/",{"$f":"KORISNICI!G227","v":"/"},{"$f":"KORISNICI!H227","v":"/"},{"$f":"KORISNICI!I227","v":"/"}]
["10.3.1",null,"A","fi 16mm2","fi 16mm2","m"]
["10.3.2",null,"B","fi 50mm2","fi 50mm2","m"]
[null,null,null,"Razvodne table i oprema","The junction boards and equipment"]
["10.4","E",4,"Razvodna tabla Stanska, za ugradnju na zid sa transparentim vratima, sa mestom za 18 modula, DIN šinom, IP40\nRazvodna tabla sadrži :","Junction board (for flat) for wall mounting with transparent door, with space for 18 modules, DIN rail, IP40\nJunction board contains:","kom/pcs"]
[null,null,null,"Jednopolni instalacioni prekidač\n(automatski osigurač) za montažu na DIN šinu nom. napona 230V/400V, 50Hz; karakteristike B; prekidne moći 6kA:","Single-pole fuse\n(Automatic fuse) for mounting on DIN rail nom. voltage 230V/400V, 50Hz, features B; breaking capacity 6kA:","/",{"$f":"KORISNICI!G232","v":"/"},{"$f":"KORISNICI!H232","v":"/"},{"$f":"KORISNICI!I232","v":"/"}]
[null,null,null,"nazivne struje 6A, komada 1","rated current of 6A","kom/pcs"]
[null,null,null,"nazivne struje 10A, komada 2","rated current of 10A","kom/pcs"]
[null,null,null,"nazivne struje 16A, komada 9","rated current of 16A","kom/pcs"]
[null,null,null,"Signalna sijalica\nza signalizaciju tarife 230V za ugradnju u stansku razvodnu tablu, montažu na DIN šinu, komada 1","The indicator lamp\nfor signaling rates 230V for use in flat junction board, mounting on DIN rail","kom/pcs"]
[null,null,null,"FID sklopka za ugradnju u stansku razvodnu tablu, montažu na DIN šinu, ","FID switch for installation in junction board, mounting on DIN rail","/",{"$f":"KORISNICI!G237","v":"/"},{"$f":"KORISNICI!H237","v":"/"},{"$f":"KORISNICI!I237","v":"/"}]
[null,null,null,"16A/30mA,  2-polna,   230V, 50Hz; komada 2","16A/30mA, 2-pole, 230V, 50Hz;","kom/pcs"]
[null,null,null,"25A/0,5A,    4-polna,    230V/400V, 50Hz; komada 1","25A / 0,5 A, 4-pole, 230V/400V, 50Hz;","kom/pcs"]
[null,null,null,"Instalaciono zvono 230V, 50Hz; za ugradnju u stansku razvodnu tablu, montažu na DIN šinu, komada 1","Bell 230V, 50Hz, for use in junction board, mounting on DIN rail","kom/pcs"]
[null,null,null,"Instalacioni materijal","Installation material"]
["10.5","E",5,"Instalaciona kutija\nza ugradnju u završnu obradu zida","Installation box\nfor installation in the wall","/",{"$f":"KORISNICI!G242","v":"/"},{"$f":"KORISNICI!H242","v":"/"},{"$f":"KORISNICI!I242","v":"/"}]
["10.5.1",null,"A","fi 60 mm","fi 60 mm","kom/pcs"]
["10.5.2",null,"B","fi 78 mm","fi 78 mm","kom/pcs"]
["10.5.3",null,"C","100x100mm","100x100mm","kom/pcs"]
["10.6","E",6,"Instalaciona priključnica IP20 za ugradnju u završnu obradu zida sa zaštitnim kontaktom","Installation socket IP20 for installation in the wall with a protection contact","/",{"$f":"KORISNICI!G246","v":"/"},{"$f":"KORISNICI!H246","v":"/"},{"$f":"KORISNICI!I246","v":"/"}]
["10.6.1",null,"A","16A, monofazna, 250 V","16A, single-phase, 250 V","kom/pcs"]
["10.6.2",null,"B","16A, monofazna, dupla, 250 V","16A, single-phase, double, 250 V","kom/pcs"]
["10.6.3",null,"C","16A, trofazna, 400V","16A, three-phase, 400V","kom/pcs"]
["10.7","E",7,"Instalaciona priključnica IP43 sa poklopcem za ugradnju u završnu obradu zida, sa zaštit. kontaktom, 16A, monofazna, 250 V","Installation socket IP43 with cover for use in wall with protection. contact, 16A, single-phase, 250 V","kom/pcs"]
["10.8","E",8,"Prekidači\n IP20 za ugradnju u završnu obradu zida","Switches \n IP20 for installation in wall","/",{"$f":"KORISNICI!G251","v":"/"},{"$f":"KORISNICI!H251","v":"/"},{"$f":"KORISNICI!I251","v":"/"}]
["10.8.1",null,"A","običan, 10A","regular, 10A","kom/pcs"]
["10.8.2",null,"B","serijski, 10A","serial, 10A","kom/pcs"]
["10.8.3",null,"C","za zvono ","for bell","kom/pcs"]
["10.8.4",null,"D","Instalacioni  prekidač \"KIP\" 16A","Installation switch \"KIP\" 16A","kom/pcs"]
["10.9","E",9,"Indikator za kupatilo\n sa tri sklopke 16A i signalnim sijalicama","The indicator for the bathroom \nThree switches 16A and signal lights","kom/pcs"]
[null,null,null,"Svetiljke","Lighting"]
["10.10","E",10,"Svetiljka za montažu na plafon  sa inkadescentnom sijalicom 60W, E-27, ","Luminaire to be mounted on the ceiling with a 60W incandescent bulb, E-27","/",{"$f":"KORISNICI!G258","v":"/"},{"$f":"KORISNICI!H258","v":"/"},{"$f":"KORISNICI!I258","v":"/"}]
["10.10.1",null,"A"," IP 43 za sanitarni čvor","IP 43 for toilet"]
["10.10.2",null,"B","IP 20 za unutrašnje prostorije","IP 20 for indoor rooms"]
[null,null,null,"Instalacija uzemljenja i gromobrana","Earthing and lightning protection"]
["10.11","E",11,"Pocinkovana traka","Galvanized strip",null,{"$f":"KORISNICI!G262","v":"/"},{"$f":"KORISNICI!H262","v":"/"},{"$f":"KORISNICI!I262","v":"/"}]
["10.11.1",null,"A","FeZn 25x4mm","FeZn 25x4mm","m"]
["10.11.2",null,"B","FeZn 20x3mm","FeZn 20x3mm","m"]
["10.12","E",12,"SIP ormarić (PS49) sa sabirnicom za izjednačenje potencijala","SIP boxes (PS 49) with bonding","kom/pcs"]
["10.13","E",13,"Provodnici za uzemljenje","Grounding conductors","/",{"$f":"KORISNICI!G266","v":"/"},{"$f":"KORISNICI!H266","v":"/"},{"$f":"KORISNICI!I266","v":"/"}]
["10.13.1",null,"A","PP00-Y  1x16mm2","PP00-Y  1x16mm2","m"]
["10.13.2",null,"B","P/F-Y      1x6mm2","P/F-Y      1x6mm2","m"]
["10.13.3",null,"C","P/F-Y      1x4mm2","P/F-Y      1x4mm2","m"]
[null,null,null,"Instalacija slabe struje","Installation of low voltage"]
["10.14","E",14,"Antenski koaksijalni kabl RG 6","Antenna Coaxial Cable RG 6","m"]
["10.15","E",15,"Telefonski kabl sa bakarnim provodnicima \nIY(St)Y 2x2x0.8mm","Telephone cable with copper conductors \nIY (St) Y 2x2x0.8mm","m"]
["10.16","E",16,"Priključnice","Connectors","/",{"$f":"KORISNICI!G273","v":"/"},{"$f":"KORISNICI!H273","v":"/"},{"$f":"KORISNICI!I273","v":"/"}]
["10.16.1",null,"A","Telefonska - RJ11 za montažu u dozni fi 60mm","Phone - RJ11 for mounting in enclosure fi 60mm","m"]
["10.16.2",null,"B","RTV priključnica za montažu u dozni fi 60mm","RTV connector for mounting in enclosure fi 60 mm","kom/pcs"]